IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView]"
File name: "2006117"
Time stamp: "2014-12-11T14:42:20"
Preprocessor: "Autodesk Revit Architecture 2012 - 1.0"
Originating system: "20110916_2132(x64)"
Application: "Autodesk Revit Architecture 2012" version "2012" identifier "Revit" by Organization "Autodesk Revit Architecture 2012"

People and organizations
  Person "Rune" of Organization (no name given)
  Owner history of Person "Rune" of Organization (no name given) | application "Autodesk Revit Architecture 2012" version "2012" identifier "Revit" by Organization "Autodesk Revit Architecture 2012" | change NOCHANGE | created 0 (1970-01-01T00:00:00Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: MILLI SQUARE_METRE
  VOLUMEUNIT: MILLI CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  TIMEUNIT: SECOND

Spatial structure
IFCPROJECT "2006117" | long name "SIRISKJÆR" | phase "Detailprojekt"
  IFCSITE "Default" | latitude 58° 58′ 9.491271″ | longitude 5° 45′ 41.603851″ | elevation above sea level 6240.
    IFCBUILDING | postal address: "58.9693031311035", "5.76155662536621"
      IFCBUILDINGSTOREY "00U" | elevation -3740.000000000639
        contains 126 elements
          2 x IFCWALL | object type "Basic Wall:241.2_Lejlighedsskel_betonvæg_220mm:7107552" | names: "Basic Wall:241.2_Lejlighedsskel_betonvæg_220mm:1251120", "Basic Wall:241.2_Lejlighedsskel_betonvæg_220mm:2992060" | material: layers "Basic Wall:241.2_Lejlighedsskel_betonvæg_220mm" ("Aart_beton" 220.) | property sets: PSet_Revit_Structural, PSet_Revit_Constraints, PSet_Revit_Identity Data, PSet_Revit_Phasing, PSet_Revit_Dimensions, Pset_WallCommon
          1 x IFCSTAIR | object type "Stair:Trappeopgang niv_0" | names: "Stair:Trappeopgang niv_0:1593417" | parts: 3 IFCRAILING, 1 IFCSTAIR | property sets: Pset_StairCommon, PSet_Revit_Dimensions, PSet_Revit_Constraints, PSet_Revit_Graphics, PSet_Revit_Identity Data, PSet_Revit_Phasing
          2 x IFCWALL | object type "Basic Wall:Aart_Yttervegg_401mm_type_2_NY:5340176" | names: "Basic Wall:Aart_Yttervegg_401mm_type_2_NY:1654698", "Basic Wall:Aart_Yttervegg_401mm_type_2_NY:1654716" | material: layers "Basic Wall:Aart_Yttervegg_401mm_type_2_NY" ("Kledningstype 2" 33., "Wood" 48., "Wood" 48., "Aart_Gips" 13., "Aart_isolering" 198., "Aart_isolering" 48., "Generic" 13.) | property sets: PSet_Revit_Structural, PSet_Revit_Constraints, PSet_Revit_Identity Data, PSet_Revit_Phasing, PSet_Revit_Dimensions, Pset_WallCommon
          1 x IFCWALL | object type "Basic Wall:Aart_Yttervegg_588mm_type_2_1:7162618" | names: "Basic Wall:Aart_Yttervegg_588mm_type_2_1:1654731" | material: layers "Basic Wall:Aart_Yttervegg_588mm_type_2_1" ("Kledningstype 2" 33., "Wood" 48., "Wood" 48., "Aart_Gips" 13., "Aart_isolering" 246., "Aart_beton" 200.) | property sets: PSet_Revit_Structural, PSet_Revit_Constraints, PSet_Revit_Identity Data, PSet_Revit_Phasing, PSet_Revit_Dimensions, Pset_WallCommon
          2 x IFCWALL | object type "Basic Wall:241.3_Betonvæg_250mm:373623" | names: "Basic Wall:241.3_Betonvæg_250mm:1741886", "Basic Wall:241.3_Betonvæg_250mm:1742025" | material: layers "Basic Wall:241.3_Betonvæg_250mm" ("Aart_beton" 250.) | property sets: PSet_Revit_Structural, PSet_Revit_Constraints, PSet_Revit_Identity Data, PSet_Revit_Phasing, PSet_Revit_Dimensions, Pset_WallCommon
          3 x IFCWALLSTANDARDCASE | object type "Basic Wall:241.2_Lejlighedsskel_betonvæg_220mm:7107552" | names: "Basic Wall:241.2_Lejlighedsskel_betonvæg_220mm:2992803", "Basic Wall:241.2_Lejlighedsskel_betonvæg_220mm:3448209", "Basic Wall:241.2_Lejlighedsskel_betonvæg_220mm:3448255" | material: layers "Basic Wall:241.2_Lejlighedsskel_betonvæg_220mm" ("Aart_beton" 220.) | property sets: PSet_Revit_Structural, PSet_Revit_Constraints, PSet_Revit_Identity Data, PSet_Revit_Phasing, PSet_Revit_Dimensions, Pset_WallCommon
          1 x IFCWALLSTANDARDCASE | object type "Basic Wall:Aart_Betonvæg_200mm:373627" | names: "Basic Wall:Aart_Betonvæg_200mm:3025837" | material: layers "Basic Wall:Aart_Betonvæg_200mm" ("Aart_beton" 200.) | property sets: PSet_Revit_Structural, PSet_Revit_Constraints, PSet_Revit_Identity Data, PSet_Revit_Phasing, PSet_Revit_Dimensions, Pset_WallCommon
          34 x IFCWALLSTANDARDCASE | object type "Basic Wall:242.1_Type_1.1_Gipsvæg_124mm_Indv. vegge:7478708" | names: "Basic Wall:242.1_Type_1.1_Gipsvæg_124mm_Indv. vegge:3559585", "Basic Wall:242.1_Type_1.1_Gipsvæg_124mm_Indv. vegge:3565096", "Basic Wall:242.1_Type_1.1_Gipsvæg_124mm_Indv. vegge:3566670" (+31 more) | material: layers "Basic Wall:242.1_Type_1.1_Gipsvæg_124mm_Indv. vegge" ("Aart_Gips" 13., "A-Wood" 98., "Aart_Gips" 13.) | property sets: PSet_Revit_Structural, PSet_Revit_Constraints, PSet_Revit_Identity Data, PSet_Revit_Phasing, PSet_Revit_Dimensions, Pset_WallCommon
          23 x IFCWALLSTANDARDCASE | object type "Basic Wall:242.7_Type_3.1_Gipsvæg_111mm_Sjakt:17953268" | names: "Basic Wall:242.7_Type_3.1_Gipsvæg_111mm_Sjakt:3628044", "Basic Wall:242.7_Type_3.1_Gipsvæg_111mm_Sjakt:3628108", "Basic Wall:242.7_Type_3.1_Gipsvæg_111mm_Sjakt:3628197" (+20 more) | material: layers "Basic Wall:242.7_Type_3.1_Gipsvæg_111mm_Sjakt" ("Aart_Gips" 13., "A-Wood" 98.) | property sets: PSet_Revit_Structural, PSet_Revit_Constraints, PSet_Revit_Identity Data, PSet_Revit_Phasing, PSet_Revit_Dimensions, Pset_WallCommon
          10 x IFCWALLSTANDARDCASE | object type "Basic Wall:242.3_Type_2.1_Gipsvæg_147mm_Indv. vegge_Bad:7797675" | names: "Basic Wall:242.3_Type_2.1_Gipsvæg_147mm_Indv. vegge_Bad:3628045", "Basic Wall:242.3_Type_2.1_Gipsvæg_147mm_Indv. vegge_Bad:3628198", "Basic Wall:242.3_Type_2.1_Gipsvæg_147mm_Indv. vegge_Bad:3628201" (+7 more) | material: layers "Basic Wall:242.3_Type_2.1_Gipsvæg_147mm_Indv. vegge_Bad" ("Aart_Gips" 13., "A-Wood" 98., "Aart_Gips" 26., "Aart_Flise" 10.) | property sets: PSet_Revit_Structural, PSet_Revit_Constraints, PSet_Revit_Identity Data, PSet_Revit_Phasing, PSet_Revit_Dimensions, Pset_WallCommon
          1 x IFCWALL | object type "Basic Wall:242.13_Type_2.2_Gipsvæg_197mm_Påforing Bad:7797614" | names: "Basic Wall:242.13_Type_2.2_Gipsvæg_197mm_Påforing Bad:3628237" | material: layers "Basic Wall:242.13_Type_2.2_Gipsvæg_197mm_Påforing Bad" ("Aart_Flise" 10., "Aart_Gips" 26., "Wood" 148., "Aart_Gips" 13.) | property sets: PSet_Revit_Structural, PSet_Revit_Constraints, PSet_Revit_Identity Data, PSet_Revit_Phasing, PSet_Revit_Dimensions, Pset_WallCommon
          2 x IFCWALLSTANDARDCASE | object type "Basic Wall:242.8_Type_3.3_Gipsvæg_134mm_Sjakt:7797367" | names: "Basic Wall:242.8_Type_3.3_Gipsvæg_134mm_Sjakt:3628238", "Basic Wall:242.8_Type_3.3_Gipsvæg_134mm_Sjakt:3628255" | material: layers "Basic Wall:242.8_Type_3.3_Gipsvæg_134mm_Sjakt" ("Aart_Flise" 10., "Aart_Gips" 26., "A-Wood" 98.) | property sets: PSet_Revit_Structural, PSet_Revit_Constraints, PSet_Revit_Identity Data, PSet_Revit_Phasing, PSet_Revit_Dimensions, Pset_WallCommon
          2 x IFCWALLSTANDARDCASE | object type "Basic Wall:242.13_Type_2.2_Gipsvæg_197mm_Påforing Bad:7797614" | names: "Basic Wall:242.13_Type_2.2_Gipsvæg_197mm_Påforing Bad:3628302", "Basic Wall:242.13_Type_2.2_Gipsvæg_197mm_Påforing Bad:4045802" | material: layers "Basic Wall:242.13_Type_2.2_Gipsvæg_197mm_Påforing Bad" ("Aart_Flise" 10., "Aart_Gips" 26., "Wood" 148., "Aart_Gips" 13.) | property sets: PSet_Revit_Structural, PSet_Revit_Constraints, PSet_Revit_Identity Data, PSet_Revit_Phasing, PSet_Revit_Dimensions, Pset_WallCommon
          1 x IFCWALLSTANDARDCASE | object type "Basic Wall:Aart_Gipsvæg_100mm:937848" | names: "Basic Wall:Aart_Gipsvæg_100mm:3977602" | material: layers "Basic Wall:Aart_Gipsvæg_100mm" ("Aart_Flise" 10., "Element vegg" 50., "Aart_Flise" 10.) | property sets: PSet_Revit_Structural, PSet_Revit_Constraints, PSet_Revit_Identity Data, PSet_Revit_Phasing, PSet_Revit_Dimensions, Pset_WallCommon
          1 x IFCBUILDINGELEMENTPROXY | object type "0box" | names: "0box4:0box:0box:5257441" | property sets: PSet_Revit_Constraints, PSet_Revit_Identity Data, PSet_Revit_Phasing, PSet_Revit_Type_Identity Data
          1 x IFCWALL | object type "Basic Wall:242.3_Type_2.1_Gipsvæg_147mm_Indv. vegge_Bad:7797675" | names: "Basic Wall:242.3_Type_2.1_Gipsvæg_147mm_Indv. vegge_Bad:8864607" | material: layers "Basic Wall:242.3_Type_2.1_Gipsvæg_147mm_Indv. vegge_Bad" ("Aart_Gips" 13., "A-Wood" 98., "Aart_Gips" 26., "Aart_Flise" 10.) | property sets: PSet_Revit_Structural, PSet_Revit_Constraints, PSet_Revit_Identity Data, PSet_Revit_Phasing, PSet_Revit_Dimensions, Pset_WallCommon
          2 x IFCWALLSTANDARDCASE | object type "Basic Wall:242.9_Type_4.1_Gipsvæg_86mm_Påforing elevator:8492360" | names: "Basic Wall:242.9_Type_4.1_Gipsvæg_86mm_Påforing elevator:8872568", "Basic Wall:242.9_Type_4.1_Gipsvæg_86mm_Påforing elevator:8873660" | material: layers "Basic Wall:242.9_Type_4.1_Gipsvæg_86mm_Påforing elevator" ("A-Wood" 73., "Aart_Gips" 13.) | property sets: PSet_Revit_Structural, PSet_Revit_Constraints, PSet_Revit_Identity Data, PSet_Revit_Phasing, PSet_Revit_Dimensions, Pset_WallCommon
          2 x IFCWALLSTANDARDCASE | object type "Basic Wall:242.11_Type_4.3_Gipsvæg_124mm_påforing elevator:7479952" | names: "Basic Wall:242.11_Type_4.3_Gipsvæg_124mm_påforing elevator:8872667", "Basic Wall:242.11_Type_4.3_Gipsvæg_124mm_påforing elevator:8873562" | material: layers "Basic Wall:242.11_Type_4.3_Gipsvæg_124mm_påforing elevator" ("Aart_Gips" 26., "Wood" 98.) | property sets: PSet_Revit_Structural, PSet_Revit_Constraints, PSet_Revit_Identity Data, PSet_Revit_Phasing, PSet_Revit_Dimensions, Pset_WallCommon
          2 x IFCWALLSTANDARDCASE | object type "Basic Wall:242.3_Type_3.5_Gipsvæg_197mm_Indv. vegge_Bad:16140526" | names: "Basic Wall:242.3_Type_3.5_Gipsvæg_197mm_Indv. vegge_Bad:8878114", "Basic Wall:242.3_Type_3.5_Gipsvæg_197mm_Indv. vegge_Bad:9010685" | material: layers "Basic Wall:242.3_Type_3.5_Gipsvæg_197mm_Indv. vegge_Bad" ("Aart_Gips" 13., "A-Wood" 148., "Aart_Gips" 26., "Aart_Flise" 10.) | property sets: PSet_Revit_Structural, PSet_Revit_Constraints, PSet_Revit_Identity Data, PSet_Revit_Phasing, PSet_Revit_Dimensions, Pset_WallCommon
          2 x IFCWALL | object type "Basic Wall:242.11_Type_4.3_Gipsvæg_124mm_påforing elevator:7479952" | names: "Basic Wall:242.11_Type_4.3_Gipsvæg_124mm_påforing elevator:9442204", "Basic Wall:242.11_Type_4.3_Gipsvæg_124mm_påforing elevator:9729507" | material: layers "Basic Wall:242.11_Type_4.3_Gipsvæg_124mm_påforing elevator" ("Aart_Gips" 26., "Wood" 98.) | property sets: PSet_Revit_Structural, PSet_Revit_Constraints, PSet_Revit_Identity Data, PSet_Revit_Phasing, PSet_Revit_Dimensions, Pset_WallCommon
          19 x IFCBUILDINGELEMENTPROXY | object type "Lodret" | names: "Beklædning - Drypkant - Vandbord, underkant:Lodret:Lodret:21514329", "Beklædning - Drypkant - Vandbord, underkant:Lodret:Lodret:21517238", "Beklædning - Drypkant - Vandbord, underkant:Lodret:Lodret:21517715" (+16 more) | property sets: PSet_Revit_Dimensions, PSet_Revit_Constraints, PSet_Revit_Identity Data, PSet_Revit_Phasing, PSet_Revit_Type_Dimensions, PSet_Revit_Type_General
          2 x IFCBUILDINGELEMENTPROXY | object type "350 mm beslag_Næring" | names: "Beslag_næring:350 mm beslag_Næring:350 mm beslag_Næring:21880910", "Beslag_næring:350 mm beslag_Næring:350 mm beslag_Næring:21880928" | property sets: PSet_Revit_Dimensions, PSet_Revit_Other, PSet_Revit_Constraints, PSet_Revit_Identity Data, PSet_Revit_Phasing, PSet_Revit_Type_Constraints
          1 x IFCWINDOW | type IFCWINDOWSTYLE "4188x2088" | object type "4188x2088" | names: "234.25_H_Udv._vindu_1fag_PAR:4188x2088:4188x2088:21880914" | property sets: Pset_WindowCommon, PSet_Revit_Other, PSet_Revit_Constraints, PSet_Revit_Visibility, PSet_Revit_Identity Data, PSet_Revit_General
          2 x IFCWINDOW | type IFCWINDOWSTYLE "2688x2088" | object type "2688x2088" | names: "234.25_F_Udv._vindu_1fag_PAR_us:2688x2088:2688x2088:21880919", "234.25_F_Udv._vindu_1fag_PAR_us:2688x2088:2688x2088:21880923" | property sets: Pset_WindowCommon, PSet_Revit_Other, PSet_Revit_Constraints, PSet_Revit_Visibility, PSet_Revit_Identity Data, PSet_Revit_Phasing
          1 x IFCBUILDINGELEMENTPROXY | object type "450 mm beslag_Næring" | names: "Beslag_næring:450 mm beslag_Næring:450 mm beslag_Næring:21880924" | property sets: PSet_Revit_Dimensions, PSet_Revit_Other, PSet_Revit_Constraints, PSet_Revit_Identity Data, PSet_Revit_Phasing, PSet_Revit_Type_Constraints
          1 x IFCWINDOW | type IFCWINDOWSTYLE "3888x2088" | object type "3888x2088" | names: "234.25_H_Udv._vindu_1fag_PAR:3888x2088:3888x2088:21880929" | property sets: Pset_WindowCommon, PSet_Revit_Other, PSet_Revit_Constraints, PSet_Revit_Visibility, PSet_Revit_Identity Data, PSet_Revit_General
          1 x IFCDOOR | type IFCDOORSTYLE "2388 x 2488 (næring)" | object type "2388 x 2488 (næring)" | names: "234.18_H24-:2388 x 2488 (næring):2388 x 2488 (næring):21880930" | property sets: Pset_DoorCommon, PSet_Revit_Dimensions, PSet_Revit_Other, PSet_Revit_Constraints, PSet_Revit_Identity Data, PSet_Revit_Phasing
          1 x IFCBUILDINGELEMENTPROXY | object type "Tilpasningsbeslag_Næring" | names: "Beslag_næring:Tilpasningsbeslag_Næring:Tilpasningsbeslag_Næring:21880937" | property sets: PSet_Revit_Dimensions, PSet_Revit_Other, PSet_Revit_Constraints, PSet_Revit_Identity Data, PSet_Revit_Phasing, PSet_Revit_Type_Constraints
          1 x IFCDOOR | type IFCDOORSTYLE "2388 x 2488 (næring)" | object type "2388 x 2488 (næring)" | names: "234.18_V24_Næring:2388 x 2488 (næring):2388 x 2488 (næring):21880939" | property sets: Pset_DoorCommon, PSet_Revit_Dimensions, PSet_Revit_Other, PSet_Revit_Constraints, PSet_Revit_Identity Data, PSet_Revit_Phasing
          1 x IFCWINDOW | type IFCWINDOWSTYLE "2988x2088" | object type "2988x2088" | names: "234.25_H_Udv._vindu_1fag_PAR:2988x2088:2988x2088:21880943" | property sets: Pset_WindowCommon, PSet_Revit_Other, PSet_Revit_Constraints, PSet_Revit_Visibility, PSet_Revit_Identity Data, PSet_Revit_General
          1 x IFCWALLSTANDARDCASE | object type "Basic Wall:242.12_Type_3.4_Gipsvæg_184mm_Påforing Bad_Sjakt:8098014" | names: "Basic Wall:242.12_Type_3.4_Gipsvæg_184mm_Påforing Bad_Sjakt:22316327" | material: layers "Basic Wall:242.12_Type_3.4_Gipsvæg_184mm_Påforing Bad_Sjakt" ("Aart_Flise" 10., "Aart_Gips" 26., "Wood" 148.) | property sets: PSet_Revit_Structural, PSet_Revit_Constraints, PSet_Revit_Identity Data, PSet_Revit_Phasing, PSet_Revit_Dimensions, Pset_WallCommon
      IFCBUILDINGSTOREY "01" | elevation 0.
        contains 116 elements
          2 x IFCSLAB | object type "Floor:Etasjedekk_250mm_betong" | FLOOR | names: "Floor:Etasjedekk_250mm_betong:847166", "Floor:Etasjedekk_250mm_betong:847166:2" | material: layers "Floor:Etasjedekk_250mm_betong" ("Aart_beton" 250.) | property sets: PSet_Revit_Constraints, PSet_Revit_Structural, PSet_Revit_Identity Data, PSet_Revit_Phasing, PSet_Revit_Dimensions, Pset_SlabCommon
          5 x IFCSLAB | object type "Floor:Gulvopbygning_400mm" | FLOOR | names: "Floor:Gulvopbygning_400mm:848059", "Floor:Gulvopbygning_400mm:848059:2", "Floor:Gulvopbygning_400mm:848059:3" (+2 more) | material: layers "Floor:Gulvopbygning_400mm" ("Wood" 14., "Wood" 22., "Aart_isolering" 364.) | property sets: PSet_Revit_Constraints, PSet_Revit_Structural, PSet_Revit_Identity Data, PSet_Revit_Phasing, PSet_Revit_Dimensions, Pset_SlabCommon
          1 x IFCSTAIR | object type "Stair:Trappeopgang" | names: "Stair:Trappeopgang:1517262" | parts: 2 IFCRAILING, 1 IFCSTAIR | property sets: Pset_StairCommon, PSet_Revit_Dimensions, PSet_Revit_Constraints, PSet_Revit_Graphics, PSet_Revit_Identity Data, PSet_Revit_Phasing
          1 x IFCDOOR | type IFCDOORSTYLE "M10x21" | object type "M10x21" | names: "Hoveddør_Leilighet:M10x21:M10x21:1517573" | property sets: Pset_DoorCommon, PSet_Revit_Other, PSet_Revit_Constraints, PSet_Revit_Identity Data, PSet_Revit_Construction, PSet_Revit_Text
          2 x IFCWALLSTANDARDCASE | object type "Basic Wall:241.3_Betonvæg_250mm:373623" | names: "Basic Wall:241.3_Betonvæg_250mm:3026288", "Basic Wall:241.3_Betonvæg_250mm:3804899" | material: layers "Basic Wall:241.3_Betonvæg_250mm" ("Aart_beton" 250.) | property sets: PSet_Revit_Structural, PSet_Revit_Constraints, PSet_Revit_Identity Data, PSet_Revit_Phasing, PSet_Revit_Dimensions, Pset_WallCommon
          3 x IFCDOOR | type IFCDOORSTYLE "M9x21" | object type "M9x21" | names: "Int_door_Aart:M9x21:M9x21:3628180", "Int_door_Aart:M9x21:M9x21:3628241", "Int_door_Aart:M9x21:M9x21:18980493" | property sets: Pset_DoorCommon, PSet_Revit_Other, PSet_Revit_Dimensions, PSet_Revit_Constraints, PSet_Revit_Identity Data, PSet_Revit_Phasing
          7 x IFCDOOR | type IFCDOORSTYLE "M9x21" | object type "M9x21" | names: "Int_door_Aart:M9x21:M9x21:3628187", "Int_door_Aart:M9x21:M9x21:3628202", "Int_door_Aart:M9x21:M9x21:3628257" (+4 more) | property sets: Pset_DoorCommon, PSet_Revit_Other, PSet_Revit_Dimensions, PSet_Revit_Constraints, PSet_Revit_Identity Data, PSet_Revit_Phasing
          1 x IFCDOOR | type IFCDOORSTYLE "M9x21" | object type "M9x21" | names: "Int_door_Aart:M9x21:M9x21:3628223" | property sets: Pset_DoorCommon, PSet_Revit_Other, PSet_Revit_Dimensions, PSet_Revit_Constraints, PSet_Revit_Identity Data, PSet_Revit_Phasing
          1 x IFCDOOR | type IFCDOORSTYLE "M9x21" | object type "M9x21" | names: "DAN_Indv. Skydedør i væg:M9x21:M9x21:3628231" | property sets: Pset_DoorCommon, PSet_Revit_Other, PSet_Revit_Materials and Finishes, PSet_Revit_Constraints, PSet_Revit_Identity Data, PSet_Revit_Phasing
          3 x IFCDOOR | type IFCDOORSTYLE "M9x21" | object type "M9x21" | names: "Int_door_Aart:M9x21:M9x21:3628242", "Int_door_Aart:M9x21:M9x21:3628258", "Int_door_Aart:M9x21:M9x21:4045799" | property sets: Pset_DoorCommon, PSet_Revit_Other, PSet_Revit_Dimensions, PSet_Revit_Constraints, PSet_Revit_Identity Data, PSet_Revit_Phasing
          1 x IFCDOOR | type IFCDOORSTYLE "M9x21" | object type "M9x21" | names: "DAN_Indv. Skydedør i væg:M9x21:M9x21:3628243" | property sets: Pset_DoorCommon, PSet_Revit_Other, PSet_Revit_Materials and Finishes, PSet_Revit_Constraints, PSet_Revit_Identity Data, PSet_Revit_Phasing
          1 x IFCWALLSTANDARDCASE | object type "Basic Wall:242.13_Type_2.2_Gipsvæg_197mm_Påforing Bad:7797614" | names: "Basic Wall:242.13_Type_2.2_Gipsvæg_197mm_Påforing Bad:3628550" | material: layers "Basic Wall:242.13_Type_2.2_Gipsvæg_197mm_Påforing Bad" ("Aart_Flise" 10., "Aart_Gips" 26., "Wood" 148., "Aart_Gips" 13.) | property sets: PSet_Revit_Structural, PSet_Revit_Constraints, PSet_Revit_Identity Data, PSet_Revit_Phasing, PSet_Revit_Dimensions, Pset_WallCommon
          2 x IFCWALLSTANDARDCASE | object type "Basic Wall:242.8_Type_3.3_Gipsvæg_134mm_Sjakt:7797367" | names: "Basic Wall:242.8_Type_3.3_Gipsvæg_134mm_Sjakt:3628551", "Basic Wall:242.8_Type_3.3_Gipsvæg_134mm_Sjakt:15771081" | material: layers "Basic Wall:242.8_Type_3.3_Gipsvæg_134mm_Sjakt" ("Aart_Flise" 10., "Aart_Gips" 26., "A-Wood" 98.) | property sets: PSet_Revit_Structural, PSet_Revit_Constraints, PSet_Revit_Identity Data, PSet_Revit_Phasing, PSet_Revit_Dimensions, Pset_WallCommon
          1 x IFCDOOR | type IFCDOORSTYLE "M10x21" | object type "M10x21" | names: "Utv. dør_Leilighet:M10x21:M10x21:3669763" | property sets: Pset_DoorCommon, PSet_Revit_Other, PSet_Revit_Constraints, PSet_Revit_Identity Data, PSet_Revit_Construction, PSet_Revit_Text
          1 x IFCDOOR | type IFCDOORSTYLE "M10x21" | object type "M10x21" | names: "Utv. dør_Leilighet:M10x21:M10x21:3669764" | property sets: Pset_DoorCommon, PSet_Revit_Other, PSet_Revit_Constraints, PSet_Revit_Identity Data, PSet_Revit_Construction, PSet_Revit_Text
          1 x IFCDOOR | type IFCDOORSTYLE "M10x21" | object type "M10x21" | names: "Hoveddør_Leilighet:M10x21:M10x21:3803965" | property sets: Pset_DoorCommon, PSet_Revit_Other, PSet_Revit_Constraints, PSet_Revit_Identity Data, PSet_Revit_Construction, PSet_Revit_Text
          2 x IFCWALLSTANDARDCASE | object type "Basic Wall:242.7_Type_3.1_Gipsvæg_111mm_Sjakt:17953268" | names: "Basic Wall:242.7_Type_3.1_Gipsvæg_111mm_Sjakt:4001792", "Basic Wall:242.7_Type_3.1_Gipsvæg_111mm_Sjakt:4048311" | material: layers "Basic Wall:242.7_Type_3.1_Gipsvæg_111mm_Sjakt" ("Aart_Gips" 13., "A-Wood" 98.) | property sets: PSet_Revit_Structural, PSet_Revit_Constraints, PSet_Revit_Identity Data, PSet_Revit_Phasing, PSet_Revit_Dimensions, Pset_WallCommon
          1 x IFCCURTAINWALL | object type "Curtain Wall:243.1_Indv_glasskillevæg:1131477" | names: "Curtain Wall:243.1_Indv_glasskillevæg:4004189" | parts: 1 IFCPLATE | property sets: Pset_CurtainWallCommon, PSet_Revit_Structural, PSet_Revit_Constraints, PSet_Revit_Identity Data, PSet_Revit_Phasing, PSet_Revit_Dimensions
          18 x IFCCOVERING | object type "Compound Ceiling:KRAFT_61mm_Gips_ himling" | CEILING | names: "Compound Ceiling:KRAFT_61mm_Gips_ himling:8881508", "Compound Ceiling:KRAFT_61mm_Gips_ himling:8881517", "Compound Ceiling:KRAFT_61mm_Gips_ himling:8881531" (+15 more) | material: layers "Compound Ceiling:KRAFT_61mm_Gips_ himling" ("A-Air" 48., "Gyproc Gipsplade_2560mm" 13.) | property sets: Pset_CoveringCommon, PSet_Revit_Constraints, PSet_Revit_Identity Data, PSet_Revit_Dimensions, PSet_Revit_Phasing, PSet_Revit_Type_Construction
          2 x IFCWALLSTANDARDCASE | object type "Basic Wall:242.12_Type_3.4_Gipsvæg_184mm_Påforing Bad_Sjakt:8098014" | names: "Basic Wall:242.12_Type_3.4_Gipsvæg_184mm_Påforing Bad_Sjakt:9031663", "Basic Wall:242.12_Type_3.4_Gipsvæg_184mm_Påforing Bad_Sjakt:9031701" | material: layers "Basic Wall:242.12_Type_3.4_Gipsvæg_184mm_Påforing Bad_Sjakt" ("Aart_Flise" 10., "Aart_Gips" 26., "Wood" 148.) | property sets: PSet_Revit_Structural, PSet_Revit_Constraints, PSet_Revit_Identity Data, PSet_Revit_Phasing, PSet_Revit_Dimensions, Pset_WallCommon
          1 x IFCWALLSTANDARDCASE | object type "Basic Wall:242.22_Type_3.7_Gipsvæg_84mm_Indv. vegge_Påforing_Badrom 48/26/10:22152513" | names: "Basic Wall:242.22_Type_3.7_Gipsvæg_84mm_Indv. vegge_Påforing_Badrom 48/26/10:9102900" | material: layers "Basic Wall:242.22_Type_3.7_Gipsvæg_84mm_Indv. vegge_Påforing_Badrom 48/26/10" ("Aart_Flise" 10., "Aart_Gips" 26., "A-Wood" 48.) | property sets: PSet_Revit_Structural, PSet_Revit_Constraints, PSet_Revit_Identity Data, PSet_Revit_Phasing, PSet_Revit_Dimensions, Pset_WallCommon
          6 x IFCSLAB | object type "Floor:Gulvopbygning_400mm_Bad" | FLOOR | names: "Floor:Gulvopbygning_400mm_Bad:9167635", "Floor:Gulvopbygning_400mm_Bad:9167635:2", "Floor:Gulvopbygning_400mm_Bad:9167635:3" (+3 more) | material: layers "Floor:Gulvopbygning_400mm_Bad" ("Stone (2)" 12., "A-Conc" 100., "Aart_isolering" 288.) | property sets: PSet_Revit_Constraints, PSet_Revit_Structural, PSet_Revit_Identity Data, PSet_Revit_Phasing, PSet_Revit_Dimensions, Pset_SlabCommon
          1 x IFCWALLSTANDARDCASE | object type "Basic Wall:242.17_Fliser_10mm:7816687" | names: "Basic Wall:242.17_Fliser_10mm:9200438" | material: layers "Basic Wall:242.17_Fliser_10mm" ("Aart_Flise" 10.) | property sets: PSet_Revit_Structural, PSet_Revit_Constraints, PSet_Revit_Identity Data, PSet_Revit_Phasing, PSet_Revit_Dimensions, Pset_WallCommon
          4 x IFCRAILING | object type "Railing:rekkverk_vinduer_type1_(1000mm)" | names: "Railing:rekkverk_vinduer_type1_(1000mm):11768708", "Railing:rekkverk_vinduer_type1_(1000mm):11768716", "Railing:rekkverk_vinduer_type1_(1000mm):11768724" (+1 more) | material: "Wood - Timber" | property sets: Pset_RailingCommon, PSet_Revit_Dimensions, PSet_Revit_Constraints, PSet_Revit_Identity Data, PSet_Revit_Phasing, PSet_Revit_Type_Construction
          2 x IFCWINDOW | type IFCWINDOWSTYLE "Skyveparti_2088x2288mm" | object type "Skyveparti_2088x2288mm" | names: "234.2_V_Udv._skyveparti_3fag Nytt:Skyveparti_2088x2288mm:Skyveparti_2088x2288mm:14707756", "234.2_V_Udv._skyveparti_3fag Nytt:Skyveparti_2088x2288mm:Skyveparti_2088x2288mm:14707759" | property sets: Pset_WindowCommon, PSet_Revit_Other, PSet_Revit_Dimensions, PSet_Revit_Constraints, PSet_Revit_Identity Data, PSet_Revit_Phasing
          4 x IFCWINDOW | type IFCWINDOWSTYLE "1188x1488 mm" | object type "1188x1488 mm" | names: "234.3_V_Udv._vindu_1fag(nytt):1188x1488 mm:1188x1488 mm:14707757", "234.3_V_Udv._vindu_1fag(nytt):1188x1488 mm:1188x1488 mm:14707758", "234.3_V_Udv._vindu_1fag(nytt):1188x1488 mm:1188x1488 mm:14707762" (+1 more) | property sets: Pset_WindowCommon, PSet_Revit_Other, PSet_Revit_Dimensions, PSet_Revit_Graphics, PSet_Revit_Constraints, PSet_Revit_Identity Data
          1 x IFCDOOR | type IFCDOORSTYLE "2388 x 2288" | object type "2388 x 2288" | names: "234.18_H24 Nytt:2388 x 2288:2388 x 2288:14707761" | property sets: Pset_DoorCommon, PSet_Revit_Dimensions, PSet_Revit_Other, PSet_Revit_Constraints, PSet_Revit_Identity Data, PSet_Revit_Phasing
          1 x IFCSLAB | object type "Floor:Repos_250mm_betong" | FLOOR | names: "Floor:Repos_250mm_betong:14876246" | material: layers "Floor:Repos_250mm_betong" ("Aart_beton" 250.) | property sets: PSet_Revit_Constraints, PSet_Revit_Structural, PSet_Revit_Identity Data, PSet_Revit_Phasing, PSet_Revit_Dimensions, Pset_SlabCommon
          2 x IFCWALLSTANDARDCASE | object type "Basic Wall:242.3_Type_2.1_Gipsvæg_147mm_Indv. vegge_Bad:7797675" | names: "Basic Wall:242.3_Type_2.1_Gipsvæg_147mm_Indv. vegge_Bad:15770620", "Basic Wall:242.3_Type_2.1_Gipsvæg_147mm_Indv. vegge_Bad:15770762" | material: layers "Basic Wall:242.3_Type_2.1_Gipsvæg_147mm_Indv. vegge_Bad" ("Aart_Gips" 13., "A-Wood" 98., "Aart_Gips" 26., "Aart_Flise" 10.) | property sets: PSet_Revit_Structural, PSet_Revit_Constraints, PSet_Revit_Identity Data, PSet_Revit_Phasing, PSet_Revit_Dimensions, Pset_WallCommon
          1 x IFCWALLSTANDARDCASE | object type "Basic Wall:Aart_Betonvæg_200mm:373627" | names: "Basic Wall:Aart_Betonvæg_200mm:18471424" | material: layers "Basic Wall:Aart_Betonvæg_200mm" ("Aart_beton" 200.) | property sets: PSet_Revit_Structural, PSet_Revit_Constraints, PSet_Revit_Identity Data, PSet_Revit_Phasing, PSet_Revit_Dimensions, Pset_WallCommon
          1 x IFCRAILING | object type "Railing:Rekkverk_hovedtrappe_lysning_1000mm" | names: "Railing:Rekkverk_hovedtrappe_lysning_1000mm:18471483" | property sets: Pset_RailingCommon, PSet_Revit_Dimensions, PSet_Revit_Constraints, PSet_Revit_Identity Data, PSet_Revit_Phasing, PSet_Revit_Type_Construction
          1 x IFCWALLSTANDARDCASE | object type "Basic Wall:242.20_Type_5.1_Eikespiler_36mm_Indv. hagestue:19455957" | names: "Basic Wall:242.20_Type_5.1_Eikespiler_36mm_Indv. hagestue:19553221" | material: layers "Basic Wall:242.20_Type_5.1_Eikespiler_36mm_Indv. hagestue" ("Wood - Eikespiler" 36.) | property sets: PSet_Revit_Structural, PSet_Revit_Constraints, PSet_Revit_Identity Data, PSet_Revit_Phasing, PSet_Revit_Dimensions, Pset_WallCommon
          1 x IFCDOOR | type IFCDOORSTYLE "M11x21" | object type "M11x21" | names: "DAN_Indv. Skydedør i væg:M11x21:M11x21:19561768" | property sets: Pset_DoorCommon, PSet_Revit_Other, PSet_Revit_Materials and Finishes, PSet_Revit_Constraints, PSet_Revit_Identity Data, PSet_Revit_Phasing
          1 x IFCDOOR | type IFCDOORSTYLE "M11x21" | object type "M11x21" | names: "DAN_Indv. Skydedør i væg:M11x21:M11x21:19562058" | property sets: Pset_DoorCommon, PSet_Revit_Other, PSet_Revit_Materials and Finishes, PSet_Revit_Constraints, PSet_Revit_Identity Data, PSet_Revit_Phasing
          3 x IFCWINDOW | type IFCWINDOWSTYLE "1188 x 1488mm" | object type "1188 x 1488mm" | names: "234.3_V_Udv._vindu_1fag_PAR:1188 x 1488mm:1188 x 1488mm:20288245", "234.3_V_Udv._vindu_1fag_PAR:1188 x 1488mm:1188 x 1488mm:21187672", "234.3_V_Udv._vindu_1fag_PAR:1188 x 1488mm:1188 x 1488mm:21188050" | property sets: Pset_WindowCommon, PSet_Revit_Other, PSet_Revit_Constraints, PSet_Revit_Visibility, PSet_Revit_Identity Data, PSet_Revit_General
          1 x IFCDOOR | type IFCDOORSTYLE "M9x21" | object type "M9x21" | names: "DAN_Indv. Skydedør i væg:M9x21:M9x21:20697993" | property sets: Pset_DoorCommon, PSet_Revit_Other, PSet_Revit_Materials and Finishes, PSet_Revit_Constraints, PSet_Revit_Identity Data, PSet_Revit_Phasing
          1 x IFCDOOR | type IFCDOORSTYLE "M8x21" | object type "M8x21" | names: "Int_door_Aart:M8x21:M8x21:20698194" | property sets: Pset_DoorCommon, PSet_Revit_Other, PSet_Revit_Dimensions, PSet_Revit_Constraints, PSet_Revit_Identity Data, PSet_Revit_Phasing
          1 x IFCCOVERING | object type "Compound Ceiling:kraft_Himling_Akustikkflåte" | CEILING | names: "Compound Ceiling:kraft_Himling_Akustikkflåte:20800403" | material: layers "Compound Ceiling:kraft_Himling_Akustikkflåte" ("Ceiling Tile 600 x 600" 40.) | property sets: Pset_CoveringCommon, PSet_Revit_Constraints, PSet_Revit_Identity Data, PSet_Revit_Dimensions, PSet_Revit_Phasing, PSet_Revit_Type_Construction
          1 x IFCWINDOW | type IFCWINDOWSTYLE "2988x2288mm" | object type "2988x2288mm" | names: "234.7_H_Udv._vindu_høyt_3fag_PAR:2988x2288mm:2988x2288mm:21170239" | property sets: Pset_WindowCommon, PSet_Revit_Other, PSet_Revit_Constraints, PSet_Revit_Visibility, PSet_Revit_Identity Data, PSet_Revit_General
          1 x IFCWINDOW | type IFCWINDOWSTYLE "1188 x 1488mm" | object type "1188 x 1488mm" | names: "234.3_H_Udv._vindu_1fag_PAR:1188 x 1488mm:1188 x 1488mm:21170258" | property sets: Pset_WindowCommon, PSet_Revit_Other, PSet_Revit_Constraints, PSet_Revit_Visibility, PSet_Revit_Identity Data, PSet_Revit_General
          1 x IFCWINDOW | type IFCWINDOWSTYLE "2988x2288mm" | object type "2988x2288mm" | names: "234.7_V_Udv._vindu_høyt_3fag_PAR:2988x2288mm:2988x2288mm:21182629" | property sets: Pset_WindowCommon, PSet_Revit_Other, PSet_Revit_Constraints, PSet_Revit_Visibility, PSet_Revit_Identity Data, PSet_Revit_General
          1 x IFCWINDOW | type IFCWINDOWSTYLE "Skyveparti_2688x2288mm" | object type "Skyveparti_2688x2288mm" | names: "234.2_V_Udv._skyveparti_3fag Nytt:Skyveparti_2688x2288mm:Skyveparti_2688x2288mm:21188430" | property sets: Pset_WindowCommon, PSet_Revit_Other, PSet_Revit_Dimensions, PSet_Revit_Constraints, PSet_Revit_Identity Data, PSet_Revit_Phasing
          1 x IFCWINDOW | type IFCWINDOWSTYLE "Skyveparti_2388x2288mm" | object type "Skyveparti_2388x2288mm" | names: "234.2_V_Udv._skyveparti_3fag Nytt:Skyveparti_2388x2288mm:Skyveparti_2388x2288mm:21188804" | property sets: Pset_WindowCommon, PSet_Revit_Other, PSet_Revit_Dimensions, PSet_Revit_Constraints, PSet_Revit_Identity Data, PSet_Revit_Phasing
          22 x IFCBUILDINGELEMENTPROXY | object type "Lodret" | names: "Beklædning - Drypkant - Vandbord, underkant:Lodret:Lodret:21513551", "Beklædning - Drypkant - Vandbord, overkant:Lodret:Lodret:21513650", "Beklædning - Drypkant - Vandbord, overkant:Lodret:Lodret:21513779" (+19 more) | property sets: PSet_Revit_Dimensions, PSet_Revit_Constraints, PSet_Revit_Identity Data, PSet_Revit_Phasing, PSet_Revit_Type_Dimensions, PSet_Revit_Type_General
      IFCBUILDINGSTOREY "02" | elevation 2900.
        contains 216 elements
          1 x IFCSLAB | object type "Floor:Etasjedekk_250mm_betong" | FLOOR | names: "Floor:Etasjedekk_250mm_betong:848419" | material: layers "Floor:Etasjedekk_250mm_betong" ("Aart_beton" 250.) | property sets: PSet_Revit_Constraints, PSet_Revit_Structural, PSet_Revit_Identity Data, PSet_Revit_Phasing, PSet_Revit_Dimensions, Pset_SlabCommon
          4 x IFCSLAB | object type "Floor:Gulvopbygning_30mm" | FLOOR | names: "Floor:Gulvopbygning_30mm:848427", "Floor:Gulvopbygning_30mm:848427:2", "Floor:Gulvopbygning_30mm:848427:3" (+1 more) | material: layers "Floor:Gulvopbygning_30mm" ("Wood - Flooring" 14., "Aart_Gips" 16.) | property sets: PSet_Revit_Constraints, PSet_Revit_Structural, PSet_Revit_Identity Data, PSet_Revit_Phasing, PSet_Revit_Dimensions, Pset_SlabCommon
          1 x IFCWALLSTANDARDCASE | object type "Basic Wall:241.2_Lejlighedsskel_betonvæg_220mm:7107552" | names: "Basic Wall:241.2_Lejlighedsskel_betonvæg_220mm:897640" | material: layers "Basic Wall:241.2_Lejlighedsskel_betonvæg_220mm" ("Aart_beton" 220.) | property sets: PSet_Revit_Structural, PSet_Revit_Constraints, PSet_Revit_Identity Data, PSet_Revit_Phasing, PSet_Revit_Dimensions, Pset_WallCommon
          1 x IFCWALLSTANDARDCASE | object type "Basic Wall:241.3_Betonvæg_250mm:373623" | names: "Basic Wall:241.3_Betonvæg_250mm:1517238" | material: layers "Basic Wall:241.3_Betonvæg_250mm" ("Aart_beton" 250.) | property sets: PSet_Revit_Structural, PSet_Revit_Constraints, PSet_Revit_Identity Data, PSet_Revit_Phasing, PSet_Revit_Dimensions, Pset_WallCommon
          1 x IFCSTAIR | object type "Stair:Trappeopgang" | names: "Stair:Trappeopgang:1517243" | parts: 3 IFCRAILING, 1 IFCSTAIR | property sets: Pset_StairCommon, PSet_Revit_Dimensions, PSet_Revit_Constraints, PSet_Revit_Graphics, PSet_Revit_Identity Data, PSet_Revit_Phasing
          1 x IFCSLAB | object type "Floor:Repos_200mm_betong" | FLOOR | names: "Floor:Repos_200mm_betong:1517310" | material: layers "Floor:Repos_200mm_betong" ("Aart_beton" 200.) | property sets: PSet_Revit_Constraints, PSet_Revit_Structural, PSet_Revit_Identity Data, PSet_Revit_Phasing, PSet_Revit_Dimensions, Pset_SlabCommon
          1 x IFCRAILING | object type "Railing:Rekkverk_hovedtrappe_lysning_990mm" | names: "Railing:Rekkverk_hovedtrappe_lysning_990mm:1517546" | property sets: Pset_RailingCommon, PSet_Revit_Dimensions, PSet_Revit_Constraints, PSet_Revit_Identity Data, PSet_Revit_Phasing, PSet_Revit_Type_Construction
          1 x IFCDOOR | type IFCDOORSTYLE "M10x21" | object type "M10x21" | names: "Hoveddør_Leilighet:M10x21:M10x21:1517571" | property sets: Pset_DoorCommon, PSet_Revit_Other, PSet_Revit_Constraints, PSet_Revit_Identity Data, PSet_Revit_Construction, PSet_Revit_Text
          2 x IFCWINDOW | type IFCWINDOWSTYLE "1188x1488 mm" | object type "1188x1488 mm" | names: "234.3_V_Udv._vindu_1fag(nytt):1188x1488 mm:1188x1488 mm:2380084", "234.3_V_Udv._vindu_1fag(nytt):1188x1488 mm:1188x1488 mm:2380085" | property sets: Pset_WindowCommon, PSet_Revit_Other, PSet_Revit_Dimensions, PSet_Revit_Graphics, PSet_Revit_Constraints, PSet_Revit_Identity Data
          1 x IFCWINDOW | type IFCWINDOWSTYLE "Skyveparti_2088x2288mm" | object type "Skyveparti_2088x2288mm" | names: "234.2_H_Udv._skyveparti_3fag Nytt:Skyveparti_2088x2288mm:Skyveparti_2088x2288mm:3508599" | property sets: Pset_WindowCommon, PSet_Revit_Other, PSet_Revit_Dimensions, PSet_Revit_Constraints, PSet_Revit_Identity Data, PSet_Revit_Phasing
          38 x IFCWALLSTANDARDCASE | object type "Basic Wall:242.1_Type_1.1_Gipsvæg_124mm_Indv. vegge:7478708" | names: "Basic Wall:242.1_Type_1.1_Gipsvæg_124mm_Indv. vegge:3564784", "Basic Wall:242.1_Type_1.1_Gipsvæg_124mm_Indv. vegge:3566984", "Basic Wall:242.1_Type_1.1_Gipsvæg_124mm_Indv. vegge:3628491" (+35 more) | material: layers "Basic Wall:242.1_Type_1.1_Gipsvæg_124mm_Indv. vegge" ("Aart_Gips" 13., "A-Wood" 98., "Aart_Gips" 13.) | property sets: PSet_Revit_Structural, PSet_Revit_Constraints, PSet_Revit_Identity Data, PSet_Revit_Phasing, PSet_Revit_Dimensions, Pset_WallCommon
          25 x IFCWALLSTANDARDCASE | object type "Basic Wall:242.7_Type_3.1_Gipsvæg_111mm_Sjakt:17953268" | names: "Basic Wall:242.7_Type_3.1_Gipsvæg_111mm_Sjakt:3628357", "Basic Wall:242.7_Type_3.1_Gipsvæg_111mm_Sjakt:3628549", "Basic Wall:242.7_Type_3.1_Gipsvæg_111mm_Sjakt:3628574" (+22 more) | material: layers "Basic Wall:242.7_Type_3.1_Gipsvæg_111mm_Sjakt" ("Aart_Gips" 13., "A-Wood" 98.) | property sets: PSet_Revit_Structural, PSet_Revit_Constraints, PSet_Revit_Identity Data, PSet_Revit_Phasing, PSet_Revit_Dimensions, Pset_WallCommon
          7 x IFCDOOR | type IFCDOORSTYLE "M9x21" | object type "M9x21" | names: "Int_door_Aart:M9x21:M9x21:3628493", "Int_door_Aart:M9x21:M9x21:3628556", "Int_door_Aart:M9x21:M9x21:4048306" (+4 more) | property sets: Pset_DoorCommon, PSet_Revit_Other, PSet_Revit_Dimensions, PSet_Revit_Constraints, PSet_Revit_Identity Data, PSet_Revit_Phasing
          11 x IFCWALLSTANDARDCASE | object type "Basic Wall:242.3_Type_2.1_Gipsvæg_147mm_Indv. vegge_Bad:7797675" | names: "Basic Wall:242.3_Type_2.1_Gipsvæg_147mm_Indv. vegge_Bad:3628499", "Basic Wall:242.3_Type_2.1_Gipsvæg_147mm_Indv. vegge_Bad:3917520", "Basic Wall:242.3_Type_2.1_Gipsvæg_147mm_Indv. vegge_Bad:4001785" (+8 more) | material: layers "Basic Wall:242.3_Type_2.1_Gipsvæg_147mm_Indv. vegge_Bad" ("Aart_Gips" 13., "A-Wood" 98., "Aart_Gips" 26., "Aart_Flise" 10.) | property sets: PSet_Revit_Structural, PSet_Revit_Constraints, PSet_Revit_Identity Data, PSet_Revit_Phasing, PSet_Revit_Dimensions, Pset_WallCommon
          7 x IFCDOOR | type IFCDOORSTYLE "M9x21" | object type "M9x21" | names: "Int_door_Aart:M9x21:M9x21:3628500", "Int_door_Aart:M9x21:M9x21:3628570", "Int_door_Aart:M9x21:M9x21:4001787" (+4 more) | property sets: Pset_DoorCommon, PSet_Revit_Other, PSet_Revit_Dimensions, PSet_Revit_Constraints, PSet_Revit_Identity Data, PSet_Revit_Phasing
          2 x IFCCURTAINWALL | object type "Curtain Wall:243.1_Indv_glasskillevæg:1131477" | names: "Curtain Wall:243.1_Indv_glasskillevæg:3628508", "Curtain Wall:243.1_Indv_glasskillevæg:3917522" | parts: 2 IFCPLATE | property sets: Pset_CurtainWallCommon, PSet_Revit_Structural, PSet_Revit_Constraints, PSet_Revit_Identity Data, PSet_Revit_Phasing, PSet_Revit_Dimensions
          2 x IFCDOOR | type IFCDOORSTYLE "M9x21" | object type "M9x21" | names: "Int_door_Aart:M9x21:M9x21:3628519", "Int_door_Aart:M9x21:M9x21:4001790" | property sets: Pset_DoorCommon, PSet_Revit_Other, PSet_Revit_Dimensions, PSet_Revit_Constraints, PSet_Revit_Identity Data, PSet_Revit_Phasing
          4 x IFCDOOR | type IFCDOORSTYLE "M9x21" | object type "M9x21" | names: "Int_door_Aart:M9x21:M9x21:3628571", "Int_door_Aart:M9x21:M9x21:3917531", "Int_door_Aart:M9x21:M9x21:4048309" (+1 more) | property sets: Pset_DoorCommon, PSet_Revit_Other, PSet_Revit_Dimensions, PSet_Revit_Constraints, PSet_Revit_Identity Data, PSet_Revit_Phasing
          1 x IFCDOOR | type IFCDOORSTYLE "M10x21" | object type "M10x21" | names: "Utv. dør_Leilighet:M10x21:M10x21:3669791" | property sets: Pset_DoorCommon, PSet_Revit_Other, PSet_Revit_Constraints, PSet_Revit_Identity Data, PSet_Revit_Construction, PSet_Revit_Text
          1 x IFCDOOR | type IFCDOORSTYLE "M10x21" | object type "M10x21" | names: "Utv. dør_Leilighet:M10x21:M10x21:3669792" | property sets: Pset_DoorCommon, PSet_Revit_Other, PSet_Revit_Constraints, PSet_Revit_Identity Data, PSet_Revit_Construction, PSet_Revit_Text
          3 x IFCWALLSTANDARDCASE | object type "Basic Wall:242.13_Type_2.2_Gipsvæg_197mm_Påforing Bad:7797614" | names: "Basic Wall:242.13_Type_2.2_Gipsvæg_197mm_Påforing Bad:4001791", "Basic Wall:242.13_Type_2.2_Gipsvæg_197mm_Påforing Bad:4048310", "Basic Wall:242.13_Type_2.2_Gipsvæg_197mm_Påforing Bad:9035773" | material: layers "Basic Wall:242.13_Type_2.2_Gipsvæg_197mm_Påforing Bad" ("Aart_Flise" 10., "Aart_Gips" 26., "Wood" 148., "Aart_Gips" 13.) | property sets: PSet_Revit_Structural, PSet_Revit_Constraints, PSet_Revit_Identity Data, PSet_Revit_Phasing, PSet_Revit_Dimensions, Pset_WallCommon
          1 x IFCDOOR | type IFCDOORSTYLE "M10x21" | object type "M10x21" | names: "Hoveddør_Leilighet:M10x21:M10x21:4222725" | property sets: Pset_DoorCommon, PSet_Revit_Other, PSet_Revit_Constraints, PSet_Revit_Identity Data, PSet_Revit_Construction, PSet_Revit_Text
          21 x IFCCOVERING | object type "Compound Ceiling:KRAFT_61mm_Gips_ himling" | CEILING | names: "Compound Ceiling:KRAFT_61mm_Gips_ himling:8884599", "Compound Ceiling:KRAFT_61mm_Gips_ himling:8885090", "Compound Ceiling:KRAFT_61mm_Gips_ himling:8885304" (+18 more) | material: layers "Compound Ceiling:KRAFT_61mm_Gips_ himling" ("A-Air" 48., "Gyproc Gipsplade_2560mm" 13.) | property sets: Pset_CoveringCommon, PSet_Revit_Constraints, PSet_Revit_Identity Data, PSet_Revit_Dimensions, PSet_Revit_Phasing, PSet_Revit_Type_Construction
          2 x IFCWALLSTANDARDCASE | object type "Basic Wall:242.11_Type_4.3_Gipsvæg_124mm_påforing elevator:7479952" | names: "Basic Wall:242.11_Type_4.3_Gipsvæg_124mm_påforing elevator:9030318", "Basic Wall:242.11_Type_4.3_Gipsvæg_124mm_påforing elevator:9030319" | material: layers "Basic Wall:242.11_Type_4.3_Gipsvæg_124mm_påforing elevator" ("Aart_Gips" 26., "Wood" 98.) | property sets: PSet_Revit_Structural, PSet_Revit_Constraints, PSet_Revit_Identity Data, PSet_Revit_Phasing, PSet_Revit_Dimensions, Pset_WallCommon
          1 x IFCWALL | object type "Basic Wall:242.3_Type_2.1_Gipsvæg_147mm_Indv. vegge_Bad:7797675" | names: "Basic Wall:242.3_Type_2.1_Gipsvæg_147mm_Indv. vegge_Bad:9036308" | material: layers "Basic Wall:242.3_Type_2.1_Gipsvæg_147mm_Indv. vegge_Bad" ("Aart_Gips" 13., "A-Wood" 98., "Aart_Gips" 26., "Aart_Flise" 10.) | property sets: PSet_Revit_Structural, PSet_Revit_Constraints, PSet_Revit_Identity Data, PSet_Revit_Phasing, PSet_Revit_Dimensions, Pset_WallCommon
          1 x IFCWALL | object type "Basic Wall:242.13_Type_2.2_Gipsvæg_197mm_Påforing Bad:7797614" | names: "Basic Wall:242.13_Type_2.2_Gipsvæg_197mm_Påforing Bad:9093891" | material: layers "Basic Wall:242.13_Type_2.2_Gipsvæg_197mm_Påforing Bad" ("Aart_Flise" 10., "Aart_Gips" 26., "Wood" 148., "Aart_Gips" 13.) | property sets: PSet_Revit_Structural, PSet_Revit_Constraints, PSet_Revit_Identity Data, PSet_Revit_Phasing, PSet_Revit_Dimensions, Pset_WallCommon
          2 x IFCWALLSTANDARDCASE | object type "Basic Wall:242.8_Type_3.3_Gipsvæg_134mm_Sjakt:7797367" | names: "Basic Wall:242.8_Type_3.3_Gipsvæg_134mm_Sjakt:9093892", "Basic Wall:242.8_Type_3.3_Gipsvæg_134mm_Sjakt:9093893" | material: layers "Basic Wall:242.8_Type_3.3_Gipsvæg_134mm_Sjakt" ("Aart_Flise" 10., "Aart_Gips" 26., "A-Wood" 98.) | property sets: PSet_Revit_Structural, PSet_Revit_Constraints, PSet_Revit_Identity Data, PSet_Revit_Phasing, PSet_Revit_Dimensions, Pset_WallCommon
          3 x IFCWALLSTANDARDCASE | object type "Basic Wall:242.12_Type_3.4_Gipsvæg_184mm_Påforing Bad_Sjakt:8098014" | names: "Basic Wall:242.12_Type_3.4_Gipsvæg_184mm_Påforing Bad_Sjakt:9094012", "Basic Wall:242.12_Type_3.4_Gipsvæg_184mm_Påforing Bad_Sjakt:9094013", "Basic Wall:242.12_Type_3.4_Gipsvæg_184mm_Påforing Bad_Sjakt:22289479" | material: layers "Basic Wall:242.12_Type_3.4_Gipsvæg_184mm_Påforing Bad_Sjakt" ("Aart_Flise" 10., "Aart_Gips" 26., "Wood" 148.) | property sets: PSet_Revit_Structural, PSet_Revit_Constraints, PSet_Revit_Identity Data, PSet_Revit_Phasing, PSet_Revit_Dimensions, Pset_WallCommon
          5 x IFCWALLSTANDARDCASE | object type "Basic Wall:242.17_Fliser_10mm:7816687" | names: "Basic Wall:242.17_Fliser_10mm:9122260", "Basic Wall:242.17_Fliser_10mm:9173160", "Basic Wall:242.17_Fliser_10mm:9173213" (+2 more) | material: layers "Basic Wall:242.17_Fliser_10mm" ("Aart_Flise" 10.) | property sets: PSet_Revit_Structural, PSet_Revit_Constraints, PSet_Revit_Identity Data, PSet_Revit_Phasing, PSet_Revit_Dimensions, Pset_WallCommon
          7 x IFCSLAB | object type "Floor:Etasjedekk_168mm_betong_Bad" | FLOOR | names: "Floor:Etasjedekk_168mm_betong_Bad:9182154", "Floor:Etasjedekk_168mm_betong_Bad:9182154:2", "Floor:Etasjedekk_168mm_betong_Bad:9182154:3" (+4 more) | material: layers "Floor:Etasjedekk_168mm_betong_Bad" ("Aart_beton" 168.) | property sets: PSet_Revit_Constraints, PSet_Revit_Structural, PSet_Revit_Identity Data, PSet_Revit_Phasing, PSet_Revit_Dimensions, Pset_SlabCommon
          10 x IFCSLAB | object type "Floor:Gulvopbygning_112mm_Bad" | FLOOR | names: "Floor:Gulvopbygning_112mm_Bad:9182747", "Floor:Gulvopbygning_112mm_Bad:9182747:2", "Floor:Gulvopbygning_112mm_Bad:9182747:3" (+7 more) | material: layers "Floor:Gulvopbygning_112mm_Bad" ("Stone (2)" 12., "A-Conc" 100.) | property sets: PSet_Revit_Constraints, PSet_Revit_Structural, PSet_Revit_Identity Data, PSet_Revit_Phasing, PSet_Revit_Dimensions, Pset_SlabCommon
          1 x IFCWINDOW | type IFCWINDOWSTYLE "Skyveparti_2088x2288mm" | object type "Skyveparti_2088x2288mm" | names: "234.2_V_Udv._skyveparti_3fag Nytt:Skyveparti_2088x2288mm:Skyveparti_2088x2288mm:10991077" | property sets: Pset_WindowCommon, PSet_Revit_Other, PSet_Revit_Dimensions, PSet_Revit_Constraints, PSet_Revit_Identity Data, PSet_Revit_Phasing
          4 x IFCRAILING | object type "Railing:rekkverk_vinduer_type1_(1000mm)" | names: "Railing:rekkverk_vinduer_type1_(1000mm):11768746", "Railing:rekkverk_vinduer_type1_(1000mm):11768843", "Railing:rekkverk_vinduer_type1_(1000mm):11768933" (+1 more) | material: "Wood - Timber" | property sets: Pset_RailingCommon, PSet_Revit_Dimensions, PSet_Revit_Constraints, PSet_Revit_Identity Data, PSet_Revit_Phasing, PSet_Revit_Type_Construction
          1 x IFCWINDOW | type IFCWINDOWSTYLE "2388x1488 mm" | object type "2388x1488 mm" | names: "234.4_V_Udv._vindu_2fag Nytt:2388x1488 mm:2388x1488 mm:14707764" | property sets: Pset_WindowCommon, PSet_Revit_Other, PSet_Revit_Dimensions, PSet_Revit_Graphics, PSet_Revit_Constraints, PSet_Revit_Identity Data
          1 x IFCWINDOW | type IFCWINDOWSTYLE "Skyveparti_2388x2288mm" | object type "Skyveparti_2388x2288mm" | names: "234.2_H_Udv._skyveparti_3fag Nytt:Skyveparti_2388x2288mm:Skyveparti_2388x2288mm:17530858" | property sets: Pset_WindowCommon, PSet_Revit_Other, PSet_Revit_Dimensions, PSet_Revit_Constraints, PSet_Revit_Identity Data, PSet_Revit_Phasing
          2 x IFCWALLSTANDARDCASE | object type "Basic Wall:242.20_Type_5.1_Eikespiler_36mm_Indv. hagestue:19455957" | names: "Basic Wall:242.20_Type_5.1_Eikespiler_36mm_Indv. hagestue:19553539", "Basic Wall:242.20_Type_5.1_Eikespiler_36mm_Indv. hagestue:19553642" | material: layers "Basic Wall:242.20_Type_5.1_Eikespiler_36mm_Indv. hagestue" ("Wood - Eikespiler" 36.) | property sets: PSet_Revit_Structural, PSet_Revit_Constraints, PSet_Revit_Identity Data, PSet_Revit_Phasing, PSet_Revit_Dimensions, Pset_WallCommon
          2 x IFCDOOR | type IFCDOORSTYLE "M11x21" | object type "M11x21" | names: "DAN_Indv. Skydedør i væg:M11x21:M11x21:19562308", "DAN_Indv. Skydedør i væg:M11x21:M11x21:19562539" | property sets: Pset_DoorCommon, PSet_Revit_Other, PSet_Revit_Materials and Finishes, PSet_Revit_Constraints, PSet_Revit_Identity Data, PSet_Revit_Phasing
          3 x IFCWINDOW | type IFCWINDOWSTYLE "1188 x 1488mm" | object type "1188 x 1488mm" | names: "234.3_V_Udv._vindu_1fag_PAR:1188 x 1488mm:1188 x 1488mm:20288201", "234.3_V_Udv._vindu_1fag_PAR:1188 x 1488mm:1188 x 1488mm:21187691", "234.3_V_Udv._vindu_1fag_PAR:1188 x 1488mm:1188 x 1488mm:21188061" | property sets: Pset_WindowCommon, PSet_Revit_Other, PSet_Revit_Constraints, PSet_Revit_Visibility, PSet_Revit_Identity Data, PSet_Revit_General
          1 x IFCWALLSTANDARDCASE | object type "Basic Wall:Aart_Gips_13mm:7855032" | names: "Basic Wall:Aart_Gips_13mm:20804587" | material: layers "Basic Wall:Aart_Gips_13mm" ("Aart_Gips" 13.) | property sets: PSet_Revit_Structural, PSet_Revit_Constraints, PSet_Revit_Identity Data, PSet_Revit_Phasing, PSet_Revit_Dimensions, Pset_WallCommon
          1 x IFCWINDOW | type IFCWINDOWSTYLE "2988x2288mm" | object type "2988x2288mm" | names: "234.7_V_Udv._vindu_høyt_3fag_PAR:2988x2288mm:2988x2288mm:21170260" | property sets: Pset_WindowCommon, PSet_Revit_Other, PSet_Revit_Constraints, PSet_Revit_Visibility, PSet_Revit_Identity Data, PSet_Revit_General
          1 x IFCWINDOW | type IFCWINDOWSTYLE "1188 x 1488mm" | object type "1188 x 1488mm" | names: "234.3_H_Udv._vindu_1fag_PAR:1188 x 1488mm:1188 x 1488mm:21173899" | property sets: Pset_WindowCommon, PSet_Revit_Other, PSet_Revit_Constraints, PSet_Revit_Visibility, PSet_Revit_Identity Data, PSet_Revit_General
          1 x IFCWINDOW | type IFCWINDOWSTYLE "2988x2288mm" | object type "2988x2288mm" | names: "234.7_H_Udv._vindu_høyt_3fag_PAR:2988x2288mm:2988x2288mm:21182769" | property sets: Pset_WindowCommon, PSet_Revit_Other, PSet_Revit_Constraints, PSet_Revit_Visibility, PSet_Revit_Identity Data, PSet_Revit_General
          1 x IFCWINDOW | type IFCWINDOWSTYLE "Skyveparti_2688x2288mm" | object type "Skyveparti_2688x2288mm" | names: "234.2_H_Udv._skyveparti_3fag Nytt:Skyveparti_2688x2288mm:Skyveparti_2688x2288mm:21189387" | property sets: Pset_WindowCommon, PSet_Revit_Other, PSet_Revit_Dimensions, PSet_Revit_Constraints, PSet_Revit_Identity Data, PSet_Revit_Phasing
          25 x IFCBUILDINGELEMENTPROXY | object type "Lodret" | names: "Beklædning - Drypkant - Vandbord, overkant:Lodret:Lodret:21513143", "Beklædning - Drypkant - Vandbord, overkant:Lodret:Lodret:21513280", "Beklædning - Drypkant - Vandbord, overkant:Lodret:Lodret:21513334" (+22 more) | property sets: PSet_Revit_Dimensions, PSet_Revit_Constraints, PSet_Revit_Identity Data, PSet_Revit_Phasing, PSet_Revit_Type_Dimensions, PSet_Revit_Type_General
          2 x IFCWALLSTANDARDCASE | object type "Basic Wall:242.3_Type_3.5_Gipsvæg_197mm_Indv. vegge_Bad:16140526" | names: "Basic Wall:242.3_Type_3.5_Gipsvæg_197mm_Indv. vegge_Bad:21834561", "Basic Wall:242.3_Type_3.5_Gipsvæg_197mm_Indv. vegge_Bad:21834582" | material: layers "Basic Wall:242.3_Type_3.5_Gipsvæg_197mm_Indv. vegge_Bad" ("Aart_Gips" 13., "A-Wood" 148., "Aart_Gips" 26., "Aart_Flise" 10.) | property sets: PSet_Revit_Structural, PSet_Revit_Constraints, PSet_Revit_Identity Data, PSet_Revit_Phasing, PSet_Revit_Dimensions, Pset_WallCommon
          1 x IFCWALLSTANDARDCASE | object type "Basic Wall:242.22_Type_3.7_Gipsvæg_84mm_Indv. vegge_Påforing_Badrom 48/26/10:22152513" | names: "Basic Wall:242.22_Type_3.7_Gipsvæg_84mm_Indv. vegge_Påforing_Badrom 48/26/10:21885203" | material: layers "Basic Wall:242.22_Type_3.7_Gipsvæg_84mm_Indv. vegge_Påforing_Badrom 48/26/10" ("Aart_Flise" 10., "Aart_Gips" 26., "A-Wood" 48.) | property sets: PSet_Revit_Structural, PSet_Revit_Constraints, PSet_Revit_Identity Data, PSet_Revit_Phasing, PSet_Revit_Dimensions, Pset_WallCommon
          1 x IFCCOVERING | object type "Compound Ceiling:kraft_Himling_Akustikkflåte" | CEILING | names: "Compound Ceiling:kraft_Himling_Akustikkflåte:22217734" | material: layers "Compound Ceiling:kraft_Himling_Akustikkflåte" ("Ceiling Tile 600 x 600" 40.) | property sets: Pset_CoveringCommon, PSet_Revit_Constraints, PSet_Revit_Identity Data, PSet_Revit_Dimensions, PSet_Revit_Phasing, PSet_Revit_Type_Construction
      IFCBUILDINGSTOREY "03" | elevation 5800.
        contains 218 elements
          1 x IFCSLAB | object type "Floor:Repos_200mm_betong" | FLOOR | names: "Floor:Repos_200mm_betong:1517412" | material: layers "Floor:Repos_200mm_betong" ("Aart_beton" 200.) | property sets: PSet_Revit_Constraints, PSet_Revit_Structural, PSet_Revit_Identity Data, PSet_Revit_Phasing, PSet_Revit_Dimensions, Pset_SlabCommon
          1 x IFCSTAIR | object type "Stair:Trappeopgang" | names: "Stair:Trappeopgang:1517423" | parts: 3 IFCRAILING, 1 IFCSTAIR | property sets: Pset_StairCommon, PSet_Revit_Dimensions, PSet_Revit_Constraints, PSet_Revit_Graphics, PSet_Revit_Identity Data, PSet_Revit_Phasing
          2 x IFCRAILING | object type "Railing:Rekkverk_hovedtrappe_lysning_990mm" | names: "Railing:Rekkverk_hovedtrappe_lysning_990mm:1517541", "Railing:Rekkverk_hovedtrappe_lysning_990mm:1517561" | property sets: Pset_RailingCommon, PSet_Revit_Dimensions, PSet_Revit_Constraints, PSet_Revit_Identity Data, PSet_Revit_Phasing, PSet_Revit_Type_Construction
          1 x IFCDOOR | type IFCDOORSTYLE "M10x21" | object type "M10x21" | names: "Hoveddør_Leilighet:M10x21:M10x21:1517569" | property sets: Pset_DoorCommon, PSet_Revit_Other, PSet_Revit_Constraints, PSet_Revit_Identity Data, PSet_Revit_Construction, PSet_Revit_Text
          1 x IFCDOOR | type IFCDOORSTYLE "M10x21" | object type "M10x21" | names: "Utv. dør_Leilighet:M10x21:M10x21:1689354" | property sets: Pset_DoorCommon, PSet_Revit_Other, PSet_Revit_Constraints, PSet_Revit_Identity Data, PSet_Revit_Construction, PSet_Revit_Text
          4 x IFCWINDOW | type IFCWINDOWSTYLE "1188x1488 mm" | object type "1188x1488 mm" | names: "234.3_V_Udv._vindu_1fag(nytt):1188x1488 mm:1188x1488 mm:2374111", "234.3_V_Udv._vindu_1fag(nytt):1188x1488 mm:1188x1488 mm:2374113", "234.3_V_Udv._vindu_1fag(nytt):1188x1488 mm:1188x1488 mm:2374114" (+1 more) | property sets: Pset_WindowCommon, PSet_Revit_Other, PSet_Revit_Dimensions, PSet_Revit_Graphics, PSet_Revit_Constraints, PSet_Revit_Identity Data
          1 x IFCDOOR | type IFCDOORSTYLE "M10x21" | object type "M10x21" | names: "Utv. dør_Leilighet:M10x21:M10x21:2992344" | property sets: Pset_DoorCommon, PSet_Revit_Other, PSet_Revit_Constraints, PSet_Revit_Identity Data, PSet_Revit_Construction, PSet_Revit_Text
          1 x IFCDOOR | type IFCDOORSTYLE "M10x21" | object type "M10x21" | names: "Hoveddør_Leilighet:M10x21:M10x21:3026092" | property sets: Pset_DoorCommon, PSet_Revit_Other, PSet_Revit_Constraints, PSet_Revit_Identity Data, PSet_Revit_Construction, PSet_Revit_Text
          2 x IFCWINDOW | type IFCWINDOWSTYLE "Skyveparti_2088x2288mm" | object type "Skyveparti_2088x2288mm" | names: "234.2_H_Udv._skyveparti_3fag Nytt:Skyveparti_2088x2288mm:Skyveparti_2088x2288mm:3508597", "234.2_H_Udv._skyveparti_3fag Nytt:Skyveparti_2088x2288mm:Skyveparti_2088x2288mm:10991079" | property sets: Pset_WindowCommon, PSet_Revit_Other, PSet_Revit_Dimensions, PSet_Revit_Constraints, PSet_Revit_Identity Data, PSet_Revit_Phasing
          36 x IFCWALLSTANDARDCASE | object type "Basic Wall:242.1_Type_1.1_Gipsvæg_124mm_Indv. vegge:7478708" | names: "Basic Wall:242.1_Type_1.1_Gipsvæg_124mm_Indv. vegge:3560839", "Basic Wall:242.1_Type_1.1_Gipsvæg_124mm_Indv. vegge:3561595", "Basic Wall:242.1_Type_1.1_Gipsvæg_124mm_Indv. vegge:3918022" (+33 more) | material: layers "Basic Wall:242.1_Type_1.1_Gipsvæg_124mm_Indv. vegge" ("Aart_Gips" 13., "A-Wood" 98., "Aart_Gips" 13.) | property sets: PSet_Revit_Structural, PSet_Revit_Constraints, PSet_Revit_Identity Data, PSet_Revit_Phasing, PSet_Revit_Dimensions, Pset_WallCommon
          20 x IFCCOVERING | object type "Compound Ceiling:KRAFT_61mm_Gips_ himling" | CEILING | names: "Compound Ceiling:KRAFT_61mm_Gips_ himling:8884700", "Compound Ceiling:KRAFT_61mm_Gips_ himling:8885148", "Compound Ceiling:KRAFT_61mm_Gips_ himling:8885476" (+17 more) | material: layers "Compound Ceiling:KRAFT_61mm_Gips_ himling" ("A-Air" 48., "Gyproc Gipsplade_2560mm" 13.) | property sets: Pset_CoveringCommon, PSet_Revit_Constraints, PSet_Revit_Identity Data, PSet_Revit_Dimensions, PSet_Revit_Phasing, PSet_Revit_Type_Construction
          27 x IFCWALLSTANDARDCASE | object type "Basic Wall:242.7_Type_3.1_Gipsvæg_111mm_Sjakt:17953268" | names: "Basic Wall:242.7_Type_3.1_Gipsvæg_111mm_Sjakt:9093868", "Basic Wall:242.7_Type_3.1_Gipsvæg_111mm_Sjakt:9093870", "Basic Wall:242.7_Type_3.1_Gipsvæg_111mm_Sjakt:9093890" (+24 more) | material: layers "Basic Wall:242.7_Type_3.1_Gipsvæg_111mm_Sjakt" ("Aart_Gips" 13., "A-Wood" 98.) | property sets: PSet_Revit_Structural, PSet_Revit_Constraints, PSet_Revit_Identity Data, PSet_Revit_Phasing, PSet_Revit_Dimensions, Pset_WallCommon
          11 x IFCWALLSTANDARDCASE | object type "Basic Wall:242.3_Type_2.1_Gipsvæg_147mm_Indv. vegge_Bad:7797675" | names: "Basic Wall:242.3_Type_2.1_Gipsvæg_147mm_Indv. vegge_Bad:9093869", "Basic Wall:242.3_Type_2.1_Gipsvæg_147mm_Indv. vegge_Bad:9093873", "Basic Wall:242.3_Type_2.1_Gipsvæg_147mm_Indv. vegge_Bad:9093944" (+8 more) | material: layers "Basic Wall:242.3_Type_2.1_Gipsvæg_147mm_Indv. vegge_Bad" ("Aart_Gips" 13., "A-Wood" 98., "Aart_Gips" 26., "Aart_Flise" 10.) | property sets: PSet_Revit_Structural, PSet_Revit_Constraints, PSet_Revit_Identity Data, PSet_Revit_Phasing, PSet_Revit_Dimensions, Pset_WallCommon
          2 x IFCCURTAINWALL | object type "Curtain Wall:243.1_Indv_glasskillevæg:1131477" | names: "Curtain Wall:243.1_Indv_glasskillevæg:9093917", "Curtain Wall:243.1_Indv_glasskillevæg:9093945" | parts: 2 IFCPLATE | property sets: Pset_CurtainWallCommon, PSet_Revit_Structural, PSet_Revit_Constraints, PSet_Revit_Identity Data, PSet_Revit_Phasing, PSet_Revit_Dimensions
          7 x IFCDOOR | type IFCDOORSTYLE "M9x21" | object type "M9x21" | names: "Int_door_Aart:M9x21:M9x21:9093923", "Int_door_Aart:M9x21:M9x21:9093924", "Int_door_Aart:M9x21:M9x21:9093928" (+4 more) | property sets: Pset_DoorCommon, PSet_Revit_Other, PSet_Revit_Dimensions, PSet_Revit_Constraints, PSet_Revit_Identity Data, PSet_Revit_Phasing
          6 x IFCDOOR | type IFCDOORSTYLE "M9x21" | object type "M9x21" | names: "Int_door_Aart:M9x21:M9x21:9093925", "Int_door_Aart:M9x21:M9x21:9093927", "Int_door_Aart:M9x21:M9x21:9093930" (+3 more) | property sets: Pset_DoorCommon, PSet_Revit_Other, PSet_Revit_Dimensions, PSet_Revit_Constraints, PSet_Revit_Identity Data, PSet_Revit_Phasing
          3 x IFCDOOR | type IFCDOORSTYLE "M9x21" | object type "M9x21" | names: "Int_door_Aart:M9x21:M9x21:9093926", "Int_door_Aart:M9x21:M9x21:9093929", "Int_door_Aart:M9x21:M9x21:9093984" | property sets: Pset_DoorCommon, PSet_Revit_Other, PSet_Revit_Dimensions, PSet_Revit_Constraints, PSet_Revit_Identity Data, PSet_Revit_Phasing
          1 x IFCDOOR | type IFCDOORSTYLE "M9x21" | object type "M9x21" | names: "DAN_Indv. Skydedør i væg:M9x21:M9x21:9093941" | property sets: Pset_DoorCommon, PSet_Revit_Other, PSet_Revit_Materials and Finishes, PSet_Revit_Constraints, PSet_Revit_Identity Data, PSet_Revit_Phasing
          1 x IFCDOOR | type IFCDOORSTYLE "M9x21" | object type "M9x21" | names: "DAN_Indv. Skydedør i væg:M9x21:M9x21:9093948" | property sets: Pset_DoorCommon, PSet_Revit_Other, PSet_Revit_Materials and Finishes, PSet_Revit_Constraints, PSet_Revit_Identity Data, PSet_Revit_Phasing
          2 x IFCDOOR | type IFCDOORSTYLE "M9x21" | object type "M9x21" | names: "Int_door_Aart:M9x21:M9x21:9093960", "Int_door_Aart:M9x21:M9x21:9094040" | property sets: Pset_DoorCommon, PSet_Revit_Other, PSet_Revit_Dimensions, PSet_Revit_Constraints, PSet_Revit_Identity Data, PSet_Revit_Phasing
          5 x IFCWALLSTANDARDCASE | object type "Basic Wall:242.13_Type_2.2_Gipsvæg_197mm_Påforing Bad:7797614" | names: "Basic Wall:242.13_Type_2.2_Gipsvæg_197mm_Påforing Bad:9093961", "Basic Wall:242.13_Type_2.2_Gipsvæg_197mm_Påforing Bad:9093985", "Basic Wall:242.13_Type_2.2_Gipsvæg_197mm_Påforing Bad:9094017" (+2 more) | material: layers "Basic Wall:242.13_Type_2.2_Gipsvæg_197mm_Påforing Bad" ("Aart_Flise" 10., "Aart_Gips" 26., "Wood" 148., "Aart_Gips" 13.) | property sets: PSet_Revit_Structural, PSet_Revit_Constraints, PSet_Revit_Identity Data, PSet_Revit_Phasing, PSet_Revit_Dimensions, Pset_WallCommon
          2 x IFCWALLSTANDARDCASE | object type "Basic Wall:242.11_Type_4.3_Gipsvæg_124mm_påforing elevator:7479952" | names: "Basic Wall:242.11_Type_4.3_Gipsvæg_124mm_påforing elevator:9094005", "Basic Wall:242.11_Type_4.3_Gipsvæg_124mm_påforing elevator:9094006" | material: layers "Basic Wall:242.11_Type_4.3_Gipsvæg_124mm_påforing elevator" ("Aart_Gips" 26., "Wood" 98.) | property sets: PSet_Revit_Structural, PSet_Revit_Constraints, PSet_Revit_Identity Data, PSet_Revit_Phasing, PSet_Revit_Dimensions, Pset_WallCommon
          1 x IFCWALL | object type "Basic Wall:242.3_Type_2.1_Gipsvæg_147mm_Indv. vegge_Bad:7797675" | names: "Basic Wall:242.3_Type_2.1_Gipsvæg_147mm_Indv. vegge_Bad:9094019" | material: layers "Basic Wall:242.3_Type_2.1_Gipsvæg_147mm_Indv. vegge_Bad" ("Aart_Gips" 13., "A-Wood" 98., "Aart_Gips" 26., "Aart_Flise" 10.) | property sets: PSet_Revit_Structural, PSet_Revit_Constraints, PSet_Revit_Identity Data, PSet_Revit_Phasing, PSet_Revit_Dimensions, Pset_WallCommon
          2 x IFCWALLSTANDARDCASE | object type "Basic Wall:242.22_Type_3.7_Gipsvæg_84mm_Indv. vegge_Påforing_Badrom 48/26/10:22152513" | names: "Basic Wall:242.22_Type_3.7_Gipsvæg_84mm_Indv. vegge_Påforing_Badrom 48/26/10:9126855", "Basic Wall:242.22_Type_3.7_Gipsvæg_84mm_Indv. vegge_Påforing_Badrom 48/26/10:22161653" | material: layers "Basic Wall:242.22_Type_3.7_Gipsvæg_84mm_Indv. vegge_Påforing_Badrom 48/26/10" ("Aart_Flise" 10., "Aart_Gips" 26., "A-Wood" 48.) | property sets: PSet_Revit_Structural, PSet_Revit_Constraints, PSet_Revit_Identity Data, PSet_Revit_Phasing, PSet_Revit_Dimensions, Pset_WallCommon
          6 x IFCWALLSTANDARDCASE | object type "Basic Wall:242.17_Fliser_10mm:7816687" | names: "Basic Wall:242.17_Fliser_10mm:9126947", "Basic Wall:242.17_Fliser_10mm:9174175", "Basic Wall:242.17_Fliser_10mm:9174176" (+3 more) | material: layers "Basic Wall:242.17_Fliser_10mm" ("Aart_Flise" 10.) | property sets: PSet_Revit_Structural, PSet_Revit_Constraints, PSet_Revit_Identity Data, PSet_Revit_Phasing, PSet_Revit_Dimensions, Pset_WallCommon
          4 x IFCRAILING | object type "Railing:rekkverk_vinduer_type1_(1000mm)" | names: "Railing:rekkverk_vinduer_type1_(1000mm):11769111", "Railing:rekkverk_vinduer_type1_(1000mm):11769186", "Railing:rekkverk_vinduer_type1_(1000mm):11769269" (+1 more) | material: "Wood - Timber" | property sets: Pset_RailingCommon, PSet_Revit_Dimensions, PSet_Revit_Constraints, PSet_Revit_Identity Data, PSet_Revit_Phasing, PSet_Revit_Type_Construction
          2 x IFCWALLSTANDARDCASE | object type "Basic Wall:242.8_Type_3.3_Gipsvæg_134mm_Sjakt:7797367" | names: "Basic Wall:242.8_Type_3.3_Gipsvæg_134mm_Sjakt:14644272", "Basic Wall:242.8_Type_3.3_Gipsvæg_134mm_Sjakt:14644276" | material: layers "Basic Wall:242.8_Type_3.3_Gipsvæg_134mm_Sjakt" ("Aart_Flise" 10., "Aart_Gips" 26., "A-Wood" 98.) | property sets: PSet_Revit_Structural, PSet_Revit_Constraints, PSet_Revit_Identity Data, PSet_Revit_Phasing, PSet_Revit_Dimensions, Pset_WallCommon
          3 x IFCWALLSTANDARDCASE | object type "Basic Wall:242.12_Type_3.4_Gipsvæg_184mm_Påforing Bad_Sjakt:8098014" | names: "Basic Wall:242.12_Type_3.4_Gipsvæg_184mm_Påforing Bad_Sjakt:14644398", "Basic Wall:242.12_Type_3.4_Gipsvæg_184mm_Påforing Bad_Sjakt:14644399", "Basic Wall:242.12_Type_3.4_Gipsvæg_184mm_Påforing Bad_Sjakt:22290437" | material: layers "Basic Wall:242.12_Type_3.4_Gipsvæg_184mm_Påforing Bad_Sjakt" ("Aart_Flise" 10., "Aart_Gips" 26., "Wood" 148.) | property sets: PSet_Revit_Structural, PSet_Revit_Constraints, PSet_Revit_Identity Data, PSet_Revit_Phasing, PSet_Revit_Dimensions, Pset_WallCommon
          1 x IFCBUILDINGELEMENTPROXY | object type "påforing_3460x270mm" | names: "påforing_3460x270mm15:påforing_3460x270mm:påforing_3460x270mm:14756848" | property sets: PSet_Revit_Constraints, PSet_Revit_Identity Data, PSet_Revit_Phasing, PSet_Revit_Type_Identity Data
          1 x IFCSLAB | object type "Floor:Etasjedekk_250mm_betong" | FLOOR | names: "Floor:Etasjedekk_250mm_betong:15746622" | material: layers "Floor:Etasjedekk_250mm_betong" ("Aart_beton" 250.) | property sets: PSet_Revit_Constraints, PSet_Revit_Structural, PSet_Revit_Identity Data, PSet_Revit_Phasing, PSet_Revit_Dimensions, Pset_SlabCommon
          10 x IFCSLAB | object type "Floor:Gulvopbygning_112mm_Bad" | FLOOR | names: "Floor:Gulvopbygning_112mm_Bad:15746691", "Floor:Gulvopbygning_112mm_Bad:15746691:2", "Floor:Gulvopbygning_112mm_Bad:15746691:3" (+7 more) | material: layers "Floor:Gulvopbygning_112mm_Bad" ("Stone (2)" 12., "A-Conc" 100.) | property sets: PSet_Revit_Constraints, PSet_Revit_Structural, PSet_Revit_Identity Data, PSet_Revit_Phasing, PSet_Revit_Dimensions, Pset_SlabCommon
          7 x IFCSLAB | object type "Floor:Etasjedekk_168mm_betong_Bad" | FLOOR | names: "Floor:Etasjedekk_168mm_betong_Bad:15746906", "Floor:Etasjedekk_168mm_betong_Bad:15746906:2", "Floor:Etasjedekk_168mm_betong_Bad:15746906:3" (+4 more) | material: layers "Floor:Etasjedekk_168mm_betong_Bad" ("Aart_beton" 168.) | property sets: PSet_Revit_Constraints, PSet_Revit_Structural, PSet_Revit_Identity Data, PSet_Revit_Phasing, PSet_Revit_Dimensions, Pset_SlabCommon
          4 x IFCSLAB | object type "Floor:Gulvopbygning_30mm" | FLOOR | names: "Floor:Gulvopbygning_30mm:15747002", "Floor:Gulvopbygning_30mm:15747002:2", "Floor:Gulvopbygning_30mm:15747002:3" (+1 more) | material: layers "Floor:Gulvopbygning_30mm" ("Wood - Flooring" 14., "Aart_Gips" 16.) | property sets: PSet_Revit_Constraints, PSet_Revit_Structural, PSet_Revit_Identity Data, PSet_Revit_Phasing, PSet_Revit_Dimensions, Pset_SlabCommon
          1 x IFCWINDOW | type IFCWINDOWSTYLE "Skyveparti_2388x2288mm" | object type "Skyveparti_2388x2288mm" | names: "234.2_V_Udv._skyveparti_3fag Nytt:Skyveparti_2388x2288mm:Skyveparti_2388x2288mm:17533459" | property sets: Pset_WindowCommon, PSet_Revit_Other, PSet_Revit_Dimensions, PSet_Revit_Constraints, PSet_Revit_Identity Data, PSet_Revit_Phasing
          1 x IFCWINDOW | type IFCWINDOWSTYLE "Skyveparti_2688x2288mm" | object type "Skyveparti_2688x2288mm" | names: "234.2_H_Udv._skyveparti_3fag Nytt:Skyveparti_2688x2288mm:Skyveparti_2688x2288mm:17533462" | property sets: Pset_WindowCommon, PSet_Revit_Other, PSet_Revit_Dimensions, PSet_Revit_Constraints, PSet_Revit_Identity Data, PSet_Revit_Phasing
          1 x IFCWALLSTANDARDCASE | object type "Basic Wall:242.20_Type_5.1_Eikespiler_36mm_Indv. hagestue:19455957" | names: "Basic Wall:242.20_Type_5.1_Eikespiler_36mm_Indv. hagestue:19553928" | material: layers "Basic Wall:242.20_Type_5.1_Eikespiler_36mm_Indv. hagestue" ("Wood - Eikespiler" 36.) | property sets: PSet_Revit_Structural, PSet_Revit_Constraints, PSet_Revit_Identity Data, PSet_Revit_Phasing, PSet_Revit_Dimensions, Pset_WallCommon
          1 x IFCDOOR | type IFCDOORSTYLE "M11x21" | object type "M11x21" | names: "DAN_Indv. Skydedør i væg:M11x21:M11x21:19562837" | property sets: Pset_DoorCommon, PSet_Revit_Other, PSet_Revit_Materials and Finishes, PSet_Revit_Constraints, PSet_Revit_Identity Data, PSet_Revit_Phasing
          1 x IFCDOOR | type IFCDOORSTYLE "M11x21" | object type "M11x21" | names: "DAN_Indv. Skydedør i væg:M11x21:M11x21:19562932" | property sets: Pset_DoorCommon, PSet_Revit_Other, PSet_Revit_Materials and Finishes, PSet_Revit_Constraints, PSet_Revit_Identity Data, PSet_Revit_Phasing
          3 x IFCWINDOW | type IFCWINDOWSTYLE "1188 x 1488mm" | object type "1188 x 1488mm" | names: "234.3_V_Udv._vindu_1fag_PAR:1188 x 1488mm:1188 x 1488mm:20288178", "234.3_V_Udv._vindu_1fag_PAR:1188 x 1488mm:1188 x 1488mm:21187704", "234.3_V_Udv._vindu_1fag_PAR:1188 x 1488mm:1188 x 1488mm:21188074" | property sets: Pset_WindowCommon, PSet_Revit_Other, PSet_Revit_Constraints, PSet_Revit_Visibility, PSet_Revit_Identity Data, PSet_Revit_General
          1 x IFCWINDOW | type IFCWINDOWSTYLE "1188 x 1488mm" | object type "1188 x 1488mm" | names: "234.3_H_Udv._vindu_1fag_PAR:1188 x 1488mm:1188 x 1488mm:21174129" | property sets: Pset_WindowCommon, PSet_Revit_Other, PSet_Revit_Constraints, PSet_Revit_Visibility, PSet_Revit_Identity Data, PSet_Revit_General
          2 x IFCWINDOW | type IFCWINDOWSTYLE "2988x2288mm" | object type "2988x2288mm" | names: "234.7_V_Udv._vindu_høyt_3fag_PAR:2988x2288mm:2988x2288mm:21182210", "234.7_V_Udv._vindu_høyt_3fag_PAR:2988x2288mm:2988x2288mm:21182794" | property sets: Pset_WindowCommon, PSet_Revit_Other, PSet_Revit_Constraints, PSet_Revit_Visibility, PSet_Revit_Identity Data, PSet_Revit_General
          29 x IFCBUILDINGELEMENTPROXY | object type "Lodret" | names: "Beklædning - Drypkant - Vandbord, underkant:Lodret:Lodret:21512108", "Beklædning - Drypkant - Vandbord, overkant:Lodret:Lodret:21512785", "Beklædning - Drypkant - Vandbord, overkant:Lodret:Lodret:21512964" (+26 more) | property sets: PSet_Revit_Dimensions, PSet_Revit_Constraints, PSet_Revit_Identity Data, PSet_Revit_Phasing, PSet_Revit_Type_Dimensions, PSet_Revit_Type_General
      IFCBUILDINGSTOREY "04" | elevation 8700.
        contains 170 elements
          1 x IFCSLAB | object type "Floor:Repos_200mm_betong" | FLOOR | names: "Floor:Repos_200mm_betong:1517472" | material: layers "Floor:Repos_200mm_betong" ("Aart_beton" 200.) | property sets: PSet_Revit_Constraints, PSet_Revit_Structural, PSet_Revit_Identity Data, PSet_Revit_Phasing, PSet_Revit_Dimensions, Pset_SlabCommon
          1 x IFCRAILING | object type "Railing:Rekkverk_hovedtrappe_lysning_990mm" | names: "Railing:Rekkverk_hovedtrappe_lysning_990mm:1517551" | property sets: Pset_RailingCommon, PSet_Revit_Dimensions, PSet_Revit_Constraints, PSet_Revit_Identity Data, PSet_Revit_Phasing, PSet_Revit_Type_Construction
          1 x IFCRAILING | object type "Railing:Rekkverk_hovedtrappe_repos_1000mm" | names: "Railing:Rekkverk_hovedtrappe_repos_1000mm:1517566" | property sets: Pset_RailingCommon, PSet_Revit_Dimensions, PSet_Revit_Constraints, PSet_Revit_Identity Data, PSet_Revit_Phasing, PSet_Revit_Type_Construction
          1 x IFCDOOR | type IFCDOORSTYLE "M10x21" | object type "M10x21" | names: "Hoveddør_Leilighet:M10x21:M10x21:1517575" | property sets: Pset_DoorCommon, PSet_Revit_Other, PSet_Revit_Constraints, PSet_Revit_Identity Data, PSet_Revit_Construction, PSet_Revit_Text
          2 x IFCWINDOW | type IFCWINDOWSTYLE "1188x1488 mm" | object type "1188x1488 mm" | names: "234.3_V_Udv._vindu_1fag(nytt):1188x1488 mm:1188x1488 mm:2380102", "234.3_V_Udv._vindu_1fag(nytt):1188x1488 mm:1188x1488 mm:2456878" | property sets: Pset_WindowCommon, PSet_Revit_Other, PSet_Revit_Dimensions, PSet_Revit_Graphics, PSet_Revit_Constraints, PSet_Revit_Identity Data
          2 x IFCWALLSTANDARDCASE | object type "Basic Wall:242.8_Type_3.3_Gipsvæg_134mm_Sjakt:7797367" | names: "Basic Wall:242.8_Type_3.3_Gipsvæg_134mm_Sjakt:3629177", "Basic Wall:242.8_Type_3.3_Gipsvæg_134mm_Sjakt:4664683" | material: layers "Basic Wall:242.8_Type_3.3_Gipsvæg_134mm_Sjakt" ("Aart_Flise" 10., "Aart_Gips" 26., "A-Wood" 98.) | property sets: PSet_Revit_Structural, PSet_Revit_Constraints, PSet_Revit_Identity Data, PSet_Revit_Phasing, PSet_Revit_Dimensions, Pset_WallCommon
          1 x IFCDOOR | type IFCDOORSTYLE "M10x21" | object type "M10x21" | names: "Utv. dør_Leilighet:M10x21:M10x21:3669819" | property sets: Pset_DoorCommon, PSet_Revit_Other, PSet_Revit_Constraints, PSet_Revit_Identity Data, PSet_Revit_Construction, PSet_Revit_Text
          1 x IFCDOOR | type IFCDOORSTYLE "M10x21" | object type "M10x21" | names: "Utv. dør_Leilighet:M10x21:M10x21:3669820" | property sets: Pset_DoorCommon, PSet_Revit_Other, PSet_Revit_Constraints, PSet_Revit_Identity Data, PSet_Revit_Construction, PSet_Revit_Text
          1 x IFCSTAIR | object type "Stair:Hemsetrappe" | names: "Stair:Hemsetrappe:3715767" | parts: 1 IFCSTAIR | property sets: Pset_StairCommon, PSet_Revit_Dimensions, PSet_Revit_Constraints, PSet_Revit_Graphics, PSet_Revit_Identity Data, PSet_Revit_Phasing
          1 x IFCWINDOW | type IFCWINDOWSTYLE "Skyveparti_2688x2288mm" | object type "Skyveparti_2688x2288mm" | names: "234.2_V_Udv._skyveparti_3fag Nytt:Skyveparti_2688x2288mm:Skyveparti_2688x2288mm:4731875" | property sets: Pset_WindowCommon, PSet_Revit_Other, PSet_Revit_Dimensions, PSet_Revit_Constraints, PSet_Revit_Identity Data, PSet_Revit_General
          1 x IFCDOOR | type IFCDOORSTYLE "M10x21" | object type "M10x21" | names: "Hoveddør_Leilighet:M10x21:M10x21:6018773" | property sets: Pset_DoorCommon, PSet_Revit_Other, PSet_Revit_Constraints, PSet_Revit_Identity Data, PSet_Revit_Construction, PSet_Revit_Text
          18 x IFCCOVERING | object type "Compound Ceiling:KRAFT_61mm_Gips_ himling" | CEILING | names: "Compound Ceiling:KRAFT_61mm_Gips_ himling:8884801", "Compound Ceiling:KRAFT_61mm_Gips_ himling:8885206", "Compound Ceiling:KRAFT_61mm_Gips_ himling:8885656" (+15 more) | material: layers "Compound Ceiling:KRAFT_61mm_Gips_ himling" ("A-Air" 48., "Gyproc Gipsplade_2560mm" 13.) | property sets: Pset_CoveringCommon, PSet_Revit_Constraints, PSet_Revit_Identity Data, PSet_Revit_Dimensions, PSet_Revit_Phasing, PSet_Revit_Type_Construction
          2 x IFCWALLSTANDARDCASE | object type "Basic Wall:242.12_Type_3.4_Gipsvæg_184mm_Påforing Bad_Sjakt:8098014" | names: "Basic Wall:242.12_Type_3.4_Gipsvæg_184mm_Påforing Bad_Sjakt:9255105", "Basic Wall:242.12_Type_3.4_Gipsvæg_184mm_Påforing Bad_Sjakt:22293253" | material: layers "Basic Wall:242.12_Type_3.4_Gipsvæg_184mm_Påforing Bad_Sjakt" ("Aart_Flise" 10., "Aart_Gips" 26., "Wood" 148.) | property sets: PSet_Revit_Structural, PSet_Revit_Constraints, PSet_Revit_Identity Data, PSet_Revit_Phasing, PSet_Revit_Dimensions, Pset_WallCommon
          2 x IFCWINDOW | type IFCWINDOWSTYLE "Skyveparti_2088x2288mm" | object type "Skyveparti_2088x2288mm" | names: "234.2_V_Udv._skyveparti_3fag Nytt:Skyveparti_2088x2288mm:Skyveparti_2088x2288mm:10991080", "234.2_V_Udv._skyveparti_3fag Nytt:Skyveparti_2088x2288mm:Skyveparti_2088x2288mm:10991087" | property sets: Pset_WindowCommon, PSet_Revit_Other, PSet_Revit_Dimensions, PSet_Revit_Constraints, PSet_Revit_Identity Data, PSet_Revit_Phasing
          3 x IFCRAILING | object type "Railing:rekkverk_vinduer_type2_(1200mm)" | names: "Railing:rekkverk_vinduer_type2_(1200mm):11769513", "Railing:rekkverk_vinduer_type2_(1200mm):11769594", "Railing:rekkverk_vinduer_type2_(1200mm):11769719" | material: "Wood - Timber" | property sets: Pset_RailingCommon, PSet_Revit_Dimensions, PSet_Revit_Constraints, PSet_Revit_Identity Data, PSet_Revit_Phasing, PSet_Revit_Type_Construction
          23 x IFCWALLSTANDARDCASE | object type "Basic Wall:242.7_Type_3.1_Gipsvæg_111mm_Sjakt:17953268" | names: "Basic Wall:242.7_Type_3.1_Gipsvæg_111mm_Sjakt:14644251", "Basic Wall:242.7_Type_3.1_Gipsvæg_111mm_Sjakt:14644253", "Basic Wall:242.7_Type_3.1_Gipsvæg_111mm_Sjakt:14644270" (+20 more) | material: layers "Basic Wall:242.7_Type_3.1_Gipsvæg_111mm_Sjakt" ("Aart_Gips" 13., "A-Wood" 98.) | property sets: PSet_Revit_Structural, PSet_Revit_Constraints, PSet_Revit_Identity Data, PSet_Revit_Phasing, PSet_Revit_Dimensions, Pset_WallCommon
          10 x IFCWALLSTANDARDCASE | object type "Basic Wall:242.3_Type_2.1_Gipsvæg_147mm_Indv. vegge_Bad:7797675" | names: "Basic Wall:242.3_Type_2.1_Gipsvæg_147mm_Indv. vegge_Bad:14644252", "Basic Wall:242.3_Type_2.1_Gipsvæg_147mm_Indv. vegge_Bad:14644259", "Basic Wall:242.3_Type_2.1_Gipsvæg_147mm_Indv. vegge_Bad:14644336" (+7 more) | material: layers "Basic Wall:242.3_Type_2.1_Gipsvæg_147mm_Indv. vegge_Bad" ("Aart_Gips" 13., "A-Wood" 98., "Aart_Gips" 26., "Aart_Flise" 10.) | property sets: PSet_Revit_Structural, PSet_Revit_Constraints, PSet_Revit_Identity Data, PSet_Revit_Phasing, PSet_Revit_Dimensions, Pset_WallCommon
          34 x IFCWALLSTANDARDCASE | object type "Basic Wall:242.1_Type_1.1_Gipsvæg_124mm_Indv. vegge:7478708" | names: "Basic Wall:242.1_Type_1.1_Gipsvæg_124mm_Indv. vegge:14644254", "Basic Wall:242.1_Type_1.1_Gipsvæg_124mm_Indv. vegge:14644255", "Basic Wall:242.1_Type_1.1_Gipsvæg_124mm_Indv. vegge:14644256" (+31 more) | material: layers "Basic Wall:242.1_Type_1.1_Gipsvæg_124mm_Indv. vegge" ("Aart_Gips" 13., "A-Wood" 98., "Aart_Gips" 13.) | property sets: PSet_Revit_Structural, PSet_Revit_Constraints, PSet_Revit_Identity Data, PSet_Revit_Phasing, PSet_Revit_Dimensions, Pset_WallCommon
          7 x IFCDOOR | type IFCDOORSTYLE "M9x21" | object type "M9x21" | names: "Int_door_Aart:M9x21:M9x21:14644273", "Int_door_Aart:M9x21:M9x21:14644275", "Int_door_Aart:M9x21:M9x21:14644364" (+4 more) | property sets: Pset_DoorCommon, PSet_Revit_Other, PSet_Revit_Dimensions, PSet_Revit_Constraints, PSet_Revit_Identity Data, PSet_Revit_Phasing
          4 x IFCDOOR | type IFCDOORSTYLE "M9x21" | object type "M9x21" | names: "Int_door_Aart:M9x21:M9x21:14644274", "Int_door_Aart:M9x21:M9x21:14644278", "Int_door_Aart:M9x21:M9x21:14644342" (+1 more) | property sets: Pset_DoorCommon, PSet_Revit_Other, PSet_Revit_Dimensions, PSet_Revit_Constraints, PSet_Revit_Identity Data, PSet_Revit_Phasing
          4 x IFCDOOR | type IFCDOORSTYLE "M9x21" | object type "M9x21" | names: "Int_door_Aart:M9x21:M9x21:14644277", "Int_door_Aart:M9x21:M9x21:14644334", "Int_door_Aart:M9x21:M9x21:14644357" (+1 more) | property sets: Pset_DoorCommon, PSet_Revit_Other, PSet_Revit_Dimensions, PSet_Revit_Constraints, PSet_Revit_Identity Data, PSet_Revit_Phasing
          2 x IFCDOOR | type IFCDOORSTYLE "M9x21" | object type "M9x21" | names: "Int_door_Aart:M9x21:M9x21:14644295", "Int_door_Aart:M9x21:M9x21:14644358" | property sets: Pset_DoorCommon, PSet_Revit_Other, PSet_Revit_Dimensions, PSet_Revit_Constraints, PSet_Revit_Identity Data, PSet_Revit_Phasing
          2 x IFCCURTAINWALL | object type "Curtain Wall:243.1_Indv_glasskillevæg:1131477" | names: "Curtain Wall:243.1_Indv_glasskillevæg:14644337", "Curtain Wall:243.1_Indv_glasskillevæg:21701806" | parts: 2 IFCPLATE | property sets: Pset_CurtainWallCommon, PSet_Revit_Structural, PSet_Revit_Constraints, PSet_Revit_Identity Data, PSet_Revit_Phasing, PSet_Revit_Dimensions
          3 x IFCWALLSTANDARDCASE | object type "Basic Wall:242.13_Type_2.2_Gipsvæg_197mm_Påforing Bad:7797614" | names: "Basic Wall:242.13_Type_2.2_Gipsvæg_197mm_Påforing Bad:14644359", "Basic Wall:242.13_Type_2.2_Gipsvæg_197mm_Påforing Bad:14644380", "Basic Wall:242.13_Type_2.2_Gipsvæg_197mm_Påforing Bad:14644410" | material: layers "Basic Wall:242.13_Type_2.2_Gipsvæg_197mm_Påforing Bad" ("Aart_Flise" 10., "Aart_Gips" 26., "Wood" 148., "Aart_Gips" 13.) | property sets: PSet_Revit_Structural, PSet_Revit_Constraints, PSet_Revit_Identity Data, PSet_Revit_Phasing, PSet_Revit_Dimensions, Pset_WallCommon
          3 x IFCWALLSTANDARDCASE | object type "Basic Wall:242.11_Type_4.3_Gipsvæg_124mm_påforing elevator:7479952" | names: "Basic Wall:242.11_Type_4.3_Gipsvæg_124mm_påforing elevator:14644397", "Basic Wall:242.11_Type_4.3_Gipsvæg_124mm_påforing elevator:14644416", "Basic Wall:242.11_Type_4.3_Gipsvæg_124mm_påforing elevator:21260708" | material: layers "Basic Wall:242.11_Type_4.3_Gipsvæg_124mm_påforing elevator" ("Aart_Gips" 26., "Wood" 98.) | property sets: PSet_Revit_Structural, PSet_Revit_Constraints, PSet_Revit_Identity Data, PSet_Revit_Phasing, PSet_Revit_Dimensions, Pset_WallCommon
          1 x IFCWALL | object type "Basic Wall:242.3_Type_2.1_Gipsvæg_147mm_Indv. vegge_Bad:7797675" | names: "Basic Wall:242.3_Type_2.1_Gipsvæg_147mm_Indv. vegge_Bad:14644411" | material: layers "Basic Wall:242.3_Type_2.1_Gipsvæg_147mm_Indv. vegge_Bad" ("Aart_Gips" 13., "A-Wood" 98., "Aart_Gips" 26., "Aart_Flise" 10.) | property sets: PSet_Revit_Structural, PSet_Revit_Constraints, PSet_Revit_Identity Data, PSet_Revit_Phasing, PSet_Revit_Dimensions, Pset_WallCommon
          1 x IFCSLAB | object type "Floor:Etasjedekk_250mm_betong" | FLOOR | names: "Floor:Etasjedekk_250mm_betong:15748267" | material: layers "Floor:Etasjedekk_250mm_betong" ("Aart_beton" 250.) | property sets: PSet_Revit_Constraints, PSet_Revit_Structural, PSet_Revit_Identity Data, PSet_Revit_Phasing, PSet_Revit_Dimensions, Pset_SlabCommon
          7 x IFCSLAB | object type "Floor:Etasjedekk_168mm_betong_Bad" | FLOOR | names: "Floor:Etasjedekk_168mm_betong_Bad:15748350", "Floor:Etasjedekk_168mm_betong_Bad:15748350:2", "Floor:Etasjedekk_168mm_betong_Bad:15748350:3" (+4 more) | material: layers "Floor:Etasjedekk_168mm_betong_Bad" ("Aart_beton" 168.) | property sets: PSet_Revit_Constraints, PSet_Revit_Structural, PSet_Revit_Identity Data, PSet_Revit_Phasing, PSet_Revit_Dimensions, Pset_SlabCommon
          4 x IFCSLAB | object type "Floor:Gulvopbygning_30mm" | FLOOR | names: "Floor:Gulvopbygning_30mm:15748557", "Floor:Gulvopbygning_30mm:15748557:2", "Floor:Gulvopbygning_30mm:15748557:3" (+1 more) | material: layers "Floor:Gulvopbygning_30mm" ("Wood - Flooring" 14., "Aart_Gips" 16.) | property sets: PSet_Revit_Constraints, PSet_Revit_Structural, PSet_Revit_Identity Data, PSet_Revit_Phasing, PSet_Revit_Dimensions, Pset_SlabCommon
          1 x IFCSLAB | object type "Floor:Gulvopbygning_112mm_Bad" | FLOOR | names: "Floor:Gulvopbygning_112mm_Bad:15749560" | material: layers "Floor:Gulvopbygning_112mm_Bad" ("Stone (2)" 12., "A-Conc" 100.) | property sets: PSet_Revit_Constraints, PSet_Revit_Structural, PSet_Revit_Identity Data, PSet_Revit_Phasing, PSet_Revit_Dimensions, Pset_SlabCommon
          1 x IFCWINDOW | type IFCWINDOWSTYLE "Skyveparti_2388x2288mm" | object type "Skyveparti_2388x2288mm" | names: "234.2_H_Udv._skyveparti_3fag Nytt:Skyveparti_2388x2288mm:Skyveparti_2388x2288mm:17537598" | property sets: Pset_WindowCommon, PSet_Revit_Other, PSet_Revit_Dimensions, PSet_Revit_Constraints, PSet_Revit_Identity Data, PSet_Revit_Phasing
          1 x IFCDOOR | type IFCDOORSTYLE "M9x21" | object type "M9x21" | names: "DAN_Indv. Skydedør i væg:M9x21:M9x21:19563276" | property sets: Pset_DoorCommon, PSet_Revit_Other, PSet_Revit_Materials and Finishes, PSet_Revit_Constraints, PSet_Revit_Identity Data, PSet_Revit_Phasing
          1 x IFCDOOR | type IFCDOORSTYLE "M9x21" | object type "M9x21" | names: "DAN_Indv. Skydedør i væg:M9x21:M9x21:19563436" | property sets: Pset_DoorCommon, PSet_Revit_Other, PSet_Revit_Materials and Finishes, PSet_Revit_Constraints, PSet_Revit_Identity Data, PSet_Revit_Phasing
          1 x IFCDOOR | type IFCDOORSTYLE "M9x21" | object type "M9x21" | names: "DAN_Indv. Skydedør i væg:M9x21:M9x21:19564550" | property sets: Pset_DoorCommon, PSet_Revit_Other, PSet_Revit_Materials and Finishes, PSet_Revit_Constraints, PSet_Revit_Identity Data, PSet_Revit_Phasing
          3 x IFCWINDOW | type IFCWINDOWSTYLE "1188 x 1488mm" | object type "1188 x 1488mm" | names: "234.3_V_Udv._vindu_1fag_PAR:1188 x 1488mm:1188 x 1488mm:20287888", "234.3_V_Udv._vindu_1fag_PAR:1188 x 1488mm:1188 x 1488mm:21187721", "234.3_V_Udv._vindu_1fag_PAR:1188 x 1488mm:1188 x 1488mm:21188085" | property sets: Pset_WindowCommon, PSet_Revit_Other, PSet_Revit_Constraints, PSet_Revit_Visibility, PSet_Revit_Identity Data, PSet_Revit_General
          1 x IFCWINDOW | type IFCWINDOWSTYLE "1188 x 1488mm" | object type "1188 x 1488mm" | names: "234.3_H_Udv._vindu_1fag_PAR:1188 x 1488mm:1188 x 1488mm:21174192" | property sets: Pset_WindowCommon, PSet_Revit_Other, PSet_Revit_Constraints, PSet_Revit_Visibility, PSet_Revit_Identity Data, PSet_Revit_General
          2 x IFCWINDOW | type IFCWINDOWSTYLE "2988x2288mm" | object type "2988x2288mm" | names: "234.7_H_Udv._vindu_høyt_3fag_PAR:2988x2288mm:2988x2288mm:21182058", "234.7_H_Udv._vindu_høyt_3fag_PAR:2988x2288mm:2988x2288mm:21182830" | property sets: Pset_WindowCommon, PSet_Revit_Other, PSet_Revit_Constraints, PSet_Revit_Visibility, PSet_Revit_Identity Data, PSet_Revit_General
          1 x IFCWINDOW | type IFCWINDOWSTYLE "2688x2288mm" | object type "2688x2288mm" | names: "234.7_H_Udv._vindu_høyt_3fag_PAR:2688x2288mm:2688x2288mm:21182861" | property sets: Pset_WindowCommon, PSet_Revit_Other, PSet_Revit_Constraints, PSet_Revit_Visibility, PSet_Revit_Identity Data, PSet_Revit_General
          14 x IFCBUILDINGELEMENTPROXY | object type "Lodret" | names: "Beklædning - Drypkant - Vandbord, underkant:Lodret:Lodret:21511773", "Beklædning - Drypkant - Vandbord, overkant:Lodret:Lodret:21512038", "Beklædning - Drypkant - Vandbord, overkant:Lodret:Lodret:21512357" (+11 more) | property sets: PSet_Revit_Dimensions, PSet_Revit_Constraints, PSet_Revit_Identity Data, PSet_Revit_Phasing, PSet_Revit_Type_Dimensions, PSet_Revit_Type_General
          1 x IFCCOVERING | object type "Compound Ceiling:kraft_Himling_Akustikkflåte" | CEILING | names: "Compound Ceiling:kraft_Himling_Akustikkflåte:22217806" | material: layers "Compound Ceiling:kraft_Himling_Akustikkflåte" ("Ceiling Tile 600 x 600" 40.) | property sets: Pset_CoveringCommon, PSet_Revit_Constraints, PSet_Revit_Identity Data, PSet_Revit_Dimensions, PSet_Revit_Phasing, PSet_Revit_Type_Construction
      IFCBUILDINGSTOREY "05" | elevation 11600.
        contains 60 elements
          1 x IFCSLAB | object type "Floor:Etasjedekk_250mm_betong" | FLOOR | names: "Floor:Etasjedekk_250mm_betong:3569711" | material: layers "Floor:Etasjedekk_250mm_betong" ("Aart_beton" 250.) | property sets: PSet_Revit_Constraints, PSet_Revit_Structural, PSet_Revit_Identity Data, PSet_Revit_Phasing, PSet_Revit_Dimensions, Pset_SlabCommon
          3 x IFCWALLSTANDARDCASE | object type "Basic Wall:242.3_Type_2.1_Gipsvæg_147mm_Indv. vegge_Bad:7797675" | names: "Basic Wall:242.3_Type_2.1_Gipsvæg_147mm_Indv. vegge_Bad:3629047", "Basic Wall:242.3_Type_2.1_Gipsvæg_147mm_Indv. vegge_Bad:4328249", "Basic Wall:242.3_Type_2.1_Gipsvæg_147mm_Indv. vegge_Bad:9159741" | material: layers "Basic Wall:242.3_Type_2.1_Gipsvæg_147mm_Indv. vegge_Bad" ("Aart_Gips" 13., "A-Wood" 98., "Aart_Gips" 26., "Aart_Flise" 10.) | property sets: PSet_Revit_Structural, PSet_Revit_Constraints, PSet_Revit_Identity Data, PSet_Revit_Phasing, PSet_Revit_Dimensions, Pset_WallCommon
          9 x IFCWALLSTANDARDCASE | object type "Basic Wall:242.1_Type_1.1_Gipsvæg_124mm_Indv. vegge:7478708" | names: "Basic Wall:242.1_Type_1.1_Gipsvæg_124mm_Indv. vegge:3629172", "Basic Wall:242.1_Type_1.1_Gipsvæg_124mm_Indv. vegge:3629176", "Basic Wall:242.1_Type_1.1_Gipsvæg_124mm_Indv. vegge:3696206" (+6 more) | material: layers "Basic Wall:242.1_Type_1.1_Gipsvæg_124mm_Indv. vegge" ("Aart_Gips" 13., "A-Wood" 98., "Aart_Gips" 13.) | property sets: PSet_Revit_Structural, PSet_Revit_Constraints, PSet_Revit_Identity Data, PSet_Revit_Phasing, PSet_Revit_Dimensions, Pset_WallCommon
          4 x IFCCURTAINWALL | object type "Curtain Wall:243.2_Indv_glasskillevæg_ikke stiplet:3935508" | names: "Curtain Wall:243.2_Indv_glasskillevæg_ikke stiplet:3629173", "Curtain Wall:243.2_Indv_glasskillevæg_ikke stiplet:3658338", "Curtain Wall:243.2_Indv_glasskillevæg_ikke stiplet:21703157" (+1 more) | parts: 4 IFCPLATE | property sets: Pset_CurtainWallCommon, PSet_Revit_Structural, PSet_Revit_Constraints, PSet_Revit_Identity Data, PSet_Revit_Phasing, PSet_Revit_Dimensions
          2 x IFCDOOR | type IFCDOORSTYLE "M9x21" | object type "M9x21" | names: "Int_door_Aart:M9x21:M9x21:3629182", "Int_door_Aart:M9x21:M9x21:21702287" | property sets: Pset_DoorCommon, PSet_Revit_Other, PSet_Revit_Dimensions, PSet_Revit_Constraints, PSet_Revit_Identity Data, PSet_Revit_Phasing
          7 x IFCWALLSTANDARDCASE | object type "Basic Wall:242.7_Type_3.1_Gipsvæg_111mm_Sjakt:17953268" | names: "Basic Wall:242.7_Type_3.1_Gipsvæg_111mm_Sjakt:3658337", "Basic Wall:242.7_Type_3.1_Gipsvæg_111mm_Sjakt:3663356", "Basic Wall:242.7_Type_3.1_Gipsvæg_111mm_Sjakt:9160124" (+4 more) | material: layers "Basic Wall:242.7_Type_3.1_Gipsvæg_111mm_Sjakt" ("Aart_Gips" 13., "A-Wood" 98.) | property sets: PSet_Revit_Structural, PSet_Revit_Constraints, PSet_Revit_Identity Data, PSet_Revit_Phasing, PSet_Revit_Dimensions, Pset_WallCommon
          2 x IFCDOOR | type IFCDOORSTYLE "M9x21" | object type "M9x21" | names: "Int_door_Aart:M9x21:M9x21:3842240", "Int_door_Aart:M9x21:M9x21:14615928" | property sets: Pset_DoorCommon, PSet_Revit_Other, PSet_Revit_Dimensions, PSet_Revit_Constraints, PSet_Revit_Identity Data, PSet_Revit_Phasing
          1 x IFCDOOR | type IFCDOORSTYLE "M10x21" | object type "M10x21" | names: "Utv. dør_Leilighet:M10x21:M10x21:5641098" | property sets: Pset_DoorCommon, PSet_Revit_Other, PSet_Revit_Constraints, PSet_Revit_Identity Data, PSet_Revit_Construction, PSet_Revit_Text
          2 x IFCDOOR | type IFCDOORSTYLE "M9x21" | object type "M9x21" | names: "Int_door_Aart:M9x21:M9x21:6020606", "Int_door_Aart:M9x21:M9x21:6020655" | property sets: Pset_DoorCommon, PSet_Revit_Other, PSet_Revit_Dimensions, PSet_Revit_Constraints, PSet_Revit_Identity Data, PSet_Revit_Phasing
          1 x IFCWALL | object type "Basic Wall:242.3_Type_2.1_Gipsvæg_147mm_Indv. vegge_Bad:7797675" | names: "Basic Wall:242.3_Type_2.1_Gipsvæg_147mm_Indv. vegge_Bad:9160695" | material: layers "Basic Wall:242.3_Type_2.1_Gipsvæg_147mm_Indv. vegge_Bad" ("Aart_Gips" 13., "A-Wood" 98., "Aart_Gips" 26., "Aart_Flise" 10.) | property sets: PSet_Revit_Structural, PSet_Revit_Constraints, PSet_Revit_Identity Data, PSet_Revit_Phasing, PSet_Revit_Dimensions, Pset_WallCommon
          1 x IFCSLAB | object type "Floor:Gulvopbygning_30mm" | FLOOR | names: "Floor:Gulvopbygning_30mm:9194954" | material: layers "Floor:Gulvopbygning_30mm" ("Wood - Flooring" 14., "Aart_Gips" 16.) | property sets: PSet_Revit_Constraints, PSet_Revit_Structural, PSet_Revit_Identity Data, PSet_Revit_Phasing, PSet_Revit_Dimensions, Pset_SlabCommon
          2 x IFCSLAB | object type "Floor:Etasjedekk_168mm_betong_Bad" | FLOOR | names: "Floor:Etasjedekk_168mm_betong_Bad:9195273", "Floor:Etasjedekk_168mm_betong_Bad:9195273:2" | material: layers "Floor:Etasjedekk_168mm_betong_Bad" ("Aart_beton" 168.) | property sets: PSet_Revit_Constraints, PSet_Revit_Structural, PSet_Revit_Identity Data, PSet_Revit_Phasing, PSet_Revit_Dimensions, Pset_SlabCommon
          3 x IFCSLAB | object type "Floor:Gulvopbygning_112mm_Bad" | FLOOR | names: "Floor:Gulvopbygning_112mm_Bad:9195430", "Floor:Gulvopbygning_112mm_Bad:9195430:2", "Floor:Gulvopbygning_112mm_Bad:9195430:3" | material: layers "Floor:Gulvopbygning_112mm_Bad" ("Stone (2)" 12., "A-Conc" 100.) | property sets: PSet_Revit_Constraints, PSet_Revit_Structural, PSet_Revit_Identity Data, PSet_Revit_Phasing, PSet_Revit_Dimensions, Pset_SlabCommon
          5 x IFCCOVERING | object type "Compound Ceiling:KRAFT_61mm_Gips_ himling" | CEILING | names: "Compound Ceiling:KRAFT_61mm_Gips_ himling:9198770", "Compound Ceiling:KRAFT_61mm_Gips_ himling:9198792", "Compound Ceiling:KRAFT_61mm_Gips_ himling:9198802" (+2 more) | material: layers "Compound Ceiling:KRAFT_61mm_Gips_ himling" ("A-Air" 48., "Gyproc Gipsplade_2560mm" 13.) | property sets: Pset_CoveringCommon, PSet_Revit_Constraints, PSet_Revit_Identity Data, PSet_Revit_Dimensions, PSet_Revit_Phasing, PSet_Revit_Type_Construction
          1 x IFCWALLSTANDARDCASE | object type "Basic Wall:242.17_Fliser_10mm:7816687" | names: "Basic Wall:242.17_Fliser_10mm:9255286" | material: layers "Basic Wall:242.17_Fliser_10mm" ("Aart_Flise" 10.) | property sets: PSet_Revit_Structural, PSet_Revit_Constraints, PSet_Revit_Identity Data, PSet_Revit_Phasing, PSet_Revit_Dimensions, Pset_WallCommon
          1 x IFCRAILING | object type "Railing:rekkverk_vinduer_type2_(1200mm)" | names: "Railing:rekkverk_vinduer_type2_(1200mm):11770693" | material: "Wood - Timber" | property sets: Pset_RailingCommon, PSet_Revit_Dimensions, PSet_Revit_Constraints, PSet_Revit_Identity Data, PSet_Revit_Phasing, PSet_Revit_Type_Construction
          3 x IFCBUILDINGELEMENTPROXY | object type "Ventilator" | names: "Køkkenaftræk mml:Ventilator:Ventilator:13329193", "Køkkenaftræk mml:Ventilator:Ventilator:13329195", "Køkkenaftræk mml:Ventilator:Ventilator:13329196" | property sets: PSet_Revit_Other, PSet_Revit_Constraints, PSet_Revit_Identity Data, PSet_Revit_Phasing, PSet_Revit_Type_Dimensions, PSet_Revit_Type_Identity Data
          1 x IFCWINDOW | type IFCWINDOWSTYLE "2388x1488 mm" | object type "2388x1488 mm" | names: "234.4_V_Udv._vindu_2fag Nytt:2388x1488 mm:2388x1488 mm:14709876" | property sets: Pset_WindowCommon, PSet_Revit_Other, PSet_Revit_Dimensions, PSet_Revit_Graphics, PSet_Revit_Constraints, PSet_Revit_Identity Data
          1 x IFCWINDOW | type IFCWINDOWSTYLE "Skyveparti_2388x2288mm" | object type "Skyveparti_2388x2288mm" | names: "234.2_H_Udv._skyveparti_3fag Nytt:Skyveparti_2388x2288mm:Skyveparti_2388x2288mm:17537759" | property sets: Pset_WindowCommon, PSet_Revit_Other, PSet_Revit_Dimensions, PSet_Revit_Constraints, PSet_Revit_Identity Data, PSet_Revit_Phasing
          1 x IFCCURTAINWALL | object type "Curtain Wall:243.1_Indv_glasskillevæg:1131477" | names: "Curtain Wall:243.1_Indv_glasskillevæg:19013334" | parts: 1 IFCPLATE | property sets: Pset_CurtainWallCommon, PSet_Revit_Structural, PSet_Revit_Constraints, PSet_Revit_Identity Data, PSet_Revit_Phasing, PSet_Revit_Dimensions
          1 x IFCDOOR | type IFCDOORSTYLE "M 8x21" | object type "M 8x21" | names: "DAN_Indv. Skydedør i væg:M 8x21:M 8x21:19566036" | property sets: Pset_DoorCommon, PSet_Revit_Other, PSet_Revit_Materials and Finishes, PSet_Revit_Constraints, PSet_Revit_Identity Data, PSet_Revit_Phasing
          1 x IFCDOOR | type IFCDOORSTYLE "M 8x21" | object type "M 8x21" | names: "DAN_Indv. Skydedør i væg:M 8x21:M 8x21:19566087" | property sets: Pset_DoorCommon, PSet_Revit_Other, PSet_Revit_Materials and Finishes, PSet_Revit_Constraints, PSet_Revit_Identity Data, PSet_Revit_Phasing
          1 x IFCWINDOW | type IFCWINDOWSTYLE "1188 x 1488mm" | object type "1188 x 1488mm" | names: "234.3_H_Udv._vindu_1fag_PAR:1188 x 1488mm:1188 x 1488mm:20288139" | property sets: Pset_WindowCommon, PSet_Revit_Other, PSet_Revit_Constraints, PSet_Revit_Visibility, PSet_Revit_Identity Data, PSet_Revit_General
          1 x IFCWINDOW | type IFCWINDOWSTYLE "1188 x 1488mm" | object type "1188 x 1488mm" | names: "234.3_H_Udv._vindu_1fag_PAR:1188 x 1488mm:1188 x 1488mm:21187754" | property sets: Pset_WindowCommon, PSet_Revit_Other, PSet_Revit_Constraints, PSet_Revit_Visibility, PSet_Revit_Identity Data, PSet_Revit_General
          5 x IFCBUILDINGELEMENTPROXY | object type "Lodret" | names: "Beklædning - Drypkant - Vandbord, underkant:Lodret:Lodret:21512634", "Beklædning - Drypkant - Vandbord, overkant:Lodret:Lodret:21512714", "Beklædning - Drypkant - Vandbord, overkant:Lodret:Lodret:21516122" (+2 more) | property sets: PSet_Revit_Dimensions, PSet_Revit_Constraints, PSet_Revit_Identity Data, PSet_Revit_Phasing, PSet_Revit_Type_Dimensions, PSet_Revit_Type_General
      IFCBUILDINGSTOREY "06" | elevation 14500.
        contains 2 elements
          2 x IFCBUILDINGELEMENTPROXY | object type "Basic Wall:Aart_Yttervegg_401mm_type_1_NY" | names: "Basic Wall:Aart_Yttervegg_401mm_type_1_NY" | property sets: Pset_BuildingElementProxyCommon, PSet_Revit_Constraints, PSet_Revit_Dimensions, PSet_Revit_Identity Data, PSet_Revit_Phasing, PSet_Revit_Type_Construction
      IFCBUILDINGSTOREY "06T" | elevation 24300.
        contains 1 element
          1 x IFCROOF | object type "Basic Roof:Tag til attach walls 649mm" | names: "Basic Roof:Tag til attach walls 649mm:1013085" | material: layers "Basic Roof:Tag til attach walls 649mm" ("Tagbeklædning_1" 50., "Tagbeklædning_1" 238., "Aart_isolering" 350., "Aart_isolering" 48., "Aart_Gips" 13.) | property sets: Pset_RoofCommon, PSet_Revit_Constraints, PSet_Revit_Dimensions, PSet_Revit_Construction, PSet_Revit_Identity Data, PSet_Revit_Phasing
      IFCBUILDINGSTOREY "etasje 06-1" | elevation 14822.
        contains 1 element
          1 x IFCBUILDINGELEMENTPROXY | object type "Ventilator" | names: "Køkkenaftræk mml:Ventilator:Ventilator:13329197" | property sets: PSet_Revit_Other, PSet_Revit_Constraints, PSet_Revit_Identity Data, PSet_Revit_Phasing, PSet_Revit_Type_Dimensions, PSet_Revit_Type_Identity Data

Types
  IFCWINDOWSTYLE "4188x2088" | 1 occurrence | property sets: 234.25_H_Udv._vindu_1fag_PAR:4188x2088:4188x2088:21880914
  IFCWINDOWSTYLE "2688x2088" | 2 occurrences | property sets: 234.25_F_Udv._vindu_1fag_PAR_us:2688x2088:2688x2088:21880919
  IFCWINDOWSTYLE "3888x2088" | 1 occurrence | property sets: 234.25_H_Udv._vindu_1fag_PAR:3888x2088:3888x2088:21880929
  IFCDOORSTYLE "2388 x 2488 (næring)" | SINGLE_SWING_LEFT | 1 occurrence | property sets: 234.18_H24-:2388 x 2488 (næring):2388 x 2488 (næring):21880930
  IFCDOORSTYLE "2388 x 2488 (næring)" | SINGLE_SWING_RIGHT | 1 occurrence | property sets: 234.18_V24_Næring:2388 x 2488 (næring):2388 x 2488 (næring):21880939
  IFCWINDOWSTYLE "2988x2088" | 1 occurrence | property sets: 234.25_H_Udv._vindu_1fag_PAR:2988x2088:2988x2088:21880943
  IFCDOORSTYLE "M10x21" | 4 occurrences | property sets: Hoveddør_Leilighet:M10x21:M10x21:1517569
  IFCDOORSTYLE "M9x21" | 25 occurrences | property sets: Int_door_Aart:M9x21:M9x21:3628180
  IFCDOORSTYLE "M9x21" | 27 occurrences | property sets: Int_door_Aart:M9x21:M9x21:3628187
  IFCDOORSTYLE "M9x21" | 9 occurrences | property sets: Int_door_Aart:M9x21:M9x21:3628223
  IFCDOORSTYLE "M9x21" | 1 occurrence | property sets: DAN_Indv. Skydedør i væg:M9x21:M9x21:3628231
  IFCDOORSTYLE "M9x21" | 14 occurrences | property sets: Int_door_Aart:M9x21:M9x21:3628242
  IFCDOORSTYLE "M9x21" | 2 occurrences | property sets: DAN_Indv. Skydedør i væg:M9x21:M9x21:3628243
  IFCDOORSTYLE "M10x21" | 5 occurrences | property sets: Utv. dør_Leilighet:M10x21:M10x21:1689354
  IFCDOORSTYLE "M10x21" | 4 occurrences | property sets: Utv. dør_Leilighet:M10x21:M10x21:2992344
  IFCDOORSTYLE "M10x21" | 4 occurrences | property sets: Hoveddør_Leilighet:M10x21:M10x21:3026092
  IFCWINDOWSTYLE "Skyveparti_2088x2288mm" | 5 occurrences | property sets: 234.2_V_Udv._skyveparti_3fag Nytt:Skyveparti_2088x2288mm:Skyveparti_2088x2288mm:10991077
  IFCWINDOWSTYLE "1188x1488 mm" | 12 occurrences | property sets: 234.3_V_Udv._vindu_1fag(nytt):1188x1488 mm:1188x1488 mm:2374111
  IFCDOORSTYLE "2388 x 2288" | SINGLE_SWING_LEFT | 1 occurrence | property sets: 234.18_H24 Nytt:2388 x 2288:2388 x 2288:14707761
  IFCDOORSTYLE "M11x21" | 4 occurrences | property sets: DAN_Indv. Skydedør i væg:M11x21:M11x21:19561768
  IFCDOORSTYLE "M11x21" | 1 occurrence | property sets: DAN_Indv. Skydedør i væg:M11x21:M11x21:19562058
  IFCWINDOWSTYLE "1188 x 1488mm" | 12 occurrences | property sets: 234.3_V_Udv._vindu_1fag_PAR:1188 x 1488mm:1188 x 1488mm:20287888
  IFCDOORSTYLE "M9x21" | 1 occurrence | property sets: DAN_Indv. Skydedør i væg:M9x21:M9x21:20697993
  IFCDOORSTYLE "M8x21" | 1 occurrence | property sets: Int_door_Aart:M8x21:M8x21:20698194
  IFCWINDOWSTYLE "2988x2288mm" | 4 occurrences | property sets: 234.7_H_Udv._vindu_høyt_3fag_PAR:2988x2288mm:2988x2288mm:21170239
  IFCWINDOWSTYLE "1188 x 1488mm" | 1 occurrence | property sets: 234.3_H_Udv._vindu_1fag_PAR:1188 x 1488mm:1188 x 1488mm:21170258
  IFCWINDOWSTYLE "2988x2288mm" | 3 occurrences | property sets: 234.7_V_Udv._vindu_høyt_3fag_PAR:2988x2288mm:2988x2288mm:21182210
  IFCWINDOWSTYLE "Skyveparti_2688x2288mm" | 1 occurrence | property sets: 234.2_V_Udv._skyveparti_3fag Nytt:Skyveparti_2688x2288mm:Skyveparti_2688x2288mm:21188430
  IFCWINDOWSTYLE "Skyveparti_2388x2288mm" | 2 occurrences | property sets: 234.2_V_Udv._skyveparti_3fag Nytt:Skyveparti_2388x2288mm:Skyveparti_2388x2288mm:17533459
  IFCWINDOWSTYLE "Skyveparti_2088x2288mm" | 3 occurrences | property sets: 234.2_H_Udv._skyveparti_3fag Nytt:Skyveparti_2088x2288mm:Skyveparti_2088x2288mm:3508597
  IFCWINDOWSTYLE "2388x1488 mm" | 2 occurrences | property sets: 234.4_V_Udv._vindu_2fag Nytt:2388x1488 mm:2388x1488 mm:14707764
  IFCWINDOWSTYLE "Skyveparti_2388x2288mm" | 3 occurrences | property sets: 234.2_H_Udv._skyveparti_3fag Nytt:Skyveparti_2388x2288mm:Skyveparti_2388x2288mm:17530858
  IFCWINDOWSTYLE "2988x2288mm" | 1 occurrence | property sets: 234.7_V_Udv._vindu_høyt_3fag_PAR:2988x2288mm:2988x2288mm:21170260
  IFCWINDOWSTYLE "1188 x 1488mm" | 4 occurrences | property sets: 234.3_H_Udv._vindu_1fag_PAR:1188 x 1488mm:1188 x 1488mm:21173899
  IFCWINDOWSTYLE "Skyveparti_2688x2288mm" | 2 occurrences | property sets: 234.2_H_Udv._skyveparti_3fag Nytt:Skyveparti_2688x2288mm:Skyveparti_2688x2288mm:17533462
  IFCDOORSTYLE "M9x21" | 2 occurrences | property sets: DAN_Indv. Skydedør i væg:M9x21:M9x21:9093941
  IFCDOORSTYLE "M9x21" | 1 occurrence | property sets: DAN_Indv. Skydedør i væg:M9x21:M9x21:9093948
  IFCDOORSTYLE "M11x21" | 1 occurrence | property sets: DAN_Indv. Skydedør i væg:M11x21:M11x21:19562932
  IFCWINDOWSTYLE "Skyveparti_2688x2288mm" | 1 occurrence | property sets: 234.2_V_Udv._skyveparti_3fag Nytt:Skyveparti_2688x2288mm:Skyveparti_2688x2288mm:4731875
  IFCDOORSTYLE "M9x21" | 1 occurrence | property sets: DAN_Indv. Skydedør i væg:M9x21:M9x21:19563436
  IFCWINDOWSTYLE "2688x2288mm" | 1 occurrence | property sets: 234.7_H_Udv._vindu_høyt_3fag_PAR:2688x2288mm:2688x2288mm:21182861
  IFCDOORSTYLE "M 8x21" | 1 occurrence | property sets: DAN_Indv. Skydedør i væg:M 8x21:M 8x21:19566036
  IFCDOORSTYLE "M 8x21" | 1 occurrence | property sets: DAN_Indv. Skydedør i væg:M 8x21:M 8x21:19566087
  IFCWINDOWSTYLE "1188 x 1488mm" | 1 occurrence | property sets: 234.3_H_Udv._vindu_1fag_PAR:1188 x 1488mm:1188 x 1488mm:20288139

Property sets
  Pset_BuildingElementProxyCommon | properties | on 2 objects (2 IFCBUILDINGELEMENTPROXY)
    Reference = "Basic Wall:Aart_Yttervegg_401mm_type_1_NY" (IFCIDENTIFIER)
  PSet_Revit_Constraints | properties | on 46 objects (46 IFCWALLSTANDARDCASE)
    Base Constraint = "02" (IFCLABEL)
    Base Extension Distance = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Base Offset = -30. (IFCLENGTHMEASURE) [MILLI METRE]
    Base is Attached = FALSE (IFCBOOLEAN)
    Location Line = 2 (IFCINTEGER)
    Related to Mass = FALSE (IFCBOOLEAN)
    Room Bounding = TRUE (IFCBOOLEAN)
    Top Constraint = "Up to level: 03" (IFCLABEL)
    Top Extension Distance = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Top Offset = -280. (IFCLENGTHMEASURE) [MILLI METRE]
    Top is Attached = FALSE (IFCBOOLEAN)
    Unconnected Height = 2650. (IFCLENGTHMEASURE) [MILLI METRE]
  PSet_Revit_Constraints | properties | on 42 objects (41 IFCWALLSTANDARDCASE, 1 IFCWALL)
    Base Constraint = "03" (IFCLABEL)
    Base Extension Distance = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Base Offset = -30. (IFCLENGTHMEASURE) [MILLI METRE]
    Base is Attached = FALSE (IFCBOOLEAN)
    Location Line = 2 (IFCINTEGER)
    Related to Mass = FALSE (IFCBOOLEAN)
    Room Bounding = TRUE (IFCBOOLEAN)
    Top Constraint = "Up to level: 04" (IFCLABEL)
    Top Extension Distance = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Top Offset = -280. (IFCLENGTHMEASURE) [MILLI METRE]
    Top is Attached = FALSE (IFCBOOLEAN)
    Unconnected Height = 2649.999999999999 (IFCLENGTHMEASURE) [MILLI METRE]
  PSet_Revit_Constraints | properties | on 37 objects (36 IFCWALLSTANDARDCASE, 1 IFCWALL)
    Base Constraint = "01" (IFCLABEL)
    Base Extension Distance = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Base Offset = -400. (IFCLENGTHMEASURE) [MILLI METRE]
    Base is Attached = FALSE (IFCBOOLEAN)
    Location Line = 2 (IFCINTEGER)
    Related to Mass = FALSE (IFCBOOLEAN)
    Room Bounding = TRUE (IFCBOOLEAN)
    Top Constraint = "Up to level: 02" (IFCLABEL)
    Top Extension Distance = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Top Offset = -280. (IFCLENGTHMEASURE) [MILLI METRE]
    Top is Attached = FALSE (IFCBOOLEAN)
    Unconnected Height = 3020. (IFCLENGTHMEASURE) [MILLI METRE]
  PSet_Revit_Constraints | properties | on 30 objects (26 IFCDOOR, 4 IFCWINDOW)
    Level = "03" (IFCLABEL)
    Sill Height = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  PSet_Revit_Constraints | properties | on 30 objects (26 IFCDOOR, 4 IFCWINDOW)
    Level = "02" (IFCLABEL)
    Sill Height = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  PSet_Revit_Constraints | properties | on 28 objects (24 IFCDOOR, 4 IFCWINDOW)
    Level = "04" (IFCLABEL)
    Sill Height = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  PSet_Revit_Constraints | properties | on 27 objects (25 IFCDOOR, 2 IFCWINDOW)
    Level = "01" (IFCLABEL)
    Sill Height = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  PSet_Revit_Constraints | properties | on 26 objects (26 IFCWALLSTANDARDCASE)
    Base Constraint = "01" (IFCLABEL)
    Base Extension Distance = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Base Offset = -400. (IFCLENGTHMEASURE) [MILLI METRE]
    Base is Attached = FALSE (IFCBOOLEAN)
    Location Line = 0 (IFCINTEGER)
    Related to Mass = FALSE (IFCBOOLEAN)
    Room Bounding = TRUE (IFCBOOLEAN)
    Top Constraint = "Up to level: 02" (IFCLABEL)
    Top Extension Distance = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Top Offset = -280. (IFCLENGTHMEASURE) [MILLI METRE]
    Top is Attached = FALSE (IFCBOOLEAN)
    Unconnected Height = 3020. (IFCLENGTHMEASURE) [MILLI METRE]
  PSet_Revit_Constraints: 295 more contents on 721 objects not shown
  PSet_Revit_Dimensions | properties | on 75 objects (75 IFCDOOR)
    Bredde = 910.0000000000001 (IFCLENGTHMEASURE) [MILLI METRE]
    Højde = 2099.999999999983 (IFCLENGTHMEASURE) [MILLI METRE]
  PSet_Revit_Dimensions | properties | on 12 objects (12 IFCWINDOW)
    Insert = 104. (IFCLENGTHMEASURE) [MILLI METRE]
  PSet_Revit_Dimensions | properties | on 11 objects (10 IFCOPENINGELEMENT, 1 IFCSLAB)
    Area = 291256327.6510285 (IFCAREAMEASURE) [MILLI SQUARE_METRE]
    Perimeter = 177974.6567981747 (IFCLENGTHMEASURE) [MILLI METRE]
    Thickness = 250. (IFCLENGTHMEASURE) [MILLI METRE]
    Volume = 72814081912.75714 (IFCVOLUMEMEASURE) [MILLI CUBIC_METRE]
  PSet_Revit_Dimensions | properties | on 11 objects (10 IFCOPENINGELEMENT, 1 IFCSLAB)
    Area = 285027909.5245574 (IFCAREAMEASURE) [MILLI SQUARE_METRE]
    Perimeter = 176771.3359067841 (IFCLENGTHMEASURE) [MILLI METRE]
    Thickness = 250. (IFCLENGTHMEASURE) [MILLI METRE]
    Volume = 71256977381.13921 (IFCVOLUMEMEASURE) [MILLI CUBIC_METRE]
  PSet_Revit_Dimensions | properties | on 11 objects (10 IFCOPENINGELEMENT, 1 IFCSLAB)
    Area = 278956093.6939705 (IFCAREAMEASURE) [MILLI SQUARE_METRE]
    Perimeter = 176020.6834755239 (IFCLENGTHMEASURE) [MILLI METRE]
    Thickness = 250. (IFCLENGTHMEASURE) [MILLI METRE]
    Volume = 69739023423.49246 (IFCVOLUMEMEASURE) [MILLI CUBIC_METRE]
  PSet_Revit_Dimensions | properties | on 10 objects (8 IFCOPENINGELEMENT, 2 IFCSLAB)
    Area = 334065440.9055131 (IFCAREAMEASURE) [MILLI SQUARE_METRE]
    Perimeter = 131354.8301420191 (IFCLENGTHMEASURE) [MILLI METRE]
    Thickness = 250. (IFCLENGTHMEASURE) [MILLI METRE]
    Volume = 83516360226.37827 (IFCVOLUMEMEASURE) [MILLI CUBIC_METRE]
  PSet_Revit_Dimensions | properties | on 10 objects (10 IFCSLAB)
    Area = 42688180.73383385 (IFCAREAMEASURE) [MILLI SQUARE_METRE]
    Perimeter = 85702.79291276804 (IFCLENGTHMEASURE) [MILLI METRE]
    Thickness = 112. (IFCLENGTHMEASURE) [MILLI METRE]
    Volume = 4781076242.189386 (IFCVOLUMEMEASURE) [MILLI CUBIC_METRE]
  PSet_Revit_Dimensions | properties | on 10 objects (10 IFCSLAB)
    Area = 42140820.01256884 (IFCAREAMEASURE) [MILLI SQUARE_METRE]
    Perimeter = 84780.79038192213 (IFCLENGTHMEASURE) [MILLI METRE]
    Thickness = 112. (IFCLENGTHMEASURE) [MILLI METRE]
    Volume = 4719771841.407725 (IFCVOLUMEMEASURE) [MILLI CUBIC_METRE]
  PSet_Revit_Dimensions: 657 more contents on 778 objects not shown
  PSet_Revit_Identity Data | properties | on 537 objects (374 IFCWALLSTANDARDCASE, 51 IFCSLAB, 33 IFCCOVERING, 30 IFCRAILING)
    Design Option = "Main Model" (IFCLABEL)
    Edited by = "" (IFCLABEL)
    Workset = 39791 (IFCINTEGER)
  PSet_Revit_Identity Data | properties | on 159 objects (52 IFCCOVERING, 50 IFCOPENINGELEMENT, 30 IFCSLAB, 12 IFCWALLSTANDARDCASE)
    Bygg = "Bygg 4" (IFCLABEL)
    Design Option = "Main Model" (IFCLABEL)
    Edited by = "" (IFCLABEL)
    Workset = 39791 (IFCINTEGER)
  PSet_Revit_Identity Data | properties | on 60 objects (60 IFCBUILDINGELEMENTPROXY)
    Design Option = "Main Model" (IFCLABEL)
    Edited by = "" (IFCLABEL)
    Mark = "T6" (IFCLABEL)
    Workset = 39791 (IFCINTEGER)
  PSet_Revit_Identity Data | properties | on 34 objects (34 IFCBUILDINGELEMENTPROXY)
    Design Option = "Main Model" (IFCLABEL)
    Edited by = "" (IFCLABEL)
    Mark = "T4" (IFCLABEL)
    Workset = 39791 (IFCINTEGER)
  PSet_Revit_Identity Data | properties | on 9 objects (9 IFCBUILDINGELEMENTPROXY)
    Design Option = "Main Model" (IFCLABEL)
    Edited by = "" (IFCLABEL)
    Mark = "T1" (IFCLABEL)
    Workset = 39791 (IFCINTEGER)
  PSet_Revit_Identity Data | properties | on 7 objects (7 IFCBUILDINGELEMENTPROXY)
    Design Option = "Main Model" (IFCLABEL)
    Edited by = "" (IFCLABEL)
    Mark = "T3" (IFCLABEL)
    Workset = 39791 (IFCINTEGER)
  PSet_Revit_Identity Data | properties | on 4 objects (4 IFCBUILDINGELEMENTPROXY)
    Bygg = "" (IFCLABEL)
    Design Option = "Main Model" (IFCLABEL)
    Edited by = "" (IFCLABEL)
    Mark = "T4" (IFCLABEL)
    Workset = 39791 (IFCINTEGER)
  PSet_Revit_Identity Data | properties | on 1 object (1 IFCDOOR)
    Brandkrav = "EI 30 - S" (IFCLABEL)
    Bygg = "Bygg 4" (IFCLABEL)
    Comments = "HC terskel" (IFCLABEL)
    Design Option = "Main Model" (IFCLABEL)
    Edited by = "" (IFCLABEL)
    Hinge Side = "H" (IFCLABEL)
    Lejlighedsnummer = "H0301" (IFCLABEL)
    Mark = "HD.04.03.1" (IFCLABEL)
    Workset = 39791 (IFCINTEGER)
  PSet_Revit_Identity Data: 189 more contents on 189 objects not shown
  PSet_Revit_Phasing | properties | on 990 objects (387 IFCWALLSTANDARDCASE, 126 IFCBUILDINGELEMENTPROXY, 112 IFCDOOR, 85 IFCCOVERING)
    Phase Created = "New Construction" (IFCLABEL)
  PSet_Revit_Structural | properties | on 422 objects (387 IFCWALLSTANDARDCASE, 16 IFCWALL, 12 IFCCURTAINWALL, 7 IFCOPENINGELEMENT)
    Enable Analytical Model = FALSE (IFCBOOLEAN)
    Structural = FALSE (IFCBOOLEAN)
    Structural Usage = 0 (IFCINTEGER)
  PSet_Revit_Structural | properties | on 131 objects (81 IFCSLAB, 50 IFCOPENINGELEMENT)
    Enable Analytical Model = FALSE (IFCBOOLEAN)
    Structural = FALSE (IFCBOOLEAN)
  PSet_Revit_Structural | properties | on 4 objects (4 IFCSTAIR)
    Rebar Cover = "Rebar Cover 1 <25>" (IFCLABEL)
  Pset_SlabCommon | properties | on 81 objects (81 IFCSLAB)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "" (IFCIDENTIFIER)
  BaseQuantities | quantities | on 14 objects (14 IFCSLAB)
    CrossArea = 92903.04000000001 [MILLI SQUARE_METRE]
    Perimeter = 241.8543912357866 [MILLI SQUARE_METRE]
  BaseQuantities | quantities | on 10 objects (10 IFCSLAB)
    CrossArea = 92903.04000000001 [MILLI SQUARE_METRE]
    Perimeter = 281.1771421022573 [MILLI SQUARE_METRE]
  BaseQuantities | quantities | on 10 objects (10 IFCSLAB)
    CrossArea = 92903.04000000001 [MILLI SQUARE_METRE]
    Perimeter = 278.152199415755 [MILLI SQUARE_METRE]
  BaseQuantities | quantities | on 7 objects (7 IFCSLAB)
    CrossArea = 92903.04000000001 [MILLI SQUARE_METRE]
    Perimeter = 241.8543912381644 [MILLI SQUARE_METRE]
  BaseQuantities | quantities | on 6 objects (6 IFCSLAB)
    CrossArea = 92903.04000000001 [MILLI SQUARE_METRE]
    Perimeter = 166.7540789994831 [MILLI SQUARE_METRE]
  BaseQuantities | quantities | on 5 objects (5 IFCSLAB)
    CrossArea = 92903.04000000001 [MILLI SQUARE_METRE]
    Perimeter = 880.3730712355279 [MILLI SQUARE_METRE]
  BaseQuantities | quantities | on 4 objects (4 IFCSLAB)
    CrossArea = 92903.04000000001 [MILLI SQUARE_METRE]
    Perimeter = 819.1986969562755 [MILLI SQUARE_METRE]
  BaseQuantities | quantities | on 4 objects (4 IFCSLAB)
    CrossArea = 92903.04000000001 [MILLI SQUARE_METRE]
    Perimeter = 798.0487669770785 [MILLI SQUARE_METRE]
  BaseQuantities: 14 more contents on 21 objects not shown
  Pset_WallCommon | properties | on 358 objects (346 IFCWALLSTANDARDCASE, 12 IFCWALL)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "" (IFCIDENTIFIER)
  Pset_WallCommon | properties | on 42 objects (41 IFCWALLSTANDARDCASE, 1 IFCWALL)
    ExtendToStructure = TRUE (IFCBOOLEAN)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "" (IFCIDENTIFIER)
  Pset_WallCommon | properties | on 3 objects (3 IFCWALL)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "" (IFCIDENTIFIER)
  Pset_RoofCommon | properties | on 1 object (1 IFCROOF)
    IsExternal = TRUE (IFCBOOLEAN)
    ProjectedArea = 350227324.5832107 (IFCAREAMEASURE) [MILLI SQUARE_METRE]
    Reference = "Basic Roof:Tag til attach walls 649mm" (IFCIDENTIFIER)
    TotalArea = 359241069.132382 (IFCAREAMEASURE) [MILLI SQUARE_METRE]
  PSet_Revit_Construction | properties | on 9 objects (9 IFCDOOR)
    Frame Type = "Tre dør/Isolert" (IFCLABEL)
  PSet_Revit_Construction | properties | on 8 objects (8 IFCDOOR)
    Frame Type = "Tre dør" (IFCLABEL)
  PSet_Revit_Construction | properties | on 1 object (1 IFCROOF)
    Fascia Depth = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Rafter Cut = 33615 (IFCINTEGER)
  Pset_StairCommon | properties | on 2 objects (2 IFCSTAIR)
    IsExternal = FALSE (IFCBOOLEAN)
    NumberOfRiser = 17 (IFCINTEGER)
    NumberOfTreads = 18 (IFCINTEGER)
    Reference = "Stair:Trappeopgang" (IFCIDENTIFIER)
    RiserHeight = 170.5882352941177 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    TreadLength = 280. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_StairCommon | properties | on 1 object (1 IFCSTAIR)
    IsExternal = FALSE (IFCBOOLEAN)
    NumberOfRiser = 17 (IFCINTEGER)
    NumberOfTreads = 18 (IFCINTEGER)
    Reference = "Stair:Trappeopgang" (IFCIDENTIFIER)
    RiserHeight = 170.5882352941176 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    TreadLength = 280. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_StairCommon | properties | on 1 object (1 IFCSTAIR)
    IsExternal = FALSE (IFCBOOLEAN)
    NumberOfRiser = 22 (IFCINTEGER)
    NumberOfTreads = 22 (IFCINTEGER)
    Reference = "Stair:Trappeopgang niv_0" (IFCIDENTIFIER)
    RiserHeight = 170.0000000000291 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    TreadLength = 250. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_StairCommon | properties | on 1 object (1 IFCSTAIR)
    IsExternal = FALSE (IFCBOOLEAN)
    NumberOfRiser = 14 (IFCINTEGER)
    NumberOfTreads = 14 (IFCINTEGER)
    Reference = "Stair:Hemsetrappe" (IFCIDENTIFIER)
    RiserHeight = 193.3333333333334 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    TreadLength = 250. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  PSet_Revit_Graphics | properties | on 14 objects (14 IFCWINDOW)
    Infatning_lige_væg = FALSE (IFCBOOLEAN)
    Infatning_skrå = FALSE (IFCBOOLEAN)
  PSet_Revit_Graphics | properties | on 5 objects (5 IFCSTAIR)
    Down arrow = FALSE (IFCBOOLEAN)
    Down label = FALSE (IFCBOOLEAN)
    Down text = "DN" (IFCLABEL)
    Show Up arrow in all views = FALSE (IFCBOOLEAN)
    Up arrow = FALSE (IFCBOOLEAN)
    Up label = FALSE (IFCBOOLEAN)
    Up text = "UP" (IFCLABEL)
  Pset_RailingCommon | properties | on 12 objects (12 IFCRAILING)
    Height = 975.0000000000001 (IFCREAL)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Railing:rekkverk_vinduer_type1_(1000mm)" (IFCIDENTIFIER)
  Pset_RailingCommon | properties | on 11 objects (11 IFCRAILING)
    Height = 900.0000000000001 (IFCREAL)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Railing:Rekkverk_hovedtrappe_lysning_990mm" (IFCIDENTIFIER)
  Pset_RailingCommon | properties | on 4 objects (4 IFCRAILING)
    Height = 900.0000000000001 (IFCREAL)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Railing:Håndliste_hovedtrappe" (IFCIDENTIFIER)
  Pset_RailingCommon | properties | on 4 objects (4 IFCRAILING)
    Height = 1175. (IFCREAL)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Railing:rekkverk_vinduer_type2_(1200mm)" (IFCIDENTIFIER)
  Pset_RailingCommon | properties | on 1 object (1 IFCRAILING)
    Height = 1000. (IFCREAL)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Railing:Rekkverk_hovedtrappe_repos_1000mm" (IFCIDENTIFIER)
  Pset_RailingCommon | properties | on 1 object (1 IFCRAILING)
    Height = 1000. (IFCREAL)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Railing:Rekkverk_hovedtrappe_lysning_1000mm" (IFCIDENTIFIER)
  Pset_DoorCommon | properties | on 75 objects (75 IFCDOOR)
    FireRating = "" (IFCLABEL)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Int_door_Aart:M9x21" (IFCIDENTIFIER)
  Pset_DoorCommon | properties | on 9 objects (9 IFCDOOR)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "Utv. dør_Leilighet:M10x21" (IFCIDENTIFIER)
  Pset_DoorCommon | properties | on 8 objects (8 IFCDOOR)
    FireRating = "EI 30 - S" (IFCLABEL)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Hoveddør_Leilighet:M10x21" (IFCIDENTIFIER)
  Pset_DoorCommon | properties | on 8 objects (8 IFCDOOR)
    FireRating = "" (IFCLABEL)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "DAN_Indv. Skydedør i væg:M9x21" (IFCIDENTIFIER)
  Pset_DoorCommon | properties | on 6 objects (6 IFCDOOR)
    FireRating = "" (IFCLABEL)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "DAN_Indv. Skydedør i væg:M11x21" (IFCIDENTIFIER)
  Pset_DoorCommon | properties | on 2 objects (2 IFCDOOR)
    FireRating = "" (IFCLABEL)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "DAN_Indv. Skydedør i væg:M 8x21" (IFCIDENTIFIER)
  Pset_DoorCommon | properties | on 1 object (1 IFCDOOR)
    FireRating = "" (IFCLABEL)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "234.18_H24 Nytt:2388 x 2288" (IFCIDENTIFIER)
  Pset_DoorCommon | properties | on 1 object (1 IFCDOOR)
    FireRating = "" (IFCLABEL)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Int_door_Aart:M8x21" (IFCIDENTIFIER)
  Pset_DoorCommon: 2 more contents on 2 objects not shown
  PSet_Revit_Other | properties | on 76 objects (76 IFCDOOR)
    Head Height = 2100. (IFCLENGTHMEASURE) [MILLI METRE]
    Material Frame = "(i2) - Træ (dørkarm)" (IFCLABEL)
    Material Handle = "(h9) - Metal (dørgreb)" (IFCLABEL)
    Material Panel = "(ie) - Træ (dørplade)" (IFCLABEL)
    Opening = 90. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Step = TRUE (IFCBOOLEAN)
  PSet_Revit_Other | properties | on 16 objects (16 IFCDOOR)
    Cavity Closure Depth To Ext = 130. (IFCLENGTHMEASURE) [MILLI METRE]
    Head Height = 2100. (IFCLENGTHMEASURE) [MILLI METRE]
    Opening = 90. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
  PSet_Revit_Other | properties | on 9 objects (9 IFCDOOR)
    Head Height = 2100. (IFCLENGTHMEASURE) [MILLI METRE]
    Lydkrav = "Rw + Ctr = 43dB" (IFCLABEL)
    Material Frame = "(i2) - Træ (dørkarm)" (IFCLABEL)
    Material Handle = "(h9) - Metal (dørgreb)" (IFCLABEL)
    Material Panel = "(ie) - Træ (dørplade)" (IFCLABEL)
    Opening = 90. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Orientering = "Sørøst" (IFCLABEL)
    Step = TRUE (IFCBOOLEAN)
  PSet_Revit_Other | properties | on 8 objects (8 IFCDOOR)
    Head Height = 2100. (IFCLENGTHMEASURE) [MILLI METRE]
    Lydkrav = "Rw + Ctr = 43dB" (IFCLABEL)
    Material Frame = "(i2) - Træ (dørkarm)" (IFCLABEL)
    Material Handle = "(h9) - Metal (dørgreb)" (IFCLABEL)
    Material Panel = "(ie) - Træ (dørplade)" (IFCLABEL)
    Opening = 90. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Step = TRUE (IFCBOOLEAN)
  PSet_Revit_Other | properties | on 5 objects (5 IFCWINDOW)
    Energikrav = "U-verdi 1.0 W/m²K" (IFCLABEL)
    Glasstype = "3-lags glass, Lt = 63, G = 37" (IFCLABEL)
    Lydkrav = "" (IFCLABEL)
    Orientering = "Nord" (IFCLABEL)
    Produsent = "Aluminiums fasadeparti" (IFCLABEL)
    Schedule Level = "00U" (IFCLABEL)
  PSet_Revit_Other | properties | on 4 objects (4 IFCWINDOW)
    Cavity Closure Depth To Ext = 249.9999999999858 (IFCLENGTHMEASURE) [MILLI METRE]
    Energikrav = "U-verdi 1.0 W/m²K" (IFCLABEL)
    Glasstype = "3-lags glass, Lt = 63, G = 37" (IFCLABEL)
    Head Height = 2288. (IFCLENGTHMEASURE) [MILLI METRE]
    Lydkrav = "32" (IFCLABEL)
    Lydkrav = "Rw + Ctr = 32dB" (IFCLABEL)
    Orientering = "Sør" (IFCLABEL)
    Produsent = "Tre- Alu vindu" (IFCLABEL)
    Utv. solavskjermning = "Mekanisk solavskjermning" (IFCLABEL)
  PSet_Revit_Other | properties | on 4 objects (4 IFCBUILDINGELEMENTPROXY)
    Schedule Level = "06" (IFCLABEL)
  PSet_Revit_Other | properties | on 4 objects (4 IFCWINDOW)
    Energikrav = "U-verdi 1.0 W/m²K" (IFCLABEL)
    Glasstype = "3-lags glass, Lt = 63, G = 37" (IFCLABEL)
    Lydkrav = "32" (IFCLABEL)
    Lydkrav = "Rw + Ctr = 32dB" (IFCLABEL)
    Orientering = "Nord" (IFCLABEL)
    Produsent = "Tre- Alu vindu" (IFCLABEL)
    Schedule Level = "01" (IFCLABEL)
  PSet_Revit_Other: 39 more contents on 58 objects not shown
  PSet_Revit_Text | properties | on 8 objects (8 IFCDOOR)
    Inngang = "21B" (IFCLABEL)
  PSet_Revit_Text | properties | on 7 objects (7 IFCDOOR)
    Inngang = "19" (IFCLABEL)
  PSet_Revit_Text | properties | on 2 objects (2 IFCDOOR)
    Inngang = "21A" (IFCLABEL)
  Pset_WindowCommon | properties | on 12 objects (12 IFCWINDOW)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "234.3_V_Udv._vindu_1fag(nytt):1188x1488 mm" (IFCIDENTIFIER)
  Pset_WindowCommon | properties | on 12 objects (12 IFCWINDOW)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "234.3_V_Udv._vindu_1fag_PAR:1188 x 1488mm" (IFCIDENTIFIER)
  Pset_WindowCommon | properties | on 6 objects (6 IFCWINDOW)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "234.3_H_Udv._vindu_1fag_PAR:1188 x 1488mm" (IFCIDENTIFIER)
  Pset_WindowCommon | properties | on 5 objects (5 IFCWINDOW)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "234.2_V_Udv._skyveparti_3fag Nytt:Skyveparti_2088x2288mm" (IFCIDENTIFIER)
  Pset_WindowCommon | properties | on 4 objects (4 IFCWINDOW)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "234.7_H_Udv._vindu_høyt_3fag_PAR:2988x2288mm" (IFCIDENTIFIER)
  Pset_WindowCommon | properties | on 4 objects (4 IFCWINDOW)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "234.7_V_Udv._vindu_høyt_3fag_PAR:2988x2288mm" (IFCIDENTIFIER)
  Pset_WindowCommon | properties | on 3 objects (3 IFCWINDOW)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "234.2_H_Udv._skyveparti_3fag Nytt:Skyveparti_2088x2288mm" (IFCIDENTIFIER)
  Pset_WindowCommon | properties | on 3 objects (3 IFCWINDOW)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "234.2_H_Udv._skyveparti_3fag Nytt:Skyveparti_2388x2288mm" (IFCIDENTIFIER)
  Pset_WindowCommon: 10 more contents on 14 objects not shown
  PSet_Revit_General | properties | on 26 objects (26 IFCWINDOW)
    Hængselside højre = FALSE (IFCBOOLEAN)
    Hængselside venstre = TRUE (IFCBOOLEAN)
  PSet_Revit_General | properties | on 11 objects (11 IFCWINDOW)
    Hængselside højre = TRUE (IFCBOOLEAN)
    Hængselside venstre = FALSE (IFCBOOLEAN)
  PSet_Revit_General | properties | on 5 objects (5 IFCWINDOW)
    Hængselside højre = TRUE (IFCBOOLEAN)
    Hængselside venstre = TRUE (IFCBOOLEAN)
  PSet_Revit_General | properties | on 2 objects (2 IFCWINDOW)
    Hængselside højre = TRUE (IFCBOOLEAN)
  PSet_Revit_General | properties | on 1 object (1 IFCWINDOW)
    Hængselside venstre = TRUE (IFCBOOLEAN)
  PSet_Revit_Materials and Finishes | properties | on 16 objects (16 IFCDOOR)
    Material Frame = "(i2) - Træ (dørkarm)" (IFCLABEL)
    Material Handle = "(h9) - Metal (dørgreb)" (IFCLABEL)
    Material Panel = "(i2) - Træ (dørplade)" (IFCLABEL)
  Pset_CurtainWallCommon | properties | on 8 objects (8 IFCCURTAINWALL)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "Curtain Wall:243.1_Indv_glasskillevæg" (IFCIDENTIFIER)
  Pset_CurtainWallCommon | properties | on 4 objects (4 IFCCURTAINWALL)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "Curtain Wall:243.2_Indv_glasskillevæg_ikke stiplet" (IFCIDENTIFIER)
  PSet_Revit_Vertical Grid Pattern | properties | on 12 objects (12 IFCCURTAINWALL)
    Angle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Justification = 4 (IFCINTEGER)
    Number = 4 (IFCINTEGER)
    Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  PSet_Revit_Horizontal Grid Pattern | properties | on 12 objects (12 IFCCURTAINWALL)
    Angle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Justification = 1 (IFCINTEGER)
    Number = 4 (IFCINTEGER)
    Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Pset_CoveringCommon | properties | on 81 objects (81 IFCCOVERING)
    Reference = "Compound Ceiling:KRAFT_61mm_Gips_ himling" (IFCIDENTIFIER)
    TotalThickness = 61.00000000000001 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_CoveringCommon | properties | on 3 objects (3 IFCCOVERING)
    Reference = "Compound Ceiling:kraft_Himling_Akustikkflåte" (IFCIDENTIFIER)
    TotalThickness = 40. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_CoveringCommon | properties | on 1 object (1 IFCCOVERING)
    Finish = "Gyproc Gipsplade_2560mm;" (IFCLABEL)
    Reference = "Compound Ceiling:KRAFT_61mm_Gips_ himling" (IFCIDENTIFIER)
    TotalThickness = 61.00000000000001 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  PSet_Revit_Visibility | properties | on 32 objects (32 IFCWINDOW)
    Opening 3D = TRUE (IFCBOOLEAN)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    NumberOfStoreys = 9 (IFCINTEGER)
  PSet_Revit_Type_Graphics | properties | on 544 objects (387 IFCWALLSTANDARDCASE, 81 IFCSLAB, 57 IFCOPENINGELEMENT, 16 IFCWALL)
    Coarse Scale Fill Color = 0 (IFCINTEGER)
  PSet_Revit_Type_Graphics | properties | on 82 objects (82 IFCCOVERING)
    Coarse Scale Fill Color = 12632256 (IFCINTEGER)
    Coarse Scale Fill Pattern = "Loft_type1" (IFCLABEL)
  PSet_Revit_Type_Graphics | properties | on 9 objects (9 IFCBUILDINGSTOREY)
    Color = 0 (IFCINTEGER)
    Line Pattern = "Dash dot" (IFCLABEL)
    Line Weight = 1 (IFCINTEGER)
    Symbol = "Level_Aart" (IFCLABEL)
    Symbol at End 1 Default = TRUE (IFCBOOLEAN)
    Symbol at End 2 Default = FALSE (IFCBOOLEAN)
  PSet_Revit_Type_Graphics | properties | on 5 objects (5 IFCSTAIR)
    Break Symbol in Plan = FALSE (IFCBOOLEAN)
    Text Font = "Arial" (IFCLABEL)
    Text Size = 0.008202099737532808 (IFCREAL)
  PSet_Revit_Type_Graphics | properties | on 3 objects (3 IFCCOVERING)
    Coarse Scale Fill Color = 12632256 (IFCINTEGER)
    Coarse Scale Fill Pattern = "Fliser" (IFCLABEL)
  PSet_Revit_Type_Identity Data | properties | on 152 objects (151 IFCWALLSTANDARDCASE, 1 IFCOPENINGELEMENT)
    Assembly Code = "" (IFCLABEL)
    Assembly Description = "" (IFCLABEL)
    Description = "" (IFCLABEL)
    Edited by = "" (IFCLABEL)
    Type Mark = "Type 1.1" (IFCLABEL)
    Workset = 14 (IFCINTEGER)
  PSet_Revit_Type_Identity Data | properties | on 107 objects (107 IFCWALLSTANDARDCASE)
    Assembly Code = "" (IFCLABEL)
    Assembly Description = "" (IFCLABEL)
    Description = "" (IFCLABEL)
    Edited by = "" (IFCLABEL)
    Type Mark = "Type 3.1" (IFCLABEL)
    Workset = 14 (IFCINTEGER)
  PSet_Revit_Type_Identity Data | properties | on 82 objects (82 IFCCOVERING)
    Assembly Code = "" (IFCLABEL)
    Assembly Description = "" (IFCLABEL)
    Edited by = "" (IFCLABEL)
    Type Mark = "257.01" (IFCLABEL)
    Workset = 18 (IFCINTEGER)
  PSet_Revit_Type_Identity Data | properties | on 75 objects (75 IFCDOOR)
    Assembly Code = "" (IFCLABEL)
    Assembly Description = "" (IFCLABEL)
    Edited by = "" (IFCLABEL)
    OmniClass Number = "" (IFCLABEL)
    OmniClass Title = "" (IFCLABEL)
    Type Mark = "244.09" (IFCLABEL)
    Workset = 33772 (IFCINTEGER)
  PSet_Revit_Type_Identity Data | properties | on 68 objects (68 IFCBUILDINGELEMENTPROXY)
    Assembly Code = "" (IFCLABEL)
    Assembly Description = "" (IFCLABEL)
    Edited by = "" (IFCLABEL)
    OmniClass Number = "" (IFCLABEL)
    OmniClass Title = "" (IFCLABEL)
    Type Mark = "" (IFCLABEL)
    Workset = 68576 (IFCINTEGER)
  PSet_Revit_Type_Identity Data | properties | on 52 objects (47 IFCWALLSTANDARDCASE, 5 IFCWALL)
    Assembly Code = "" (IFCLABEL)
    Assembly Description = "" (IFCLABEL)
    Description = "" (IFCLABEL)
    Edited by = "" (IFCLABEL)
    Type Mark = "Type 2.1" (IFCLABEL)
    Workset = 14 (IFCINTEGER)
  PSet_Revit_Type_Identity Data | properties | on 46 objects (46 IFCBUILDINGELEMENTPROXY)
    Assembly Code = "" (IFCLABEL)
    Assembly Description = "" (IFCLABEL)
    Edited by = "" (IFCLABEL)
    OmniClass Number = "" (IFCLABEL)
    OmniClass Title = "" (IFCLABEL)
    Workset = 68603 (IFCINTEGER)
  PSet_Revit_Type_Identity Data | properties | on 45 objects (39 IFCOPENINGELEMENT, 6 IFCSLAB)
    Assembly Code = "" (IFCLABEL)
    Assembly Description = "" (IFCLABEL)
    Edited by = "" (IFCLABEL)
    Type Mark = "253.1" (IFCLABEL)
    Workset = 17 (IFCINTEGER)
  PSet_Revit_Type_Identity Data: 59 more contents on 372 objects not shown
  PSet_Revit_Type_Constraints | properties | on 32 objects (32 IFCWINDOW)
    Centralized transom = TRUE (IFCBOOLEAN)
    Default Elevation = 800. (IFCLENGTHMEASURE) [MILLI METRE]
  PSet_Revit_Type_Constraints | properties | on 12 objects (12 IFCPLATE)
    Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  PSet_Revit_Type_Constraints | properties | on 9 objects (9 IFCBUILDINGSTOREY)
    Elevation Base = 1 (IFCINTEGER)
  PSet_Revit_Type_Constraints | properties | on 4 objects (4 IFCBUILDINGELEMENTPROXY)
    Default Elevation = 1219.2 (IFCLENGTHMEASURE) [MILLI METRE]
  PSet_Revit_Type_Construction | properties | on 152 objects (151 IFCWALLSTANDARDCASE, 1 IFCOPENINGELEMENT)
    Function = 0 (IFCINTEGER)
    Width = 124. (IFCLENGTHMEASURE) [MILLI METRE]
    Wrapping at Ends = 0 (IFCINTEGER)
    Wrapping at Inserts = 0 (IFCINTEGER)
  PSet_Revit_Type_Construction | properties | on 107 objects (107 IFCWALLSTANDARDCASE)
    Function = 0 (IFCINTEGER)
    Width = 111. (IFCLENGTHMEASURE) [MILLI METRE]
    Wrapping at Ends = 0 (IFCINTEGER)
    Wrapping at Inserts = 0 (IFCINTEGER)
  PSet_Revit_Type_Construction | properties | on 82 objects (82 IFCCOVERING)
    Thickness = 61.00000000000001 (IFCLENGTHMEASURE) [MILLI METRE]
  PSet_Revit_Type_Construction | properties | on 76 objects (76 IFCDOOR)
    Function = 0 (IFCINTEGER)
    Wall Closure = 1 (IFCINTEGER)
  PSet_Revit_Type_Construction | properties | on 52 objects (47 IFCWALLSTANDARDCASE, 5 IFCWALL)
    Function = 0 (IFCINTEGER)
    Width = 147. (IFCLENGTHMEASURE) [MILLI METRE]
    Wrapping at Ends = 0 (IFCINTEGER)
    Wrapping at Inserts = 0 (IFCINTEGER)
  PSet_Revit_Type_Construction | properties | on 46 objects (39 IFCOPENINGELEMENT, 7 IFCSLAB)
    Default Thickness = 250. (IFCLENGTHMEASURE) [MILLI METRE]
    Function = 0 (IFCINTEGER)
  PSet_Revit_Type_Construction | properties | on 31 objects (31 IFCWINDOW)
    Wall Closure = 0 (IFCINTEGER)
  PSet_Revit_Type_Construction | properties | on 24 objects (24 IFCSLAB)
    Default Thickness = 112. (IFCLENGTHMEASURE) [MILLI METRE]
    Function = 0 (IFCINTEGER)
  PSet_Revit_Type_Construction: 34 more contents on 252 objects not shown
  PSet_Revit_Type_Other | properties | on 75 objects (75 IFCDOOR)
    Area = 1911000. (IFCAREAMEASURE) [MILLI SQUARE_METRE]
    Areal = 1911000. (IFCAREAMEASURE) [MILLI SQUARE_METRE]
    Frame Width = 40. (IFCLENGTHMEASURE) [MILLI METRE]
    Handel Distance From Floor = 1000. (IFCLENGTHMEASURE) [MILLI METRE]
    Height Door = 2088. (IFCLENGTHMEASURE) [MILLI METRE]
    Joint = 12. (IFCLENGTHMEASURE) [MILLI METRE]
    Panel Length = 806.0000000000002 (IFCLENGTHMEASURE) [MILLI METRE]
    Panel Width = 40. (IFCLENGTHMEASURE) [MILLI METRE]
    Width Door = 886.0000000000001 (IFCLENGTHMEASURE) [MILLI METRE]
  PSet_Revit_Type_Other | properties | on 18 objects (18 IFCWINDOW)
    Areal = 1767744. (IFCAREAMEASURE) [MILLI SQUARE_METRE]
    FLP = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Sash height = 1388. (IFCLENGTHMEASURE) [MILLI METRE]
    Sash width = 1088. (IFCLENGTHMEASURE) [MILLI METRE]
  PSet_Revit_Type_Other | properties | on 16 objects (16 IFCDOOR)
    Handel Distance From Floor = 1080. (IFCLENGTHMEASURE) [MILLI METRE]
    Structural Tolerance = 12. (IFCLENGTHMEASURE) [MILLI METRE]
  PSet_Revit_Type_Other | properties | on 12 objects (12 IFCWINDOW)
    Areal = 1767744. (IFCAREAMEASURE) [MILLI SQUARE_METRE]
  PSet_Revit_Type_Other | properties | on 9 objects (9 IFCDOOR)
    Area = 2121000. (IFCAREAMEASURE) [MILLI SQUARE_METRE]
    Areal = 2121000. (IFCAREAMEASURE) [MILLI SQUARE_METRE]
    Frame Width = 40. (IFCLENGTHMEASURE) [MILLI METRE]
    Handel Distance From Floor = 1000. (IFCLENGTHMEASURE) [MILLI METRE]
    Height Door = 2088. (IFCLENGTHMEASURE) [MILLI METRE]
    Joint = 12. (IFCLENGTHMEASURE) [MILLI METRE]
    Panel Length = 906. (IFCLENGTHMEASURE) [MILLI METRE]
    Panel Width = 40. (IFCLENGTHMEASURE) [MILLI METRE]
    Width Door = 986. (IFCLENGTHMEASURE) [MILLI METRE]
  PSet_Revit_Type_Other | properties | on 8 objects (8 IFCDOOR)
    Frame Width = 40. (IFCLENGTHMEASURE) [MILLI METRE]
    Handel Distance From Floor = 1000. (IFCLENGTHMEASURE) [MILLI METRE]
    Height Door = 2088. (IFCLENGTHMEASURE) [MILLI METRE]
    Joint = 12. (IFCLENGTHMEASURE) [MILLI METRE]
    Panel Length = 906. (IFCLENGTHMEASURE) [MILLI METRE]
    Panel Width = 40. (IFCLENGTHMEASURE) [MILLI METRE]
    Width Door = 986. (IFCLENGTHMEASURE) [MILLI METRE]
  PSet_Revit_Type_Other | properties | on 8 objects (8 IFCWINDOW)
    Areal = 4777344.000000001 (IFCAREAMEASURE) [MILLI SQUARE_METRE]
    Arrow Pos 2 = 340. (IFCLENGTHMEASURE) [MILLI METRE]
    Arrow Position = 562.9999999999874 (IFCLENGTHMEASURE) [MILLI METRE]
    Ext Frame Thickness inc. 10 mm fuge = 75. (IFCLENGTHMEASURE) [MILLI METRE]
    Int Frame Thickness = 120. (IFCLENGTHMEASURE) [MILLI METRE]
    Int Frame Width = 85. (IFCLENGTHMEASURE) [MILLI METRE]
    Last Dr Offset = 370. (IFCLENGTHMEASURE) [MILLI METRE]
    No of Panels = 3 (IFCINTEGER)
    Offset Ext = 200. (IFCLENGTHMEASURE) [MILLI METRE]
    Panel Height = 2234.999999999999 (IFCLENGTHMEASURE) [MILLI METRE]
    Panel Width = 726. (IFCLENGTHMEASURE) [MILLI METRE]
    Track Depth = 10.00000000000172 (IFCLENGTHMEASURE) [MILLI METRE]
  PSet_Revit_Type_Other | properties | on 8 objects (8 IFCWINDOW)
    Areal = 6836544. (IFCAREAMEASURE) [MILLI SQUARE_METRE]
    FLP = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Sash H = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Sash W = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  PSet_Revit_Type_Other: 11 more contents on 21 objects not shown
  PSet_Revit_Type_Dimensions | properties | on 75 objects (75 IFCDOOR)
    Height = 2100. (IFCLENGTHMEASURE) [MILLI METRE]
    Rough Height = 910.0000000000001 (IFCLENGTHMEASURE) [MILLI METRE]
    Rough Width = 2100. (IFCLENGTHMEASURE) [MILLI METRE]
    Width = 910.0000000000001 (IFCLENGTHMEASURE) [MILLI METRE]
  PSet_Revit_Type_Dimensions | properties | on 68 objects (68 IFCBUILDINGELEMENTPROXY)
    a = 26.49999999999999 (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    insert = 112. (IFCLENGTHMEASURE) [MILLI METRE]
    joint = 16. (IFCLENGTHMEASURE) [MILLI METRE]
    klip over = 29.99999999999958 (IFCLENGTHMEASURE) [MILLI METRE]
  PSet_Revit_Type_Dimensions | properties | on 46 objects (46 IFCBUILDINGELEMENTPROXY)
    Fuge - Skrå snit = 16. (IFCLENGTHMEASURE) [MILLI METRE]
    a = 26.4999999999999 (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    h = 76.77589407244152 (IFCLENGTHMEASURE) [MILLI METRE]
    insert = 130. (IFCLENGTHMEASURE) [MILLI METRE]
    joint = 16. (IFCLENGTHMEASURE) [MILLI METRE]
    klip over = 29.99999999999958 (IFCLENGTHMEASURE) [MILLI METRE]
  PSet_Revit_Type_Dimensions | properties | on 18 objects (18 IFCWINDOW)
    Frame depth = 150. (IFCLENGTHMEASURE) [MILLI METRE]
    Frame width = 49.99999999999994 (IFCLENGTHMEASURE) [MILLI METRE]
    Fuge = 16. (IFCLENGTHMEASURE) [MILLI METRE]
    Glass depth = 20.00000000000002 (IFCLENGTHMEASURE) [MILLI METRE]
    Glass thickness = 24. (IFCLENGTHMEASURE) [MILLI METRE]
    Height = 1488. (IFCLENGTHMEASURE) [MILLI METRE]
    Rough Height = 1520. (IFCLENGTHMEASURE) [MILLI METRE]
    Rough Width = 1220. (IFCLENGTHMEASURE) [MILLI METRE]
    Width = 1188. (IFCLENGTHMEASURE) [MILLI METRE]
  PSet_Revit_Type_Dimensions | properties | on 17 objects (17 IFCDOOR)
    Height = 2100. (IFCLENGTHMEASURE) [MILLI METRE]
    Width = 1010. (IFCLENGTHMEASURE) [MILLI METRE]
  PSet_Revit_Type_Dimensions | properties | on 12 objects (12 IFCPLATE)
    Thickness = 25. (IFCLENGTHMEASURE) [MILLI METRE]
  PSet_Revit_Type_Dimensions | properties | on 12 objects (12 IFCWINDOW)
    Default Sill Height = 800. (IFCLENGTHMEASURE) [MILLI METRE]
    Fuge = 16. (IFCLENGTHMEASURE) [MILLI METRE]
    Height = 1488. (IFCLENGTHMEASURE) [MILLI METRE]
    Karmdybde = 100. (IFCLENGTHMEASURE) [MILLI METRE]
    Rough Height = 1520. (IFCLENGTHMEASURE) [MILLI METRE]
    Rough Width = 1220. (IFCLENGTHMEASURE) [MILLI METRE]
    Width = 1188. (IFCLENGTHMEASURE) [MILLI METRE]
    openingline = 1034. (IFCLENGTHMEASURE) [MILLI METRE]
  PSet_Revit_Type_Dimensions | properties | on 8 objects (8 IFCDOOR)
    Door panel width = 40. (IFCLENGTHMEASURE) [MILLI METRE]
    Frame Width = 54. (IFCLENGTHMEASURE) [MILLI METRE]
    Height = 2100. (IFCLENGTHMEASURE) [MILLI METRE]
    Height Door = 2100. (IFCLENGTHMEASURE) [MILLI METRE]
    Panel Length = 802.0000000000001 (IFCLENGTHMEASURE) [MILLI METRE]
    Rough Height = 2112. (IFCLENGTHMEASURE) [MILLI METRE]
    Rough Width = 934. (IFCLENGTHMEASURE) [MILLI METRE]
    Thickness = 2101. (IFCLENGTHMEASURE) [MILLI METRE]
    Width = 910.0000000000001 (IFCLENGTHMEASURE) [MILLI METRE]
  PSet_Revit_Type_Dimensions: 16 more contents on 49 objects not shown
  PSet_Revit_Type_Treads | properties | on 3 objects (3 IFCSTAIR)
    Apply Nosing Profile = 0 (IFCINTEGER)
    Minimum Tread Depth = 280. (IFCLENGTHMEASURE) [MILLI METRE]
    Nosing Length = 15. (IFCLENGTHMEASURE) [MILLI METRE]
    Tread Thickness = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  PSet_Revit_Type_Treads | properties | on 1 object (1 IFCSTAIR)
    Apply Nosing Profile = 0 (IFCINTEGER)
    Minimum Tread Depth = 250. (IFCLENGTHMEASURE) [MILLI METRE]
    Nosing Length = 30. (IFCLENGTHMEASURE) [MILLI METRE]
    Tread Thickness = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  PSet_Revit_Type_Treads | properties | on 1 object (1 IFCSTAIR)
    Apply Nosing Profile = 0 (IFCINTEGER)
    Minimum Tread Depth = 250. (IFCLENGTHMEASURE) [MILLI METRE]
    Nosing Length = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Tread Thickness = 30. (IFCLENGTHMEASURE) [MILLI METRE]
  PSet_Revit_Type_Risers | properties | on 3 objects (3 IFCSTAIR)
    Begin with Riser = FALSE (IFCBOOLEAN)
    End with Riser = FALSE (IFCBOOLEAN)
    Maximum Riser Height = 190. (IFCLENGTHMEASURE) [MILLI METRE]
    Riser Thickness = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Riser Type = 2 (IFCINTEGER)
    Riser to Tread Connection = 1 (IFCINTEGER)
  PSet_Revit_Type_Risers | properties | on 1 object (1 IFCSTAIR)
    Begin with Riser = TRUE (IFCBOOLEAN)
    End with Riser = FALSE (IFCBOOLEAN)
    Maximum Riser Height = 180. (IFCLENGTHMEASURE) [MILLI METRE]
    Riser Thickness = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Riser Type = 2 (IFCINTEGER)
    Riser to Tread Connection = 1 (IFCINTEGER)
  PSet_Revit_Type_Risers | properties | on 1 object (1 IFCSTAIR)
    Begin with Riser = TRUE (IFCBOOLEAN)
    End with Riser = FALSE (IFCBOOLEAN)
    Maximum Riser Height = 250. (IFCLENGTHMEASURE) [MILLI METRE]
    Riser Thickness = 30. (IFCLENGTHMEASURE) [MILLI METRE]
    Riser Type = 0 (IFCINTEGER)
    Riser to Tread Connection = 1 (IFCINTEGER)
  PSet_Revit_Type_Stringers | properties | on 4 objects (4 IFCSTAIR)
    Landing Carriage Height = 200. (IFCLENGTHMEASURE) [MILLI METRE]
    Left Stringer = 1 (IFCINTEGER)
    Middle Stringers = 0 (IFCINTEGER)
    Open Stringer Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Right Stringer = 1 (IFCINTEGER)
    Stringer Carriage Height = 150. (IFCLENGTHMEASURE) [MILLI METRE]
    Stringer Height = 400. (IFCLENGTHMEASURE) [MILLI METRE]
    Stringer Thickness = 50. (IFCLENGTHMEASURE) [MILLI METRE]
    Trim Stringers at Top = 1 (IFCINTEGER)
  PSet_Revit_Type_Stringers | properties | on 1 object (1 IFCSTAIR)
    Landing Carriage Height = 200. (IFCLENGTHMEASURE) [MILLI METRE]
    Left Stringer = 1 (IFCINTEGER)
    Middle Stringers = 0 (IFCINTEGER)
    Open Stringer Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Right Stringer = 1 (IFCINTEGER)
    Stringer Carriage Height = 35. (IFCLENGTHMEASURE) [MILLI METRE]
    Stringer Height = 250. (IFCLENGTHMEASURE) [MILLI METRE]
    Stringer Thickness = 50. (IFCLENGTHMEASURE) [MILLI METRE]
    Trim Stringers at Top = 1 (IFCINTEGER)
  PSet_Revit_Type_Materials and Finishes | properties | on 114 objects (114 IFCBUILDINGELEMENTPROXY)
    Materiale = "Metal - Aluminum" (IFCLABEL)
  PSet_Revit_Type_Materials and Finishes | properties | on 32 objects (32 IFCWINDOW)
    Frame = "Aluminium Vinduer" (IFCLABEL)
    Glass = "Glass" (IFCLABEL)
  PSet_Revit_Type_Materials and Finishes | properties | on 12 objects (12 IFCPLATE)
    Material = "Glass" (IFCLABEL)
  PSet_Revit_Type_Materials and Finishes | properties | on 4 objects (4 IFCBUILDINGELEMENTPROXY)
    Beslag = "Beslag" (IFCLABEL)
  PSet_Revit_Type_Materials and Finishes | properties | on 3 objects (3 IFCSTAIR)
    Monolithic Material = "Aart_beton" (IFCLABEL)
    Riser Material = "Aart_beton" (IFCLABEL)
    Tread Material = "Aart_beton" (IFCLABEL)
  PSet_Revit_Type_Materials and Finishes | properties | on 2 objects (2 IFCSTAIR)
    Monolithic Material = "Aart_beton" (IFCLABEL)
  PSet_Revit_Type_Vertical Grid Pattern | properties | on 12 objects (12 IFCCURTAINWALL)
    Adjust for Mullion Size = FALSE (IFCBOOLEAN)
    Layout = 0 (IFCINTEGER)
  PSet_Revit_Type_Horizontal Grid Pattern | properties | on 12 objects (12 IFCCURTAINWALL)
    Adjust for Mullion Size = FALSE (IFCBOOLEAN)
    Layout = 0 (IFCINTEGER)
  PSet_Revit_Type_General | properties | on 114 objects (114 IFCBUILDINGELEMENTPROXY)
    Lodret = TRUE (IFCBOOLEAN)
    Skrå = FALSE (IFCBOOLEAN)
  PSet_Revit_Type_Visibility | properties | on 18 objects (18 IFCWINDOW)
    Bottom hung = TRUE (IFCBOOLEAN)
    Left hung = FALSE (IFCBOOLEAN)
    Right hung = TRUE (IFCBOOLEAN)
    Topp hung = FALSE (IFCBOOLEAN)
  PSet_Revit_Type_Visibility | properties | on 16 objects (16 IFCDOOR)
    Gerigter = FALSE (IFCBOOLEAN)
  PSet_Revit_Type_Visibility | properties | on 5 objects (5 IFCWINDOW)
    Bottom hung = FALSE (IFCBOOLEAN)
    Left hung = FALSE (IFCBOOLEAN)
    Right hung = TRUE (IFCBOOLEAN)
    Top hung = TRUE (IFCBOOLEAN)
  PSet_Revit_Type_Visibility | properties | on 5 objects (5 IFCWINDOW)
    Bottom hung = TRUE (IFCBOOLEAN)
    Left hung = TRUE (IFCBOOLEAN)
    Right hung = FALSE (IFCBOOLEAN)
    Topp hung = FALSE (IFCBOOLEAN)
  PSet_Revit_Type_Visibility | properties | on 4 objects (4 IFCWINDOW)
    Bottom hung = FALSE (IFCBOOLEAN)
    Left hung = TRUE (IFCBOOLEAN)
    Right hung = FALSE (IFCBOOLEAN)
    Top hung = TRUE (IFCBOOLEAN)
  234.25_H_Udv._vindu_1fag_PAR:4188x2088:4188x2088:21880914 | predefined | on 1 type object
  234.25_F_Udv._vindu_1fag_PAR_us:2688x2088:2688x2088:21880919 | predefined | on 1 type object
  234.25_H_Udv._vindu_1fag_PAR:3888x2088:3888x2088:21880929 | predefined | on 1 type object
  234.18_H24-:2388 x 2488 (næring):2388 x 2488 (næring):21880930 | predefined | on 1 type object
  234.18_V24_Næring:2388 x 2488 (næring):2388 x 2488 (næring):21880939 | predefined | on 1 type object
  234.25_H_Udv._vindu_1fag_PAR:2988x2088:2988x2088:21880943 | predefined | on 1 type object
  Hoveddør_Leilighet:M10x21:M10x21:1517569 | predefined | on 1 type object
  Int_door_Aart:M9x21:M9x21:3628180 | predefined | on 1 type object
  Int_door_Aart:M9x21:M9x21:3628187 | predefined | on 1 type object
  Int_door_Aart:M9x21:M9x21:3628223 | predefined | on 1 type object
  DAN_Indv. Skydedør i væg:M9x21:M9x21:3628231 | predefined | on 1 type object
  Int_door_Aart:M9x21:M9x21:3628242 | predefined | on 1 type object
  DAN_Indv. Skydedør i væg:M9x21:M9x21:3628243 | predefined | on 1 type object
  Utv. dør_Leilighet:M10x21:M10x21:1689354 | predefined | on 1 type object
  Utv. dør_Leilighet:M10x21:M10x21:2992344 | predefined | on 1 type object
  Hoveddør_Leilighet:M10x21:M10x21:3026092 | predefined | on 1 type object
  234.2_V_Udv._skyveparti_3fag Nytt:Skyveparti_2088x2288mm:Skyveparti_2088x2288mm:10991077 | predefined | on 1 type object
  234.3_V_Udv._vindu_1fag(nytt):1188x1488 mm:1188x1488 mm:2374111 | predefined | on 1 type object
  234.18_H24 Nytt:2388 x 2288:2388 x 2288:14707761 | predefined | on 1 type object
  DAN_Indv. Skydedør i væg:M11x21:M11x21:19561768 | predefined | on 1 type object
  DAN_Indv. Skydedør i væg:M11x21:M11x21:19562058 | predefined | on 1 type object
  234.3_V_Udv._vindu_1fag_PAR:1188 x 1488mm:1188 x 1488mm:20287888 | predefined | on 1 type object
  DAN_Indv. Skydedør i væg:M9x21:M9x21:20697993 | predefined | on 1 type object
  Int_door_Aart:M8x21:M8x21:20698194 | predefined | on 1 type object
  234.7_H_Udv._vindu_høyt_3fag_PAR:2988x2288mm:2988x2288mm:21170239 | predefined | on 1 type object
  234.3_H_Udv._vindu_1fag_PAR:1188 x 1488mm:1188 x 1488mm:21170258 | predefined | on 1 type object
  234.7_V_Udv._vindu_høyt_3fag_PAR:2988x2288mm:2988x2288mm:21182210 | predefined | on 1 type object
  234.2_V_Udv._skyveparti_3fag Nytt:Skyveparti_2688x2288mm:Skyveparti_2688x2288mm:21188430 | predefined | on 1 type object
  234.2_V_Udv._skyveparti_3fag Nytt:Skyveparti_2388x2288mm:Skyveparti_2388x2288mm:17533459 | predefined | on 1 type object
  234.2_H_Udv._skyveparti_3fag Nytt:Skyveparti_2088x2288mm:Skyveparti_2088x2288mm:3508597 | predefined | on 1 type object
  234.4_V_Udv._vindu_2fag Nytt:2388x1488 mm:2388x1488 mm:14707764 | predefined | on 1 type object
  234.2_H_Udv._skyveparti_3fag Nytt:Skyveparti_2388x2288mm:Skyveparti_2388x2288mm:17530858 | predefined | on 1 type object
  234.7_V_Udv._vindu_høyt_3fag_PAR:2988x2288mm:2988x2288mm:21170260 | predefined | on 1 type object
  234.3_H_Udv._vindu_1fag_PAR:1188 x 1488mm:1188 x 1488mm:21173899 | predefined | on 1 type object
  234.2_H_Udv._skyveparti_3fag Nytt:Skyveparti_2688x2288mm:Skyveparti_2688x2288mm:17533462 | predefined | on 1 type object
  DAN_Indv. Skydedør i væg:M9x21:M9x21:9093941 | predefined | on 1 type object
  DAN_Indv. Skydedør i væg:M9x21:M9x21:9093948 | predefined | on 1 type object
  DAN_Indv. Skydedør i væg:M11x21:M11x21:19562932 | predefined | on 1 type object
  234.2_V_Udv._skyveparti_3fag Nytt:Skyveparti_2688x2288mm:Skyveparti_2688x2288mm:4731875 | predefined | on 1 type object
  DAN_Indv. Skydedør i væg:M9x21:M9x21:19563436 | predefined | on 1 type object
  234.7_H_Udv._vindu_høyt_3fag_PAR:2688x2288mm:2688x2288mm:21182861 | predefined | on 1 type object
  DAN_Indv. Skydedør i væg:M 8x21:M 8x21:19566036 | predefined | on 1 type object
  DAN_Indv. Skydedør i væg:M 8x21:M 8x21:19566087 | predefined | on 1 type object
  234.3_H_Udv._vindu_1fag_PAR:1188 x 1488mm:1188 x 1488mm:20288139 | predefined | on 1 type object