IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView]"
File name: "20672_RIB_Vannkanten_B9.ifc"
Time stamp: "2014-05-22T11:34:12"
Preprocessor: "Autodesk Revit 2013"
Originating system: "20130531_2115(x64) - Exporter 2.15.1.0 - Default UI"
Application: "Autodesk Revit 2013 (ENU)" version "2013" identifier "Revit" by Organization "Autodesk Revit 2013 (ENU)"

People and organizations
  Person "Gábor" "Schnierer" of Organization "CEOS Ltd."
  Owner history of Person "Gábor" "Schnierer" of Organization "CEOS Ltd." | application "Autodesk Revit 2013 (ENU)" version "2013" identifier "Revit" by Organization "Autodesk Revit 2013 (ENU)" | change NOCHANGE | created 1400580827 (2014-05-20T10:13:47Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: MILLI SQUARE_METRE
  VOLUMEUNIT: MILLI CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: KELVIN
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  PRESSUREUNIT: PASCAL

Spatial structure
IFCPROJECT "20672" | long name "1103_54_1060" | phase "Project Status"
  IFCSITE "Default" | latitude 42° 21′ 30.344238″ | longitude -71° 3′ 35.194702″ | elevation above sea level -1.08286712929839E-12
    IFCBUILDING "Bygg 9" | long name "Bygg 9" | postal address: "1103_54_1060", "1103_54_1060"
      IFCBUILDINGSTOREY "00U" | long name "00U" | elevation 1900.
        contains 2 elements
          1 x IFCBUILDINGELEMENTPROXY | object type "OrientationCube" | names: "OrientationCube:OrientationCube:380126" | property sets: Pset_BuildingElementProxyCommon, Constraints, Phasing, Dimensions, Identity Data
          1 x IFCBUILDINGELEMENTPROXY | object type "Stairs T3" | names: "Stairs T3:Stairs T3:182194" | material: "Concrete, Precast" | property sets: Pset_BuildingElementProxyCommon, Constraints, Dimensions, Identity Data, Materials and Finishes, Other
      IFCBUILDINGSTOREY "01" | long name "01" | elevation 5590.
        contains 24 elements
          4 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:RC Wall 220 mm" | object type "Basic Wall:RC Wall 220 mm:4537" | names: "Basic Wall:RC Wall 220 mm:25497", "Basic Wall:RC Wall 220 mm:25510", "Basic Wall:RC Wall 220 mm:27733" (+1 more) | material: layers "Basic Wall:RC Wall 220 mm" ("Concrete, Cast-in-Place gray" 220.) | property sets: Constraints, Dimensions, Identity Data, Phasing, Structural, Pset_WallCommon
          5 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:RC Wall 250 mm" | object type "Basic Wall:RC Wall 250 mm:4536" | names: "Basic Wall:RC Wall 250 mm:25614", "Basic Wall:RC Wall 250 mm:25636", "Basic Wall:RC Wall 250 mm:25726" (+2 more) | material: layers "Basic Wall:RC Wall 250 mm" ("Concrete, Cast-in-Place gray" 250.) | property sets: Constraints, Dimensions, Identity Data, Phasing, Structural, Pset_WallCommon
          1 x IFCSLAB | object type "Floor:RC Floor - 250 mm" | FLOOR | names: "Floor:RC Floor - 250 mm:26841" | material: "Concrete, Cast-in-Place gray" | property sets: Pset_SlabCommon, Constraints, Dimensions, Phasing, Structural, Analytical Properties
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:RC Wall 200 mm" | object type "Basic Wall:RC Wall 200 mm:4535" | names: "Basic Wall:RC Wall 200 mm:131001" | material: layers "Basic Wall:RC Wall 200 mm" ("Concrete, Cast-in-Place gray" 200.) | property sets: Constraints, Dimensions, Identity Data, Phasing, Structural, Pset_WallCommon
          1 x IFCSLAB | object type "Floor:RC Floor - 200 mm" | FLOOR | names: "Floor:RC Floor - 200 mm:150169" | material: layers "Floor:RC Floor - 200 mm" ("Concrete, Cast-in-Place gray" 200.) | property sets: Pset_SlabCommon, Constraints, Dimensions, Identity Data, Phasing, Structural
          1 x IFCELEMENTASSEMBLY | object type "Structural Columns Assembly:B9-ST24" | USERDEFINED | names: "Structural Columns Assembly:B9-ST24:350643" | parts: 1 IFCCOLUMN | property sets: Identity Data, Phasing
          3 x IFCELEMENTASSEMBLY | object type "Structural Columns Assembly:B9-ST04" | USERDEFINED | names: "Structural Columns Assembly:B9-ST04:516628", "Structural Columns Assembly:B9-ST04:517153", "Structural Columns Assembly:B9-ST04:569557" | parts: 3 IFCBUILDINGELEMENTPROXY, 3 IFCCOLUMN | property sets: Identity Data, Phasing
          1 x IFCELEMENTASSEMBLY | object type "Structural Columns Assembly:B9-ST05" | USERDEFINED | names: "Structural Columns Assembly:B9-ST05:518407" | parts: 1 IFCBUILDINGELEMENTPROXY, 1 IFCCOLUMN | property sets: Identity Data, Phasing
          3 x IFCELEMENTASSEMBLY | object type "Structural Columns Assembly:B9-ST22" | USERDEFINED | names: "Structural Columns Assembly:B9-ST22:519489", "Structural Columns Assembly:B9-ST22:520124", "Structural Columns Assembly:B9-ST22:520386" | parts: 3 IFCBUILDINGELEMENTPROXY, 3 IFCCOLUMN | property sets: Identity Data, Phasing
          1 x IFCELEMENTASSEMBLY | object type "Structural Columns Assembly:B9-ST23" | USERDEFINED | names: "Structural Columns Assembly:B9-ST23:521485" | parts: 1 IFCBUILDINGELEMENTPROXY, 1 IFCCOLUMN | property sets: Identity Data, Phasing
          1 x IFCELEMENTASSEMBLY | object type "Structural Columns Assembly:B9-ST07" | USERDEFINED | names: "Structural Columns Assembly:B9-ST07:522353" | parts: 1 IFCBUILDINGELEMENTPROXY, 1 IFCCOLUMN | property sets: Identity Data, Phasing
          2 x IFCELEMENTASSEMBLY | object type "Structural Columns Assembly:B9-ST03" | USERDEFINED | names: "Structural Columns Assembly:B9-ST03:522455", "Structural Columns Assembly:B9-ST03:522552" | parts: 2 IFCBUILDINGELEMENTPROXY, 2 IFCCOLUMN | property sets: Identity Data, Phasing
      IFCBUILDINGSTOREY "02" | long name "02" | elevation 8860.00000000009
        contains 37 elements
          3 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:RC Wall 220 mm" | object type "Basic Wall:RC Wall 220 mm:4537" | names: "Basic Wall:RC Wall 220 mm:27187", "Basic Wall:RC Wall 220 mm:487237", "Basic Wall:RC Wall 220 mm:487527" | material: layers "Basic Wall:RC Wall 220 mm" ("Concrete, Cast-in-Place gray" 220.) | property sets: Constraints, Dimensions, Identity Data, Phasing, Structural, Pset_WallCommon
          1 x IFCSLAB | object type "Floor:RC Floor - 250 mm" | FLOOR | names: "Floor:RC Floor - 250 mm:27206" | material: "Concrete, Cast-in-Place gray" | property sets: Pset_SlabCommon, Constraints, Dimensions, Phasing, Structural, Analytical Properties
          3 x IFCWALL | type IFCWALLTYPE "Basic Wall:RC Wall 250 mm" | object type "Basic Wall:RC Wall 250 mm:4536" | names: "Basic Wall:RC Wall 250 mm:28205", "Basic Wall:RC Wall 250 mm:28207", "Basic Wall:RC Wall 250 mm:28209" | material: layers "Basic Wall:RC Wall 250 mm" ("Concrete, Cast-in-Place gray" 250.) | property sets: Constraints, Dimensions, Identity Data, Phasing, Structural, Pset_WallCommon
          3 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:RC Wall 250 mm" | object type "Basic Wall:RC Wall 250 mm:4536" | names: "Basic Wall:RC Wall 250 mm:28211", "Basic Wall:RC Wall 250 mm:28213", "Basic Wall:RC Wall 250 mm:28215" | material: layers "Basic Wall:RC Wall 250 mm" ("Concrete, Cast-in-Place gray" 250.) | property sets: Constraints, Dimensions, Identity Data, Phasing, Structural, Pset_WallCommon
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:RC Wall 200 mm" | object type "Basic Wall:RC Wall 200 mm:4535" | names: "Basic Wall:RC Wall 200 mm:131609" | material: layers "Basic Wall:RC Wall 200 mm" ("Concrete, Cast-in-Place gray" 200.) | property sets: Constraints, Dimensions, Identity Data, Phasing, Structural, Pset_WallCommon
          1 x IFCSLAB | object type "Floor:RC Floor - 200 mm" | FLOOR | names: "Floor:RC Floor - 200 mm:183588" | material: layers "Floor:RC Floor - 200 mm" ("Concrete, Cast-in-Place gray" 200.) | property sets: Pset_SlabCommon, Constraints, Dimensions, Identity Data, Phasing, Structural
          1 x IFCSLAB | object type "Floor:Precast Floor - 200 mm" | FLOOR | names: "Floor:Precast Floor - 200 mm:190740" | material: layers "Floor:Precast Floor - 200 mm" ("Concrete, Precast" 200.) | property sets: Pset_SlabCommon, Constraints, Dimensions, Identity Data, Phasing, Structural
          2 x IFCBUILDINGELEMENTPROXY | object type "Stairs T4" | names: "Stairs T4:Stairs T4:195399", "Stairs T4:Stairs T4:207352" | material: "Concrete, Precast" | property sets: Pset_BuildingElementProxyCommon, Constraints, Dimensions, Identity Data, Materials and Finishes, Phasing
          1 x IFCBUILDINGELEMENTPROXY | object type "Stairs T5" | names: "Stairs T5:Stairs T5:197561" | material: "Concrete, Precast" | property sets: Pset_BuildingElementProxyCommon, Constraints, Dimensions, Identity Data, Materials and Finishes, Phasing
          2 x IFCANNOTATION
          4 x IFCSLAB | object type "Floor:RC Floor - 210 mm" | FLOOR | names: "Floor:RC Floor - 210 mm:390155", "Floor:RC Floor - 210 mm:530917", "Floor:RC Floor - 210 mm:530981" (+1 more) | material: layers "Floor:RC Floor - 210 mm" ("Concrete, Cast-in-Place gray" 210.) | property sets: Pset_SlabCommon, Constraints, Dimensions, Phasing, Structural, Materials and Finishes
          4 x IFCELEMENTASSEMBLY | object type "Structural Columns Assembly:B9-ST11" | USERDEFINED | names: "Structural Columns Assembly:B9-ST11:516637", "Structural Columns Assembly:B9-ST11:517094", "Structural Columns Assembly:B9-ST11:518412" (+1 more) | parts: 4 IFCBUILDINGELEMENTPROXY, 4 IFCCOLUMN | property sets: Identity Data, Phasing
          2 x IFCELEMENTASSEMBLY | object type "Structural Columns Assembly:B9-ST08" | USERDEFINED | names: "Structural Columns Assembly:B9-ST08:519330", "Structural Columns Assembly:B9-ST08:520370" | parts: 2 IFCBUILDINGELEMENTPROXY, 2 IFCCOLUMN | property sets: Identity Data, Phasing
          3 x IFCELEMENTASSEMBLY | object type "Structural Columns Assembly:B9-ST13" | USERDEFINED | names: "Structural Columns Assembly:B9-ST13:520044", "Structural Columns Assembly:B9-ST13:522439", "Structural Columns Assembly:B9-ST13:522536" | parts: 3 IFCBUILDINGELEMENTPROXY, 3 IFCCOLUMN | property sets: Identity Data, Phasing
          1 x IFCELEMENTASSEMBLY | object type "Structural Columns Assembly:B9-ST27" | USERDEFINED | names: "Structural Columns Assembly:B9-ST27:521411" | parts: 1 IFCBUILDINGELEMENTPROXY, 1 IFCCOLUMN | property sets: Identity Data, Phasing
          1 x IFCELEMENTASSEMBLY | object type "Structural Columns Assembly:B9-ST26" | USERDEFINED | names: "Structural Columns Assembly:B9-ST26:522337" | parts: 1 IFCBUILDINGELEMENTPROXY, 1 IFCCOLUMN | property sets: Identity Data, Phasing
          3 x IFCSLAB | object type "Floor:RC Floor - 160 mm" | FLOOR | names: "Floor:RC Floor - 160 mm:531052", "Floor:RC Floor - 160 mm:531052:2", "Floor:RC Floor - 160 mm:531052:3" | material: layers "Floor:RC Floor - 160 mm" ("Concrete, Cast-in-Place gray" 160.) | property sets: Materials and Finishes, Identity Data, Graphics, Construction, Analytical Properties, Pset_SlabCommon
          1 x IFCBUILDINGELEMENTPROXY | object type "floor edge" | names: "floor edge:floor edge:623148" | material: "Default" | property sets: Identity Data, Pset_BuildingElementProxyCommon, Constraints, Dimensions, Phasing, Structural
      IFCBUILDINGSTOREY "03" | long name "03" | elevation 11760.0000000001
        contains 24 elements
          1 x IFCSLAB | object type "Floor:RC Floor - 250 mm" | FLOOR | names: "Floor:RC Floor - 250 mm:27760" | material: "Concrete, Cast-in-Place gray" | property sets: Pset_SlabCommon, Constraints, Dimensions, Phasing, Structural, Analytical Properties
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:RC Wall 200 mm" | object type "Basic Wall:RC Wall 200 mm:4535" | names: "Basic Wall:RC Wall 200 mm:132080" | material: layers "Basic Wall:RC Wall 200 mm" ("Concrete, Cast-in-Place gray" 200.) | property sets: Constraints, Dimensions, Identity Data, Phasing, Structural, Pset_WallCommon
          1 x IFCBUILDINGELEMENTPROXY | object type "Stairs T5" | names: "Stairs T5:Stairs T5:207886" | material: "Concrete, Precast" | property sets: Pset_BuildingElementProxyCommon, Constraints, Dimensions, Identity Data, Materials and Finishes, Phasing
          1 x IFCBUILDINGELEMENTPROXY | object type "Stairs T4" | names: "Stairs T4:Stairs T4:210597" | material: "Concrete, Precast" | property sets: Pset_BuildingElementProxyCommon, Constraints, Dimensions, Identity Data, Materials and Finishes, Phasing
          3 x IFCSLAB | object type "Floor:RC Floor - 210 mm" | FLOOR | names: "Floor:RC Floor - 210 mm:393293", "Floor:RC Floor - 210 mm:608769", "Floor:RC Floor - 210 mm:608795" | material: layers "Floor:RC Floor - 210 mm" ("Concrete, Cast-in-Place gray" 210.) | property sets: Pset_SlabCommon, Constraints, Dimensions, Phasing, Structural, Materials and Finishes
          2 x IFCELEMENTASSEMBLY | object type "Structural Columns Assembly:B9-ST11" | USERDEFINED | names: "Structural Columns Assembly:B9-ST11:516646", "Structural Columns Assembly:B9-ST11:518417" | parts: 2 IFCBUILDINGELEMENTPROXY, 2 IFCCOLUMN | property sets: Identity Data, Phasing
          2 x IFCELEMENTASSEMBLY | object type "Structural Columns Assembly:B9-ST10" | USERDEFINED | names: "Structural Columns Assembly:B9-ST10:517102", "Structural Columns Assembly:B9-ST10:628387" | parts: 2 IFCBUILDINGELEMENTPROXY, 2 IFCCOLUMN | property sets: Identity Data, Phasing
          5 x IFCELEMENTASSEMBLY | object type "Structural Columns Assembly:B9-ST13" | USERDEFINED | names: "Structural Columns Assembly:B9-ST13:519331", "Structural Columns Assembly:B9-ST13:520045", "Structural Columns Assembly:B9-ST13:520371" (+2 more) | parts: 5 IFCBUILDINGELEMENTPROXY, 5 IFCCOLUMN | property sets: Identity Data, Phasing
          1 x IFCELEMENTASSEMBLY | object type "Structural Columns Assembly:B9-ST27" | USERDEFINED | names: "Structural Columns Assembly:B9-ST27:521311" | parts: 1 IFCBUILDINGELEMENTPROXY, 1 IFCCOLUMN | property sets: Identity Data, Phasing
          1 x IFCELEMENTASSEMBLY | object type "Structural Columns Assembly:B9-ST08" | USERDEFINED | names: "Structural Columns Assembly:B9-ST08:522338" | parts: 1 IFCBUILDINGELEMENTPROXY, 1 IFCCOLUMN | property sets: Identity Data, Phasing
          1 x IFCSLAB | object type "Floor:RC Floor - 200 mm" | FLOOR | names: "Floor:RC Floor - 200 mm:526309" | material: layers "Floor:RC Floor - 200 mm" ("Concrete, Cast-in-Place gray" 200.) | property sets: Pset_SlabCommon, Constraints, Dimensions, Identity Data, Phasing, Structural
          1 x IFCSLAB | object type "Floor:Precast Floor - 200 mm" | FLOOR | names: "Floor:Precast Floor - 200 mm:538903" | material: layers "Floor:Precast Floor - 200 mm" ("Concrete, Precast" 200.) | property sets: Pset_SlabCommon, Constraints, Dimensions, Identity Data, Phasing, Structural
          3 x IFCSLAB | object type "Floor:RC Floor - 160 mm" | FLOOR | names: "Floor:RC Floor - 160 mm:608725", "Floor:RC Floor - 160 mm:608725:2", "Floor:RC Floor - 160 mm:608725:3" | material: layers "Floor:RC Floor - 160 mm" ("Concrete, Cast-in-Place gray" 160.) | property sets: Materials and Finishes, Identity Data, Graphics, Construction, Analytical Properties, Pset_SlabCommon
          1 x IFCBUILDINGELEMENTPROXY | object type "floor edge" | names: "floor edge:floor edge:623534" | material: "Default" | property sets: Identity Data, Pset_BuildingElementProxyCommon, Constraints, Dimensions, Phasing, Structural
      IFCBUILDINGSTOREY "04" | long name "04" | elevation 14660.0000000001
        contains 24 elements
          1 x IFCSLAB | object type "Floor:RC Floor - 250 mm" | FLOOR | names: "Floor:RC Floor - 250 mm:27914" | material: "Concrete, Cast-in-Place gray" | property sets: Pset_SlabCommon, Constraints, Dimensions, Phasing, Structural, Analytical Properties
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:RC Wall 200 mm" | object type "Basic Wall:RC Wall 200 mm:4535" | names: "Basic Wall:RC Wall 200 mm:132518" | material: layers "Basic Wall:RC Wall 200 mm" ("Concrete, Cast-in-Place gray" 200.) | property sets: Constraints, Dimensions, Identity Data, Phasing, Structural, Pset_WallCommon
          1 x IFCBUILDINGELEMENTPROXY | object type "Stairs T5" | names: "Stairs T5:Stairs T5:213724" | material: "Concrete, Precast" | property sets: Pset_BuildingElementProxyCommon, Constraints, Dimensions, Identity Data, Materials and Finishes, Phasing
          4 x IFCELEMENTASSEMBLY | object type "Structural Columns Assembly:B9-ST10" | USERDEFINED | names: "Structural Columns Assembly:B9-ST10:516655", "Structural Columns Assembly:B9-ST10:517110", "Structural Columns Assembly:B9-ST10:518422" (+1 more) | parts: 4 IFCBUILDINGELEMENTPROXY, 4 IFCCOLUMN | property sets: Identity Data, Phasing
          6 x IFCELEMENTASSEMBLY | object type "Structural Columns Assembly:B9-ST13" | USERDEFINED | names: "Structural Columns Assembly:B9-ST13:519332", "Structural Columns Assembly:B9-ST13:520046", "Structural Columns Assembly:B9-ST13:520372" (+3 more) | parts: 6 IFCBUILDINGELEMENTPROXY, 6 IFCCOLUMN | property sets: Identity Data, Phasing
          1 x IFCELEMENTASSEMBLY | object type "Structural Columns Assembly:B9-ST09" | USERDEFINED | names: "Structural Columns Assembly:B9-ST09:521181" | parts: 1 IFCBUILDINGELEMENTPROXY, 1 IFCCOLUMN | property sets: Identity Data, Phasing
          1 x IFCSLAB | object type "Floor:RC Floor - 200 mm" | FLOOR | names: "Floor:RC Floor - 200 mm:526656" | material: layers "Floor:RC Floor - 200 mm" ("Concrete, Cast-in-Place gray" 200.) | property sets: Pset_SlabCommon, Constraints, Dimensions, Identity Data, Phasing, Structural
          1 x IFCBUILDINGELEMENTPROXY | object type "Stairs T4" | names: "Stairs T4:Stairs T4:537153" | material: "Concrete, Precast" | property sets: Pset_BuildingElementProxyCommon, Constraints, Dimensions, Identity Data, Materials and Finishes, Phasing
          1 x IFCSLAB | object type "Floor:Precast Floor - 200 mm" | FLOOR | names: "Floor:Precast Floor - 200 mm:538942" | material: layers "Floor:Precast Floor - 200 mm" ("Concrete, Precast" 200.) | property sets: Pset_SlabCommon, Constraints, Dimensions, Identity Data, Phasing, Structural
          3 x IFCSLAB | object type "Floor:RC Floor - 210 mm" | FLOOR | names: "Floor:RC Floor - 210 mm:610560", "Floor:RC Floor - 210 mm:610632", "Floor:RC Floor - 210 mm:610660" | material: layers "Floor:RC Floor - 210 mm" ("Concrete, Cast-in-Place gray" 210.) | property sets: Materials and Finishes, Pset_SlabCommon, Constraints, Dimensions, Identity Data, Phasing
          3 x IFCSLAB | object type "Floor:RC Floor - 160 mm" | FLOOR | names: "Floor:RC Floor - 160 mm:610588", "Floor:RC Floor - 160 mm:610588:2", "Floor:RC Floor - 160 mm:610588:3" | material: layers "Floor:RC Floor - 160 mm" ("Concrete, Cast-in-Place gray" 160.) | property sets: Materials and Finishes, Identity Data, Graphics, Construction, Analytical Properties, Pset_SlabCommon
          1 x IFCBUILDINGELEMENTPROXY | object type "floor edge" | names: "floor edge:floor edge:624165" | material: "Default" | property sets: Identity Data, Pset_BuildingElementProxyCommon, Constraints, Dimensions, Phasing, Structural
      IFCBUILDINGSTOREY "05" | long name "05" | elevation 17560.0000000001
        contains 23 elements
          1 x IFCSLAB | object type "Floor:RC Floor - 250 mm" | FLOOR | names: "Floor:RC Floor - 250 mm:28068" | material: "Concrete, Cast-in-Place gray" | property sets: Pset_SlabCommon, Constraints, Dimensions, Phasing, Structural, Analytical Properties
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:RC Wall 200 mm" | object type "Basic Wall:RC Wall 200 mm:4535" | names: "Basic Wall:RC Wall 200 mm:133049" | material: layers "Basic Wall:RC Wall 200 mm" ("Concrete, Cast-in-Place gray" 200.) | property sets: Constraints, Dimensions, Identity Data, Phasing, Structural, Pset_WallCommon
          1 x IFCBUILDINGELEMENTPROXY | object type "Stairs T5" | names: "Stairs T5:Stairs T5:215298" | material: "Concrete, Precast" | property sets: Pset_BuildingElementProxyCommon, Constraints, Dimensions, Identity Data, Materials and Finishes, Phasing
          4 x IFCELEMENTASSEMBLY | object type "Structural Columns Assembly:B9-ST10" | USERDEFINED | names: "Structural Columns Assembly:B9-ST10:516600", "Structural Columns Assembly:B9-ST10:516989", "Structural Columns Assembly:B9-ST10:518402" (+1 more) | parts: 4 IFCBUILDINGELEMENTPROXY, 4 IFCCOLUMN | property sets: Identity Data, Phasing
          6 x IFCELEMENTASSEMBLY | object type "Structural Columns Assembly:B9-ST13" | USERDEFINED | names: "Structural Columns Assembly:B9-ST13:519333", "Structural Columns Assembly:B9-ST13:520047", "Structural Columns Assembly:B9-ST13:520373" (+3 more) | parts: 6 IFCBUILDINGELEMENTPROXY, 6 IFCCOLUMN | property sets: Identity Data, Phasing
          1 x IFCELEMENTASSEMBLY | object type "Structural Columns Assembly:B9-ST09" | USERDEFINED | names: "Structural Columns Assembly:B9-ST09:521217" | parts: 1 IFCBUILDINGELEMENTPROXY, 1 IFCCOLUMN | property sets: Identity Data, Phasing
          1 x IFCSLAB | object type "Floor:RC Floor - 200 mm" | FLOOR | names: "Floor:RC Floor - 200 mm:526685" | material: layers "Floor:RC Floor - 200 mm" ("Concrete, Cast-in-Place gray" 200.) | property sets: Pset_SlabCommon, Constraints, Dimensions, Identity Data, Phasing, Structural
          1 x IFCSLAB | object type "Floor:Precast Floor - 200 mm" | FLOOR | names: "Floor:Precast Floor - 200 mm:538981" | material: layers "Floor:Precast Floor - 200 mm" ("Concrete, Precast" 200.) | property sets: Pset_SlabCommon, Constraints, Dimensions, Identity Data, Phasing, Structural
          3 x IFCSLAB | object type "Floor:RC Floor - 210 mm" | FLOOR | names: "Floor:RC Floor - 210 mm:615158", "Floor:RC Floor - 210 mm:615223", "Floor:RC Floor - 210 mm:615263" | material: layers "Floor:RC Floor - 210 mm" ("Concrete, Cast-in-Place gray" 210.) | property sets: Materials and Finishes, Pset_SlabCommon, Constraints, Dimensions, Identity Data, Phasing
          3 x IFCSLAB | object type "Floor:RC Floor - 160 mm" | FLOOR | names: "Floor:RC Floor - 160 mm:615182", "Floor:RC Floor - 160 mm:615182:2", "Floor:RC Floor - 160 mm:615182:3" | material: layers "Floor:RC Floor - 160 mm" ("Concrete, Cast-in-Place gray" 160.) | property sets: Materials and Finishes, Identity Data, Graphics, Construction, Analytical Properties, Pset_SlabCommon
          1 x IFCBUILDINGELEMENTPROXY | object type "floor edge" | names: "floor edge:floor edge:624580" | material: "Default" | property sets: Identity Data, Pset_BuildingElementProxyCommon, Constraints, Dimensions, Phasing, Structural
      IFCBUILDINGSTOREY "06" | long name "06" | elevation 20460.0000000001
        contains 12 elements
          1 x IFCBUILDINGELEMENTPROXY | object type "floor edge" | names: "floor edge:floor edge:625158" | material: "Default" | property sets: Identity Data, Pset_BuildingElementProxyCommon, Constraints, Dimensions, Phasing, Structural
          1 x IFCSLAB | object type "Floor:RC Floor - 250 mm" | FLOOR | names: "Floor:RC Floor - 250 mm:28222" | material: "Concrete, Cast-in-Place gray" | property sets: Pset_SlabCommon, Constraints, Dimensions, Phasing, Structural, Analytical Properties
          2 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:RC Wall 200 mm" | object type "Basic Wall:RC Wall 200 mm:4535" | names: "Basic Wall:RC Wall 200 mm:133407", "Basic Wall:RC Wall 200 mm:297553" | material: layers "Basic Wall:RC Wall 200 mm" ("Concrete, Cast-in-Place gray" 200.) | property sets: Constraints, Dimensions, Identity Data, Phasing, Structural, Pset_WallCommon
          1 x IFCSLAB | object type "Floor:RC Floor - 200 mm" | FLOOR | names: "Floor:RC Floor - 200 mm:212606" | material: layers "Floor:RC Floor - 200 mm" ("Concrete, Cast-in-Place gray" 200.) | property sets: Pset_SlabCommon, Constraints, Dimensions, Phasing, Structural, Analytical Properties
          4 x IFCELEMENTASSEMBLY | object type "Structural Columns Assembly:B9-ST28" | USERDEFINED | names: "Structural Columns Assembly:B9-ST28:515275", "Structural Columns Assembly:B9-ST28:515337", "Structural Columns Assembly:B9-ST28:515374" (+1 more) | parts: 4 IFCBUILDINGELEMENTPROXY, 4 IFCCOLUMN | property sets: Identity Data, Phasing
          1 x IFCELEMENTASSEMBLY | object type "Structural Columns Assembly:B9-ST25" | USERDEFINED | names: "Structural Columns Assembly:B9-ST25:519683" | parts: 1 IFCBUILDINGELEMENTPROXY, 1 IFCCOLUMN | property sets: Identity Data, Phasing
          2 x IFCSLAB | object type "Floor:RC Floor - 160 mm" | FLOOR | names: "Floor:RC Floor - 160 mm:619926", "Floor:RC Floor - 160 mm:619926:2" | material: layers "Floor:RC Floor - 160 mm" ("Concrete, Cast-in-Place gray" 160.) | property sets: Materials and Finishes, Identity Data, Graphics, Construction, Analytical Properties, Pset_SlabCommon
      IFCBUILDINGSTOREY "07" | long name "07" | elevation 23360.0000000001
        contains 18 elements
          1 x IFCSLAB | object type "Floor:RC Floor - 250 mm" | FLOOR | names: "Floor:RC Floor - 250 mm:297690" | material: layers "Floor:RC Floor - 250 mm" ("Concrete, Cast-in-Place gray" 250.) | property sets: Pset_SlabCommon, Constraints, Dimensions, Phasing, Structural, Analytical Properties
          1 x IFCSLAB | object type "Floor:RC Floor - 200 mm" | FLOOR | names: "Floor:RC Floor - 200 mm:502657" | material: layers "Floor:RC Floor - 200 mm" ("Concrete, Cast-in-Place gray" 200.) | property sets: Pset_SlabCommon, Constraints, Dimensions, Identity Data, Phasing, Structural
          3 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:RC Wall 250 mm" | object type "Basic Wall:RC Wall 250 mm:4536" | names: "Basic Wall:RC Wall 250 mm:503108", "Basic Wall:RC Wall 250 mm:503110", "Basic Wall:RC Wall 250 mm:540951" | material: layers "Basic Wall:RC Wall 250 mm" ("Concrete, Cast-in-Place gray" 250.) | property sets: Constraints, Dimensions, Identity Data, Phasing, Structural, Pset_WallCommon
          9 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:RC Wall 150 mm" | object type "Basic Wall:RC Wall 150 mm:503675" | names: "Basic Wall:RC Wall 150 mm:503702", "Basic Wall:RC Wall 150 mm:503715", "Basic Wall:RC Wall 150 mm:503732" (+6 more) | material: layers "Basic Wall:RC Wall 150 mm" ("Concrete, Cast-in-Place gray" 150.) | property sets: Constraints, Dimensions, Identity Data, Phasing, Structural, Pset_WallCommon
          4 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:RC Wall 100 mm" | object type "Basic Wall:RC Wall 100 mm:522683" | names: "Basic Wall:RC Wall 100 mm:522727", "Basic Wall:RC Wall 100 mm:522729", "Basic Wall:RC Wall 100 mm:522731" (+1 more) | material: layers "Basic Wall:RC Wall 100 mm" ("Concrete, Cast-in-Place gray" 100.) | property sets: Constraints, Dimensions, Identity Data, Phasing, Structural, Pset_WallCommon

Types
  IFCWALLTYPE "Basic Wall:RC Wall 220 mm" | STANDARD | 7 occurrences | material: layers "Basic Wall:RC Wall 220 mm" ("Concrete, Cast-in-Place gray" 220.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Materials and Finishes
  IFCWALLTYPE "Basic Wall:RC Wall 250 mm" | STANDARD | 14 occurrences | material: layers "Basic Wall:RC Wall 250 mm" ("Concrete, Cast-in-Place gray" 250.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Materials and Finishes
  IFCWALLTYPE "Basic Wall:RC Wall 200 mm" | STANDARD | 7 occurrences | material: layers "Basic Wall:RC Wall 200 mm" ("Concrete, Cast-in-Place gray" 200.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Materials and Finishes
  IFCWALLTYPE "Basic Wall:RC Wall 150 mm" | STANDARD | 9 occurrences | material: layers "Basic Wall:RC Wall 150 mm" ("Concrete, Cast-in-Place gray" 150.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Materials and Finishes
  IFCWALLTYPE "Basic Wall:RC Wall 100 mm" | STANDARD | 4 occurrences | material: layers "Basic Wall:RC Wall 100 mm" ("Concrete, Cast-in-Place gray" 100.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Materials and Finishes

Property sets
  Other | properties | on 11 objects (11 IFCBUILDINGELEMENTPROXY)
    Schedule Level = "Level: +23.64" (IFCLABEL)
  Other | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Client Name = "Dimensjon Rådgivning AS" (IFCTEXT)
    Project Address = "1103_54_1060" (IFCTEXT)
    Project Issue Date = "Issue Date" (IFCTEXT)
    Project Name = "1103_54_1060" (IFCTEXT)
    Project Number = "20672" (IFCTEXT)
    Project Status = "Project Status" (IFCTEXT)
    RM_R2R_LinkSessionIdList = "c65f412a-9893-49d9-ac34-c625748d36d6;" (IFCTEXT)
    RM_R2R_OriginOffset = "-418.339397558397;273.056832006751;0" (IFCTEXT)
    SOptDeadLoadCase = 1 (IFCINTEGER)
    SOptRevitBuild = "20120221_2030(x64)" (IFCTEXT)
    SOptViews = -1 (IFCINTEGER)
    UOptConnections = 0 (IFCINTEGER)
    UOptIsFileMode = 0 (IFCINTEGER)
    UOptReinforcement = 0 (IFCINTEGER)
    UOptSilentMode = 0 (IFCINTEGER)
    UOptSilentModeFileName = "" (IFCTEXT)
    UOptTransferDirSend = -1 (IFCINTEGER)
    UOptTransferSubject = 0 (IFCINTEGER)
  Other | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Schedule Level = "Level: +6.24" (IFCLABEL)
  Constraints | properties | on 60 objects (60 IFCBUILDINGELEMENTPROXY)
    Default Elevation = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 47 objects (47 IFCBUILDINGELEMENTPROXY)
    Elevation = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Host = "<not associated>" (IFCTEXT)
  Constraints | properties | on 8 objects (8 IFCBUILDINGSTOREY)
    Elevation Base = 0 (IFCINTEGER)
  Constraints | properties | on 7 objects (7 IFCWALLSTANDARDCASE)
    Base Constraint = "Level: +23.64" (IFCLABEL)
    Base Extension Distance = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Base Offset = -80. (IFCLENGTHMEASURE) [MILLI METRE]
    Base is Attached = FALSE (IFCBOOLEAN)
    Location Line = 3 (IFCINTEGER)
    Related to Mass = FALSE (IFCBOOLEAN)
    Room Bounding = TRUE (IFCBOOLEAN)
    Top Extension Distance = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Top Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Top is Attached = FALSE (IFCBOOLEAN)
    Unconnected Height = 480. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 6 objects (6 IFCCOLUMN)
    Base Level = "Level: +17.84" (IFCLABEL)
    Base Offset = -40.0059244951287 (IFCLENGTHMEASURE) [MILLI METRE]
    Column Location Mark = "" (IFCTEXT)
    Column Style = 1 (IFCINTEGER)
    Cross-Section Rotation = 360. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Move Base With Grids = TRUE (IFCBOOLEAN)
    Move Top With Grids = TRUE (IFCBOOLEAN)
    Top Level = "Level: +20.74" (IFCLABEL)
    Top Offset = -270.018676780456 (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 6 objects (6 IFCCOLUMN)
    Base Level = "Level: +14.94" (IFCLABEL)
    Base Offset = -39.9994982329277 (IFCLENGTHMEASURE) [MILLI METRE]
    Column Location Mark = "" (IFCTEXT)
    Column Style = 1 (IFCINTEGER)
    Cross-Section Rotation = 360. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Move Base With Grids = TRUE (IFCBOOLEAN)
    Move Top With Grids = TRUE (IFCBOOLEAN)
    Top Level = "Level: +17.84" (IFCLABEL)
    Top Offset = -270.012250518251 (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 5 objects (5 IFCCOLUMN)
    Base Level = "Level: +12.04" (IFCLABEL)
    Base Offset = -39.9994982329234 (IFCLENGTHMEASURE) [MILLI METRE]
    Column Location Mark = "" (IFCTEXT)
    Column Style = 1 (IFCINTEGER)
    Cross-Section Rotation = 360. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Move Base With Grids = TRUE (IFCBOOLEAN)
    Move Top With Grids = TRUE (IFCBOOLEAN)
    Top Level = "Level: +14.94" (IFCLABEL)
    Top Offset = -270.012250518251 (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 4 objects (4 IFCSLAB)
    Height Offset From Level = -70. (IFCLENGTHMEASURE) [MILLI METRE]
    Level = "Level: +9.14" (IFCLABEL)
    Related to Mass = FALSE (IFCBOOLEAN)
    Room Bounding = TRUE (IFCBOOLEAN)
  Constraints: 115 more contents on 155 objects not shown
  Dimensions | properties | on 55 objects (55 IFCBUILDINGELEMENTPROXY)
    Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Plate_X = 200. (IFCLENGTHMEASURE) [MILLI METRE]
    Plate_Y = 200. (IFCLENGTHMEASURE) [MILLI METRE]
    Plate_t = 12. (IFCLENGTHMEASURE) [MILLI METRE]
    R1_X = 50. (IFCLENGTHMEASURE) [MILLI METRE]
    R1_Y = 75. (IFCLENGTHMEASURE) [MILLI METRE]
    R2_X = 50. (IFCLENGTHMEASURE) [MILLI METRE]
    R2_Y = 25. (IFCLENGTHMEASURE) [MILLI METRE]
    R_D = 16. (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions | properties | on 30 objects (30 IFCBUILDINGELEMENTPROXY)
    Column_X = 100. (IFCLENGTHMEASURE) [MILLI METRE]
    Column_Y = 40. (IFCLENGTHMEASURE) [MILLI METRE]
    Height = 230. (IFCLENGTHMEASURE) [MILLI METRE]
    Plate_dX = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Plate_dY = 20. (IFCLENGTHMEASURE) [MILLI METRE]
    Rd_X = 100. (IFCLENGTHMEASURE) [MILLI METRE]
    Rd_Y = 80. (IFCLENGTHMEASURE) [MILLI METRE]
    Volume = 1077667.16666954 (IFCVOLUMEMEASURE) [MILLI CUBIC_METRE]
  Dimensions | properties | on 20 objects (20 IFCBUILDINGELEMENTPROXY)
    Column_X = 100. (IFCLENGTHMEASURE) [MILLI METRE]
    Column_Y = 100. (IFCLENGTHMEASURE) [MILLI METRE]
    Height = 230. (IFCLENGTHMEASURE) [MILLI METRE]
    Plate_dX = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Plate_dY = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Rd_X = 100. (IFCLENGTHMEASURE) [MILLI METRE]
    Rd_Y = 100. (IFCLENGTHMEASURE) [MILLI METRE]
    Volume = 1125667.16666943 (IFCVOLUMEMEASURE) [MILLI CUBIC_METRE]
  Dimensions | properties | on 14 objects (14 IFCCOLUMN)
    Volume = 4741920.00000002 (IFCVOLUMEMEASURE) [MILLI CUBIC_METRE]
  Dimensions | properties | on 8 objects (8 IFCBUILDINGSTOREY)
    Computation Height = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions | properties | on 5 objects (5 IFCBUILDINGELEMENTPROXY)
    Column_X = 40. (IFCLENGTHMEASURE) [MILLI METRE]
    Column_Y = 40. (IFCLENGTHMEASURE) [MILLI METRE]
    Height = 230. (IFCLENGTHMEASURE) [MILLI METRE]
    Plate_dX = 20. (IFCLENGTHMEASURE) [MILLI METRE]
    Plate_dY = 20. (IFCLENGTHMEASURE) [MILLI METRE]
    Rd_X = 80. (IFCLENGTHMEASURE) [MILLI METRE]
    Rd_Y = 80. (IFCLENGTHMEASURE) [MILLI METRE]
    Volume = 1034467.16666966 (IFCVOLUMEMEASURE) [MILLI CUBIC_METRE]
  Dimensions | properties | on 5 objects (5 IFCBUILDINGELEMENTPROXY)
    Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Plate_X = 200. (IFCLENGTHMEASURE) [MILLI METRE]
    Plate_Y = 200. (IFCLENGTHMEASURE) [MILLI METRE]
    Plate_t = 12. (IFCLENGTHMEASURE) [MILLI METRE]
    R1_X = 75. (IFCLENGTHMEASURE) [MILLI METRE]
    R1_Y = 75. (IFCLENGTHMEASURE) [MILLI METRE]
    R2_X = 25. (IFCLENGTHMEASURE) [MILLI METRE]
    R2_Y = 25. (IFCLENGTHMEASURE) [MILLI METRE]
    R_D = 16. (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions | properties | on 4 objects (4 IFCSLAB)
    Area = 3526694.54812603 (IFCAREAMEASURE) [MILLI SQUARE_METRE]
    Perimeter = 8630.43523610902 (IFCLENGTHMEASURE) [MILLI METRE]
    Thickness = 200. (IFCLENGTHMEASURE) [MILLI METRE]
    Volume = 679300549.279382 (IFCVOLUMEMEASURE) [MILLI CUBIC_METRE]
  Dimensions: 111 more contents on 149 objects not shown
  Identity Data | properties | on 99 objects (61 IFCELEMENTASSEMBLY, 38 IFCSLAB) | on 5 type objects
    Assembly Code = "" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
  Identity Data | properties | on 66 objects (66 IFCBUILDINGELEMENTPROXY)
    Assembly Code = "" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    OmniClass Number = "" (IFCTEXT)
    OmniClass Title = "" (IFCTEXT)
  Identity Data | properties | on 60 objects (60 IFCELEMENTASSEMBLY)
    Naming Category = "-2001330" (IFCLABEL)
  Identity Data | properties | on 58 objects (35 IFCWALLSTANDARDCASE, 20 IFCSLAB, 3 IFCWALL)
    Comments = "" (IFCTEXT)
  Identity Data | properties | on 20 objects (20 IFCBUILDINGELEMENTPROXY)
    Assembly Name = "B9-ST13" (IFCTEXT)
  Identity Data | properties | on 10 objects (10 IFCBUILDINGELEMENTPROXY)
    Assembly Name = "B9-ST10" (IFCTEXT)
  Identity Data | properties | on 7 objects (7 IFCSLAB)
    Assembly Code = "" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    Model = "R1" (IFCTEXT)
  Identity Data | properties | on 6 objects (6 IFCBUILDINGELEMENTPROXY)
    Assembly Name = "B9-ST11" (IFCTEXT)
  Identity Data: 54 more contents on 118 objects not shown
  Phasing | properties | on 283 objects (75 IFCBUILDINGELEMENTPROXY, 61 IFCCOLUMN, 61 IFCELEMENTASSEMBLY, 45 IFCSLAB)
    Phase Created = "New Construction" (IFCLABEL)
  Structural | properties | on 61 objects (61 IFCCOLUMN)
    Enable Analytical Model = TRUE (IFCBOOLEAN)
  Structural | properties | on 44 objects (44 IFCSLAB)
    Enable Analytical Model = TRUE (IFCBOOLEAN)
    Rebar Cover - Bottom Face = "Rebar Cover Settings: Rebar Cover 1" (IFCLABEL)
    Rebar Cover - Other Faces = "Rebar Cover Settings: Rebar Cover 1" (IFCLABEL)
    Rebar Cover - Top Face = "Rebar Cover Settings: Rebar Cover 1" (IFCLABEL)
    Structural = TRUE (IFCBOOLEAN)
  Structural | properties | on 39 objects (36 IFCWALLSTANDARDCASE, 3 IFCWALL)
    Enable Analytical Model = TRUE (IFCBOOLEAN)
    Rebar Cover - Exterior Face = "Rebar Cover Settings: Rebar Cover 1" (IFCLABEL)
    Rebar Cover - Interior Face = "Rebar Cover Settings: Rebar Cover 1" (IFCLABEL)
    Rebar Cover - Other Faces = "Rebar Cover Settings: Rebar Cover 1" (IFCLABEL)
    Structural = TRUE (IFCBOOLEAN)
    Structural Usage = 1 (IFCINTEGER)
  Structural | properties | on 9 objects (9 IFCBUILDINGELEMENTPROXY)
    Rebar Cover - Bottom Face = "Rebar Cover Settings: Rebar Cover 1" (IFCLABEL)
    Rebar Cover - Other Faces = "Rebar Cover Settings: Rebar Cover 1" (IFCLABEL)
    Rebar Cover - Top Face = "Rebar Cover Settings: Rebar Cover 1" (IFCLABEL)
  Structural | properties | on 5 objects (5 IFCBUILDINGELEMENTPROXY)
    Rebar Cover - Other Faces = "Rebar Cover Settings: Rebar Cover 1" (IFCLABEL)
    Rebar Cover - Top Face = "Rebar Cover Settings: Rebar Cover 1" (IFCLABEL)
  Structural | properties | on 2 objects (2 IFCWALLSTANDARDCASE)
    Enable Analytical Model = TRUE (IFCBOOLEAN)
    Rebar Cover - Exterior Face = "Rebar Cover Settings: Rebar Cover 1" (IFCLABEL)
    Rebar Cover - Interior Face = "Rebar Cover Settings: Rebar Cover 1" (IFCLABEL)
    Structural = TRUE (IFCBOOLEAN)
    Structural Usage = 1 (IFCINTEGER)
  Structural | properties | on 1 object (1 IFCSLAB)
    Enable Analytical Model = TRUE (IFCBOOLEAN)
    Rebar Cover - Bottom Face = "Rebar Cover Settings: Rebar Cover 1" (IFCLABEL)
    Structural = TRUE (IFCBOOLEAN)
  Pset_WallCommon | properties | on 9 objects (9 IFCWALLSTANDARDCASE)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "RC Wall 150 mm" (IFCIDENTIFIER)
    ThermalTransmittance = 6.97333333333333 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_WallCommon | properties | on 8 objects (6 IFCWALLSTANDARDCASE, 2 IFCWALL)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "RC Wall 250 mm" (IFCIDENTIFIER)
    ThermalTransmittance = 4.184 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_WallCommon | properties | on 6 objects (5 IFCWALLSTANDARDCASE, 1 IFCWALL)
    ExtendToStructure = TRUE (IFCBOOLEAN)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "RC Wall 250 mm" (IFCIDENTIFIER)
    ThermalTransmittance = 4.184 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_WallCommon | properties | on 5 objects (5 IFCWALLSTANDARDCASE)
    ExtendToStructure = TRUE (IFCBOOLEAN)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "RC Wall 220 mm" (IFCIDENTIFIER)
    ThermalTransmittance = 4.75454545454545 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_WallCommon | properties | on 5 objects (5 IFCWALLSTANDARDCASE)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "RC Wall 200 mm" (IFCIDENTIFIER)
    ThermalTransmittance = 5.23 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_WallCommon | properties | on 4 objects (4 IFCWALLSTANDARDCASE)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "RC Wall 100 mm" (IFCIDENTIFIER)
    ThermalTransmittance = 10.46 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_WallCommon | properties | on 2 objects (2 IFCWALLSTANDARDCASE)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "RC Wall 220 mm" (IFCIDENTIFIER)
    ThermalTransmittance = 4.75454545454545 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_WallCommon | properties | on 2 objects (2 IFCWALLSTANDARDCASE)
    ExtendToStructure = TRUE (IFCBOOLEAN)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "RC Wall 200 mm" (IFCIDENTIFIER)
    ThermalTransmittance = 5.23 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_SlabCommon | properties | on 14 objects (14 IFCSLAB)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "RC Floor - 160 mm" (IFCIDENTIFIER)
    ThermalTransmittance = 6.5375 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_SlabCommon | properties | on 13 objects (13 IFCSLAB)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "RC Floor - 210 mm" (IFCIDENTIFIER)
    ThermalTransmittance = 4.98095238095238 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_SlabCommon | properties | on 7 objects (7 IFCSLAB)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "RC Floor - 250 mm" (IFCIDENTIFIER)
    ThermalTransmittance = 4.184 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_SlabCommon | properties | on 7 objects (7 IFCSLAB)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "RC Floor - 200 mm" (IFCIDENTIFIER)
    ThermalTransmittance = 5.23 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_SlabCommon | properties | on 4 objects (4 IFCSLAB)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "Precast Floor - 200 mm" (IFCIDENTIFIER)
    ThermalTransmittance = 5.23 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_BuildingElementProxyCommon | properties | on 55 objects (55 IFCBUILDINGELEMENTPROXY)
    Reference = "Edge" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 5 objects (5 IFCBUILDINGELEMENTPROXY)
    Reference = "Corner" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 5 objects (5 IFCBUILDINGELEMENTPROXY)
    Reference = "floor edge" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 4 objects (4 IFCBUILDINGELEMENTPROXY)
    Reference = "Stairs T4" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 4 objects (4 IFCBUILDINGELEMENTPROXY)
    Reference = "Stairs T5" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Reference = "Stairs T3" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Reference = "OrientationCube" (IFCIDENTIFIER)
  Materials and Finishes | properties | on 60 objects (60 IFCBUILDINGELEMENTPROXY)
    Structural Material = "Default" (IFCLABEL)
  Materials and Finishes | properties | on 41 objects (41 IFCSLAB) | on 5 type objects
    Structural Material = "Concrete, Cast-in-Place gray" (IFCLABEL)
  Materials and Finishes | properties | on 13 objects (9 IFCBUILDINGELEMENTPROXY, 4 IFCSLAB)
    Structural Material = "Concrete, Precast" (IFCLABEL)
  Materials and Finishes | properties | on 9 objects (9 IFCBUILDINGELEMENTPROXY)
    Material = "Concrete, Precast" (IFCLABEL)
  Pset_ColumnCommon | properties | on 33 objects (33 IFCCOLUMN)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "80x80x6" (IFCIDENTIFIER)
  Pset_ColumnCommon | properties | on 16 objects (16 IFCCOLUMN)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "120x80x8" (IFCIDENTIFIER)
  Pset_ColumnCommon | properties | on 4 objects (4 IFCCOLUMN)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "120x80x8" (IFCIDENTIFIER)
    Slope = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
  Pset_ColumnCommon | properties | on 4 objects (4 IFCCOLUMN)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "80x80x6" (IFCIDENTIFIER)
    Slope = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
  Pset_ColumnCommon | properties | on 3 objects (3 IFCCOLUMN)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "160x80x10" (IFCIDENTIFIER)
  Pset_ColumnCommon | properties | on 1 object (1 IFCCOLUMN)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "160x80x10" (IFCIDENTIFIER)
    Slope = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
  Construction | properties | on 37 objects (37 IFCCOLUMN)
    Base Cut Style = 1 (IFCINTEGER)
    Base Extension = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Top Cut Style = 1 (IFCINTEGER)
    Top Extension = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Construction | properties | on 14 objects (14 IFCSLAB)
    Default Thickness = 160. (IFCLENGTHMEASURE) [MILLI METRE]
    Function = 0 (IFCINTEGER)
  Construction | properties | on 13 objects (13 IFCSLAB)
    Default Thickness = 210. (IFCLENGTHMEASURE) [MILLI METRE]
    Function = 0 (IFCINTEGER)
  Construction | properties | on 11 objects (11 IFCSLAB)
    Default Thickness = 200. (IFCLENGTHMEASURE) [MILLI METRE]
    Function = 0 (IFCINTEGER)
  Construction | properties | on 7 objects (7 IFCSLAB)
    Default Thickness = 250. (IFCLENGTHMEASURE) [MILLI METRE]
    Function = 0 (IFCINTEGER)
  Construction | properties | on 1 type object
    Function = 1 (IFCINTEGER)
    Width = 220. (IFCLENGTHMEASURE) [MILLI METRE]
    Wrapping at Ends = 1 (IFCINTEGER)
    Wrapping at Inserts = 1 (IFCINTEGER)
  Construction | properties | on 1 type object
    Function = 1 (IFCINTEGER)
    Width = 250. (IFCLENGTHMEASURE) [MILLI METRE]
    Wrapping at Ends = 1 (IFCINTEGER)
    Wrapping at Inserts = 1 (IFCINTEGER)
  Construction | properties | on 1 type object
    Function = 1 (IFCINTEGER)
    Width = 200. (IFCLENGTHMEASURE) [MILLI METRE]
    Wrapping at Ends = 1 (IFCINTEGER)
    Wrapping at Inserts = 1 (IFCINTEGER)
  Construction: 2 more contents on 0 objects not shown
  Graphics | properties | on 45 objects (45 IFCSLAB) | on 5 type objects
    Coarse Scale Fill Color = 0 (IFCINTEGER)
  Graphics | properties | on 8 objects (8 IFCBUILDINGSTOREY)
    Color = 0 (IFCINTEGER)
    Line Pattern = "Dot" (IFCLABEL)
    Line Weight = 1 (IFCINTEGER)
    Symbol = "Level Head - Name: Level Head - Name" (IFCLABEL)
    Symbol at End 1 Default = FALSE (IFCBOOLEAN)
    Symbol at End 2 Default = TRUE (IFCBOOLEAN)
  Analytical Properties | properties | on 14 objects (14 IFCSLAB)
    Absorptance = 0.1 (IFCREAL)
    Heat Transfer Coefficient (U) = 6.5375 (IFCREAL)
    Roughness = 1 (IFCINTEGER)
    Thermal Resistance (R) = 0.152963671128107 (IFCREAL)
    Thermal mass = 241776. (IFCREAL)
  Analytical Properties | properties | on 13 objects (13 IFCSLAB)
    Absorptance = 0.1 (IFCREAL)
    Heat Transfer Coefficient (U) = 4.98095238095238 (IFCREAL)
    Roughness = 1 (IFCINTEGER)
    Thermal Resistance (R) = 0.200764818355641 (IFCREAL)
    Thermal mass = 317331. (IFCREAL)
  Analytical Properties | properties | on 11 objects (11 IFCSLAB) | on 1 type object
    Absorptance = 0.1 (IFCREAL)
    Heat Transfer Coefficient (U) = 5.23 (IFCREAL)
    Roughness = 1 (IFCINTEGER)
    Thermal Resistance (R) = 0.191204588910134 (IFCREAL)
    Thermal mass = 302220. (IFCREAL)
  Analytical Properties | properties | on 7 objects (7 IFCSLAB) | on 1 type object
    Absorptance = 0.1 (IFCREAL)
    Heat Transfer Coefficient (U) = 4.184 (IFCREAL)
    Roughness = 1 (IFCINTEGER)
    Thermal Resistance (R) = 0.239005736137667 (IFCREAL)
    Thermal mass = 377775. (IFCREAL)
  Analytical Properties | properties | on 1 type object
    Absorptance = 0.1 (IFCREAL)
    Heat Transfer Coefficient (U) = 4.75454545454545 (IFCREAL)
    Roughness = 1 (IFCINTEGER)
    Thermal Resistance (R) = 0.210325047801147 (IFCREAL)
    Thermal mass = 332442. (IFCREAL)
  Analytical Properties | properties | on 1 type object
    Absorptance = 0.1 (IFCREAL)
    Heat Transfer Coefficient (U) = 6.97333333333333 (IFCREAL)
    Roughness = 1 (IFCINTEGER)
    Thermal Resistance (R) = 0.1434034416826 (IFCREAL)
    Thermal mass = 226665. (IFCREAL)
  Analytical Properties | properties | on 1 type object
    Absorptance = 0.1 (IFCREAL)
    Heat Transfer Coefficient (U) = 10.46 (IFCREAL)
    Roughness = 1 (IFCINTEGER)
    Thermal Resistance (R) = 0.0956022944550669 (IFCREAL)
    Thermal mass = 151110. (IFCREAL)
  Pset_BuildingStoreyCommon | properties | on 8 objects (8 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Extents | properties | on 8 objects (8 IFCBUILDINGSTOREY)
    Scope Box = "B9" (IFCLABEL)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    NumberOfStoreys = 8 (IFCINTEGER)