IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [SurfaceGeometry]"
File name: "20672_RIB_Vannkanten_B4.i.ifc"
Time stamp: "2011-07-12T17:19:12"
Author: "DIMENSJON/Svein.Grude"
Organization: "Structural Designer"
Preprocessor: "IFC Database Version:Work"
Originating system: "Tekla Structures 18.0 Build:12834/24.10.2012, IFC Export Version: 309Mar 29 2012"
Application: "Tekla Structures" version "18.0" identifier "Multi material modeling" by Organization "Tekla Corporation"

People and organizations
  Person "Undefined" id "DIMENSJON/Svein.Grude" of Organization "Tekla Corporation"
  Owner history of Person "Undefined" id "DIMENSJON/Svein.Grude" of Organization "Tekla Corporation" | application "Tekla Structures" version "18.0" identifier "Multi material modeling" by Organization "Tekla Corporation" | change NOCHANGE | created 1379572968 (2013-09-19T06:42:48Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  MASSUNIT: KILO GRAM
  TIMEUNIT: SECOND
  PLANEANGLEUNIT: RADIAN
  SOLIDANGLEUNIT: STERADIAN
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  LUMINOUSINTENSITYUNIT: LUMEN

Spatial structure
IFCPROJECT "20672"
  IFCSITE "1103_54_1060" | elevation above sea level 0.
    IFCBUILDING "Bygg 4"
      IFCBUILDINGSTOREY "Undefined" | elevation 0.
        contains 8 elements
          8 x IFCPLATE | type IFCPLATETYPE "PL15*300" | object type "PL15*300" | names: "SBKL300x300" | descriptions: "PL15*300" | material: "STEEL/Steel_Undefined" | property sets: Tekla Common, Tekla Quantity
      IFCBUILDINGSTOREY "01" | elevation 0.
        contains 149 elements
          2 x IFCPLATE | type IFCPLATETYPE "25*200" | object type "25*200" | names: "=MINERALULL" | descriptions: "25*200" | material: "/=MINERALULL" | property sets: Tekla Common, Tekla Quantity
          8 x IFCPLATE | type IFCPLATETYPE "25*100" | object type "25*100" | names: "=MINERALULL" | descriptions: "25*100" | material: "/=MINERALULL" | property sets: Tekla Common, Tekla Quantity
          6 x IFCPLATE | type IFCPLATETYPE "25*150" | object type "25*150" | names: "=MINERALULL" | descriptions: "25*150" | material: "/=MINERALULL" | property sets: Tekla Common, Tekla Quantity
          12 x IFCPLATE | type IFCPLATETYPE "25*130" | object type "25*130" | names: "=MINERALULL" | descriptions: "25*130" | material: "/=MINERALULL" | property sets: Tekla Common, Tekla Quantity
          12 x IFCPLATE | type IFCPLATETYPE "25*80" | object type "25*80" | names: "=MINERALULL" | descriptions: "25*80" | material: "/=MINERALULL" | property sets: Tekla Common, Tekla Quantity
          70 x IFCBUILDINGELEMENTPART | object type "PL50*15" | names: "BETONGTRAPP" | descriptions: "PL50*15" | material: "CONCRETE/B35" | property sets: Tekla Common, Tekla Quantity
          1 x IFCBUILDINGELEMENTPART | object type "PL1185*356" | names: "BETONGTRAPP" | descriptions: "PL1185*356" | material: "CONCRETE/B35" | property sets: Tekla Common, Tekla Quantity
          7 x IFCPLATE | type IFCPLATETYPE "PL12*200" | object type "PL12*200" | names: "SBKL200x200" | descriptions: "PL12*200" | material: "STEEL/Steel_Undefined" | property sets: Tekla Common, Tekla Quantity
          3 x IFCBEAM | type IFCBEAMTYPE "PL20*250" | object type "PL20*250" | names: "STÅLBJELKE" | descriptions: "PL20*250" | material: "STEEL/S355J0" | property sets: Tekla Common, Tekla Quantity
          3 x IFCBEAM | type IFCBEAMTYPE "PL20*284" | object type "PL20*284" | names: "STÅLBJELKE" | descriptions: "PL20*284" | material: "STEEL/S355J0" | property sets: Tekla Common, Tekla Quantity
          2 x IFCWALL | type IFCWALLTYPE "3020*250" | object type "3020*250" | names: "BETONGVEGG" | descriptions: "3020*250" | material: "CONCRETE/B35" | property sets: Tekla Common, Tekla Quantity
          1 x IFCWALL | type IFCWALLTYPE "3270*200" | object type "3270*200" | names: "BETONGVEGG" | descriptions: "3270*200" | material: "CONCRETE/B35" | property sets: Tekla Common, Tekla Quantity
          1 x IFCWALL | type IFCWALLTYPE "3270*250" | object type "3270*250" | names: "BETONGVEGG" | descriptions: "3270*250" | material: "CONCRETE/B35" | property sets: Tekla Common, Tekla Quantity
          1 x IFCWALL | type IFCWALLTYPE "3300*200" | object type "3300*200" | names: "BETONGVEGG" | descriptions: "3300*200" | material: "CONCRETE/B35" | property sets: Tekla Common, Tekla Quantity
          5 x IFCWALL | type IFCWALLTYPE "3020*220" | object type "3020*220" | names: "BETONGVEGG" | descriptions: "3020*220" | material: "CONCRETE/B35" | property sets: Tekla Common, Tekla Quantity
          1 x IFCWALL | type IFCWALLTYPE "3020*200" | object type "3020*200" | names: "BETONGVEGG" | descriptions: "3020*200" | material: "CONCRETE/B35" | property sets: Tekla Common, Tekla Quantity
          1 x IFCSLAB | type IFCSLABTYPE "250*9081" | object type "250*9081" | FLOOR | names: "BETONGDEKKE" | descriptions: "250*9081" | material: "CONCRETE/B35" | property sets: Tekla Common, Tekla Quantity
          1 x IFCSLAB | type IFCSLABTYPE "250*14291" | object type "250*14291" | FLOOR | names: "BETONGDEKKE" | descriptions: "250*14291" | material: "CONCRETE/B35" | property sets: Tekla Common, Tekla Quantity
          2 x IFCCOLUMN | type IFCCOLUMNTYPE "CFRHS100X8" | object type "CFRHS100X8" | names: "STÅLSØYLE" | descriptions: "CFRHS100X8" | material: "STEEL/S355J0" | property sets: Tekla Common, Tekla Quantity
          5 x IFCCOLUMN | type IFCCOLUMNTYPE "CFRHS80X6" | object type "CFRHS80X6" | names: "STÅLSØYLE" | descriptions: "CFRHS80X6" | material: "STEEL/S355J0" | property sets: Tekla Common, Tekla Quantity
          1 x IFCBEAM | type IFCBEAMTYPE "CFRHS80X6" | object type "CFRHS80X6" | names: "STÅLSØYLE" | descriptions: "CFRHS80X6" | material: "STEEL/S355J0" | property sets: Tekla Common, Tekla Quantity
          1 x IFCBEAM | type IFCBEAMTYPE "CFRHS100X8" | object type "CFRHS100X8" | names: "STÅLSØYLE" | descriptions: "CFRHS100X8" | material: "STEEL/S355J0" | property sets: Tekla Common, Tekla Quantity
          1 x IFCBEAM | type IFCBEAMTYPE "CFRHS150X100X8" | object type "CFRHS150X100X8" | names: "STÅLSØYLE" | descriptions: "CFRHS150X100X8" | material: "STEEL/S355J0" | property sets: Tekla Common, Tekla Quantity
          1 x IFCWALL | type IFCWALLTYPE "650*200" | object type "650*200" | names: "BETONGVEGG" | descriptions: "650*200" | material: "CONCRETE/B35" | property sets: Tekla Common, Tekla Quantity
          1 x IFCSLAB | type IFCSLABTYPE "200*2752" | object type "200*2752" | FLOOR | names: "BETONGDEKKE" | descriptions: "200*2752" | material: "CONCRETE/B35" | property sets: Tekla Common, Tekla Quantity
      IFCBUILDINGSTOREY "02" | elevation 0.
        contains 203 elements
          2 x IFCPLATE | type IFCPLATETYPE "25*150" | object type "25*150" | names: "=MINERALULL" | descriptions: "25*150" | material: "/=MINERALULL" | property sets: Tekla Common, Tekla Quantity
          2 x IFCPLATE | type IFCPLATETYPE "25*100" | object type "25*100" | names: "=MINERALULL" | descriptions: "25*100" | material: "/=MINERALULL" | property sets: Tekla Common, Tekla Quantity
          18 x IFCPLATE | type IFCPLATETYPE "25*130" | object type "25*130" | names: "=MINERALULL" | descriptions: "25*130" | material: "/=MINERALULL" | property sets: Tekla Common, Tekla Quantity
          22 x IFCPLATE | type IFCPLATETYPE "25*80" | object type "25*80" | names: "=MINERALULL" | descriptions: "25*80" | material: "/=MINERALULL" | property sets: Tekla Common, Tekla Quantity
          4 x IFCPLATE | type IFCPLATETYPE "25*170" | object type "25*170" | names: "=MINERALULL" | descriptions: "25*170" | material: "/=MINERALULL" | property sets: Tekla Common, Tekla Quantity
          72 x IFCBUILDINGELEMENTPART | object type "PL50*15" | names: "BETONGTRAPP" | descriptions: "PL50*15" | material: "CONCRETE/B35" | property sets: Tekla Common, Tekla Quantity
          2 x IFCBUILDINGELEMENTPART | object type "PL1235*336" | names: "BETONGTRAPP" | descriptions: "PL1235*336" | material: "CONCRETE/B35" | property sets: Tekla Common, Tekla Quantity
          4 x IFCBEAM | type IFCBEAMTYPE "50*3" | object type "50*3" | names: "RVK 41" | descriptions: "50*3" | material: "STEEL/Steel_Undefined" | property sets: Tekla Common, Tekla Quantity
          8 x IFCBEAM | type IFCBEAMTYPE "D12" | object type "D12" | names: "RVK 41" | descriptions: "D12" | material: "STEEL/Steel_Undefined" | property sets: Tekla Common, Tekla Quantity
          4 x IFCPLATE | type IFCPLATETYPE "PL4*90" | object type "PL4*90" | names: "RVK 41" | descriptions: "PL4*90" | material: "STEEL/Steel_Undefined" | property sets: Tekla Common, Tekla Quantity
          4 x IFCBEAM | type IFCBEAMTYPE "P50*80*4" | object type "P50*80*4" | names: "RVK 41" | descriptions: "P50*80*4" | material: "STEEL/Steel_Undefined" | property sets: Tekla Common, Tekla Quantity
          4 x IFCBEAM | type IFCBEAMTYPE "P40*70*4" | object type "P40*70*4" | names: "RVK 41" | descriptions: "P40*70*4" | material: "STEEL/Steel_Undefined" | property sets: Tekla Common, Tekla Quantity
          19 x IFCBEAM | type IFCBEAMTYPE "PL20*250" | object type "PL20*250" | names: "STÅLBJELKE" | descriptions: "PL20*250" | material: "STEEL/S355J0" | property sets: Tekla Common, Tekla Quantity
          1 x IFCBEAM | type IFCBEAMTYPE "PL20*284" | object type "PL20*284" | names: "STÅLBJELKE" | descriptions: "PL20*284" | material: "STEEL/S355J0" | property sets: Tekla Common, Tekla Quantity
          2 x IFCPLATE | type IFCPLATETYPE "PL12*150" | object type "PL12*150" | names: "SBKL150x150" | descriptions: "PL12*150" | material: "STEEL/Steel_Undefined" | property sets: Tekla Common, Tekla Quantity
          3 x IFCWALL | type IFCWALLTYPE "2650*250" | object type "2650*250" | names: "BETONGVEGG" | descriptions: "2650*250" | material: "CONCRETE/B35" | property sets: Tekla Common, Tekla Quantity
          2 x IFCWALL | type IFCWALLTYPE "2900*200" | object type "2900*200" | names: "BETONGVEGG" | descriptions: "2900*200" | material: "CONCRETE/B35" | property sets: Tekla Common, Tekla Quantity
          1 x IFCWALL | type IFCWALLTYPE "2900*250" | object type "2900*250" | names: "BETONGVEGG" | descriptions: "2900*250" | material: "CONCRETE/B35" | property sets: Tekla Common, Tekla Quantity
          6 x IFCWALL | type IFCWALLTYPE "2650*220" | object type "2650*220" | names: "BETONGVEGG" | descriptions: "2650*220" | material: "CONCRETE/B35" | property sets: Tekla Common, Tekla Quantity
          1 x IFCSLAB | type IFCSLABTYPE "250*9138" | object type "250*9138" | FLOOR | names: "BETONGDEKKE" | descriptions: "250*9138" | material: "CONCRETE/B35" | property sets: Tekla Common, Tekla Quantity
          1 x IFCSLAB | type IFCSLABTYPE "250*14016" | object type "250*14016" | FLOOR | names: "BETONGDEKKE" | descriptions: "250*14016" | material: "CONCRETE/B35" | property sets: Tekla Common, Tekla Quantity
          1 x IFCWALL | type IFCWALLTYPE "2650*200" | object type "2650*200" | names: "BETONGVEGG" | descriptions: "2650*200" | material: "CONCRETE/B35" | property sets: Tekla Common, Tekla Quantity
          2 x IFCCOLUMN | type IFCCOLUMNTYPE "CFRHS120X80X8" | object type "CFRHS120X80X8" | names: "STÅLSØYLE" | descriptions: "CFRHS120X80X8" | material: "STEEL/S355J0" | property sets: Tekla Common, Tekla Quantity
          7 x IFCCOLUMN | type IFCCOLUMNTYPE "CFRHS80X6" | object type "CFRHS80X6" | names: "STÅLSØYLE" | descriptions: "CFRHS80X6" | material: "STEEL/S355J0" | property sets: Tekla Common, Tekla Quantity
          2 x IFCBEAM | type IFCBEAMTYPE "CFRHS80X6" | object type "CFRHS80X6" | names: "STÅLSØYLE" | descriptions: "CFRHS80X6" | material: "STEEL/S355J0" | property sets: Tekla Common, Tekla Quantity
          1 x IFCBEAM | type IFCBEAMTYPE "CFRHS100X10" | object type "CFRHS100X10" | names: "STÅLSØYLE" | descriptions: "CFRHS100X10" | material: "STEEL/S355J0" | property sets: Tekla Common, Tekla Quantity
          1 x IFCWALL | type IFCWALLTYPE "650*200" | object type "650*200" | names: "BETONGVEGG" | descriptions: "650*200" | material: "CONCRETE/B35" | property sets: Tekla Common, Tekla Quantity
          1 x IFCSLAB | type IFCSLABTYPE "200*1840" | object type "200*1840" | FLOOR | names: "BETONGDEKKE" | descriptions: "200*1840" | material: "CONCRETE/B35" | property sets: Tekla Common, Tekla Quantity
          1 x IFCSLAB | type IFCSLABTYPE "200*1455" | object type "200*1455" | FLOOR | names: "BETONGDEKKE" | descriptions: "200*1455" | material: "CONCRETE/B35" | property sets: Tekla Common, Tekla Quantity
          2 x IFCBEAM | type IFCBEAMTYPE "50*15" | object type "50*15" | names: "BETONGBJELKE" | descriptions: "50*15" | material: "CONCRETE/B55" | property sets: Tekla Common, Tekla Quantity
          3 x IFCSLAB | type IFCSLABTYPE "170*80" | object type "170*80" | FLOOR | names: "MINERALULL" | descriptions: "170*80" | material: "MISCELLANEOUS/MINERALULL" | property sets: Tekla Common, Tekla Quantity
      IFCBUILDINGSTOREY "03" | elevation 0.
        contains 196 elements
          2 x IFCPLATE | type IFCPLATETYPE "25*170" | object type "25*170" | names: "=MINERALULL" | descriptions: "25*170" | material: "/=MINERALULL" | property sets: Tekla Common, Tekla Quantity
          24 x IFCPLATE | type IFCPLATETYPE "25*80" | object type "25*80" | names: "=MINERALULL" | descriptions: "25*80" | material: "/=MINERALULL" | property sets: Tekla Common, Tekla Quantity
          22 x IFCPLATE | type IFCPLATETYPE "25*130" | object type "25*130" | names: "=MINERALULL" | descriptions: "25*130" | material: "/=MINERALULL" | property sets: Tekla Common, Tekla Quantity
          71 x IFCBUILDINGELEMENTPART | object type "PL50*15" | names: "BETONGTRAPP" | descriptions: "PL50*15" | material: "CONCRETE/B35" | property sets: Tekla Common, Tekla Quantity
          2 x IFCBUILDINGELEMENTPART | object type "PL1235*336" | names: "BETONGTRAPP" | descriptions: "PL1235*336" | material: "CONCRETE/B35" | property sets: Tekla Common, Tekla Quantity
          4 x IFCBEAM | type IFCBEAMTYPE "50*3" | object type "50*3" | names: "RVK 41" | descriptions: "50*3" | material: "STEEL/Steel_Undefined" | property sets: Tekla Common, Tekla Quantity
          8 x IFCBEAM | type IFCBEAMTYPE "D12" | object type "D12" | names: "RVK 41" | descriptions: "D12" | material: "STEEL/Steel_Undefined" | property sets: Tekla Common, Tekla Quantity
          4 x IFCPLATE | type IFCPLATETYPE "PL4*90" | object type "PL4*90" | names: "RVK 41" | descriptions: "PL4*90" | material: "STEEL/Steel_Undefined" | property sets: Tekla Common, Tekla Quantity
          4 x IFCBEAM | type IFCBEAMTYPE "P50*80*4" | object type "P50*80*4" | names: "RVK 41" | descriptions: "P50*80*4" | material: "STEEL/Steel_Undefined" | property sets: Tekla Common, Tekla Quantity
          4 x IFCBEAM | type IFCBEAMTYPE "P40*70*4" | object type "P40*70*4" | names: "RVK 41" | descriptions: "P40*70*4" | material: "STEEL/Steel_Undefined" | property sets: Tekla Common, Tekla Quantity
          16 x IFCBEAM | type IFCBEAMTYPE "PL20*250" | object type "PL20*250" | names: "STÅLBJELKE" | descriptions: "PL20*250" | material: "STEEL/S355J0" | property sets: Tekla Common, Tekla Quantity
          1 x IFCSLAB | type IFCSLABTYPE "250*9138" | object type "250*9138" | FLOOR | names: "BETONGDEKKE" | descriptions: "250*9138" | material: "CONCRETE/B35" | property sets: Tekla Common, Tekla Quantity
          1 x IFCSLAB | type IFCSLABTYPE "250*13772" | object type "250*13772" | FLOOR | names: "BETONGDEKKE" | descriptions: "250*13772" | material: "CONCRETE/B35" | property sets: Tekla Common, Tekla Quantity
          1 x IFCWALL | type IFCWALLTYPE "2650*200" | object type "2650*200" | names: "BETONGVEGG" | descriptions: "2650*200" | material: "CONCRETE/B35" | property sets: Tekla Common, Tekla Quantity
          6 x IFCWALL | type IFCWALLTYPE "2650*220" | object type "2650*220" | names: "BETONGVEGG" | descriptions: "2650*220" | material: "CONCRETE/B35" | property sets: Tekla Common, Tekla Quantity
          3 x IFCWALL | type IFCWALLTYPE "2650*250" | object type "2650*250" | names: "BETONGVEGG" | descriptions: "2650*250" | material: "CONCRETE/B35" | property sets: Tekla Common, Tekla Quantity
          2 x IFCWALL | type IFCWALLTYPE "2900*200" | object type "2900*200" | names: "BETONGVEGG" | descriptions: "2900*200" | material: "CONCRETE/B35" | property sets: Tekla Common, Tekla Quantity
          1 x IFCWALL | type IFCWALLTYPE "2900*250" | object type "2900*250" | names: "BETONGVEGG" | descriptions: "2900*250" | material: "CONCRETE/B35" | property sets: Tekla Common, Tekla Quantity
          9 x IFCCOLUMN | type IFCCOLUMNTYPE "CFRHS80X6" | object type "CFRHS80X6" | names: "STÅLSØYLE" | descriptions: "CFRHS80X6" | material: "STEEL/S355J0" | property sets: Tekla Common, Tekla Quantity
          2 x IFCBEAM | type IFCBEAMTYPE "CFRHS80X6" | object type "CFRHS80X6" | names: "STÅLSØYLE" | descriptions: "CFRHS80X6" | material: "STEEL/S355J0" | property sets: Tekla Common, Tekla Quantity
          1 x IFCBEAM | type IFCBEAMTYPE "CFRHS120X80X8" | object type "CFRHS120X80X8" | names: "STÅLSØYLE" | descriptions: "CFRHS120X80X8" | material: "STEEL/S355J0" | property sets: Tekla Common, Tekla Quantity
          1 x IFCWALL | type IFCWALLTYPE "650*200" | object type "650*200" | names: "BETONGVEGG" | descriptions: "650*200" | material: "CONCRETE/B35" | property sets: Tekla Common, Tekla Quantity
          1 x IFCSLAB | type IFCSLABTYPE "200*1455" | object type "200*1455" | FLOOR | names: "BETONGDEKKE" | descriptions: "200*1455" | material: "CONCRETE/B35" | property sets: Tekla Common, Tekla Quantity
          2 x IFCBEAM | type IFCBEAMTYPE "50*15" | object type "50*15" | names: "BETONGBJELKE" | descriptions: "50*15" | material: "CONCRETE/B55" | property sets: Tekla Common, Tekla Quantity
          1 x IFCSLAB | type IFCSLABTYPE "200*1840" | object type "200*1840" | FLOOR | names: "BETONGDEKKE" | descriptions: "200*1840" | material: "CONCRETE/B35" | property sets: Tekla Common, Tekla Quantity
          3 x IFCSLAB | type IFCSLABTYPE "170*80" | object type "170*80" | FLOOR | names: "MINERALULL" | descriptions: "170*80" | material: "MISCELLANEOUS/MINERALULL" | property sets: Tekla Common, Tekla Quantity
      IFCBUILDINGSTOREY "04" | elevation 0.
        contains 54 elements
          4 x IFCPLATE | type IFCPLATETYPE "25*130" | object type "25*130" | names: "=MINERALULL" | descriptions: "25*130" | material: "/=MINERALULL" | property sets: Tekla Common, Tekla Quantity
          4 x IFCPLATE | type IFCPLATETYPE "25*80" | object type "25*80" | names: "=MINERALULL" | descriptions: "25*80" | material: "/=MINERALULL" | property sets: Tekla Common, Tekla Quantity
          1 x IFCBUILDINGELEMENTPART | object type "PL50*15" | names: "BETONGTRAPP" | descriptions: "PL50*15" | material: "CONCRETE/B35" | property sets: Tekla Common, Tekla Quantity
          20 x IFCBEAM | type IFCBEAMTYPE "PL20*250" | object type "PL20*250" | names: "STÅLBJELKE" | descriptions: "PL20*250" | material: "STEEL/S355J0" | property sets: Tekla Common, Tekla Quantity
          4 x IFCBEAM | type IFCBEAMTYPE "PL20*150" | object type "PL20*150" | names: "STÅLBJELKE" | descriptions: "PL20*150" | material: "STEEL/S355J0" | property sets: Tekla Common, Tekla Quantity
          1 x IFCSLAB | type IFCSLABTYPE "250*9138" | object type "250*9138" | FLOOR | names: "BETONGDEKKE" | descriptions: "250*9138" | material: "CONCRETE/B35" | property sets: Tekla Common, Tekla Quantity
          1 x IFCSLAB | type IFCSLABTYPE "250*13528" | object type "250*13528" | FLOOR | names: "BETONGDEKKE" | descriptions: "250*13528" | material: "CONCRETE/B35" | property sets: Tekla Common, Tekla Quantity
          1 x IFCWALL | type IFCWALLTYPE "2650*200" | object type "2650*200" | names: "BETONGVEGG" | descriptions: "2650*200" | material: "CONCRETE/B35" | property sets: Tekla Common, Tekla Quantity
          4 x IFCWALL | type IFCWALLTYPE "2650*220" | object type "2650*220" | names: "BETONGVEGG" | descriptions: "2650*220" | material: "CONCRETE/B35" | property sets: Tekla Common, Tekla Quantity
          2 x IFCWALL | type IFCWALLTYPE "2900*220" | object type "2900*220" | names: "BETONGVEGG" | descriptions: "2900*220" | material: "CONCRETE/B35" | property sets: Tekla Common, Tekla Quantity
          4 x IFCWALL | type IFCWALLTYPE "2900*250" | object type "2900*250" | names: "BETONGVEGG" | descriptions: "2900*250" | material: "CONCRETE/B35" | property sets: Tekla Common, Tekla Quantity
          2 x IFCWALL | type IFCWALLTYPE "2900*200" | object type "2900*200" | names: "BETONGVEGG" | descriptions: "2900*200" | material: "CONCRETE/B35" | property sets: Tekla Common, Tekla Quantity
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "CFRHS80X6" | object type "CFRHS80X6" | names: "STÅLSØYLE" | descriptions: "CFRHS80X6" | material: "STEEL/S355J0" | property sets: Tekla Common, Tekla Quantity
          1 x IFCBEAM | type IFCBEAMTYPE "CFRHS80X6" | object type "CFRHS80X6" | names: "STÅLSØYLE" | descriptions: "CFRHS80X6" | material: "STEEL/S355J0" | property sets: Tekla Common, Tekla Quantity
          1 x IFCSLAB | type IFCSLABTYPE "200*1620" | object type "200*1620" | FLOOR | names: "BETONGDEKKE" | descriptions: "200*1620" | material: "CONCRETE/B35" | property sets: Tekla Common, Tekla Quantity
          3 x IFCSLAB | type IFCSLABTYPE "170*80" | object type "170*80" | FLOOR | names: "MINERALULL" | descriptions: "170*80" | material: "MISCELLANEOUS/MINERALULL" | property sets: Tekla Common, Tekla Quantity
      IFCBUILDINGSTOREY "05" | elevation 0.
        contains 31 elements
          4 x IFCBEAM | type IFCBEAMTYPE "PL5*40" | object type "PL5*40" | names: "HYLSE" | descriptions: "PL5*40" | material: "STEEL/S355J0" | property sets: Tekla Common, Tekla Quantity
          4 x IFCCOLUMN | type IFCCOLUMNTYPE "D20" | object type "D20" | names: "HYLSE" | descriptions: "D20" | material: "STEEL/S355J0" | property sets: Tekla Common, Tekla Quantity
          4 x IFCCOLUMN | type IFCCOLUMNTYPE "40*40" | object type "40*40" | names: "HYLSE" | descriptions: "40*40" | material: "STEEL/S355J0" | property sets: Tekla Common, Tekla Quantity
          4 x IFCBEAM | type IFCBEAMTYPE "PL20*250" | object type "PL20*250" | names: "STÅLBJELKE" | descriptions: "PL20*250" | material: "STEEL/S355J0" | property sets: Tekla Common, Tekla Quantity
          1 x IFCWALL | type IFCWALLTYPE "5000*200" | object type "5000*200" | names: "BETONGVEGG" | descriptions: "5000*200" | material: "CONCRETE/B35" | property sets: Tekla Common, Tekla Quantity
          1 x IFCWALL | type IFCWALLTYPE "2430*220" | object type "2430*220" | names: "BETONGVEGG" | descriptions: "2430*220" | material: "CONCRETE/B35" | property sets: Tekla Common, Tekla Quantity
          1 x IFCWALL | type IFCWALLTYPE "1390*250" | object type "1390*250" | names: "BETONGVEGG" | descriptions: "1390*250" | material: "CONCRETE/B35" | property sets: Tekla Common, Tekla Quantity
          1 x IFCWALL | type IFCWALLTYPE "2700*200" | object type "2700*200" | names: "BETONGVEGG" | descriptions: "2700*200" | material: "CONCRETE/B35" | property sets: Tekla Common, Tekla Quantity
          1 x IFCWALL | type IFCWALLTYPE "2700*250" | object type "2700*250" | names: "BETONGVEGG" | descriptions: "2700*250" | material: "CONCRETE/B35" | property sets: Tekla Common, Tekla Quantity
          1 x IFCWALL | type IFCWALLTYPE "2900*200" | object type "2900*200" | names: "BETONGVEGG" | descriptions: "2900*200" | material: "CONCRETE/B35" | property sets: Tekla Common, Tekla Quantity
          1 x IFCWALL | type IFCWALLTYPE "1445*250" | object type "1445*250" | names: "BETONGVEGG" | descriptions: "1445*250" | material: "CONCRETE/B35" | property sets: Tekla Common, Tekla Quantity
          1 x IFCWALL | type IFCWALLTYPE "2900*250" | object type "2900*250" | names: "BETONGVEGG" | descriptions: "2900*250" | material: "CONCRETE/B35" | property sets: Tekla Common, Tekla Quantity
          1 x IFCWALL | type IFCWALLTYPE "1240*220" | object type "1240*220" | names: "BETONGVEGG" | descriptions: "1240*220" | material: "CONCRETE/B35" | property sets: Tekla Common, Tekla Quantity
          1 x IFCSLAB | type IFCSLABTYPE "250*9964" | object type "250*9964" | FLOOR | names: "BETONGDEKKE" | descriptions: "250*9964" | material: "CONCRETE/B35" | property sets: Tekla Common, Tekla Quantity
          1 x IFCSLAB | type IFCSLABTYPE "200*1705" | object type "200*1705" | FLOOR | names: "BETONGDEKKE" | descriptions: "200*1705" | material: "CONCRETE/B35" | property sets: Tekla Common, Tekla Quantity
          1 x IFCWALL | type IFCWALLTYPE "3000*200" | object type "3000*200" | names: "BETONGVEGG" | descriptions: "3000*200" | material: "CONCRETE/B35" | property sets: Tekla Common, Tekla Quantity
          3 x IFCSLAB | type IFCSLABTYPE "170*80" | object type "170*80" | FLOOR | names: "MINERALULL" | descriptions: "170*80" | material: "MISCELLANEOUS/MINERALULL" | property sets: Tekla Common, Tekla Quantity
      IFCBUILDINGSTOREY "06" | elevation 0.
        contains 3 elements
          3 x IFCSLAB | type IFCSLABTYPE "170*80" | object type "170*80" | FLOOR | names: "MINERALULL" | descriptions: "170*80" | material: "MISCELLANEOUS/MINERALULL" | property sets: Tekla Common, Tekla Quantity
      IFCBUILDINGSTOREY "001" | elevation 0.
        contains 1 element
          1 x IFCFOOTING | object type "1000*1000" | names: "PLASSTØPTFUNDAMENT" | descriptions: "1000*1000" | material: "CONCRETE/B35" | property sets: Tekla Common, Tekla Quantity

Types
  IFCPLATETYPE "PL15*300" | 8 occurrences
  IFCPLATETYPE "25*200" | 2 occurrences
  IFCPLATETYPE "25*100" | 10 occurrences
  IFCPLATETYPE "25*150" | 8 occurrences
  IFCPLATETYPE "25*130" | 56 occurrences
  IFCPLATETYPE "25*80" | 62 occurrences
  IFCPLATETYPE "PL12*200" | 7 occurrences
  IFCBEAMTYPE "PL20*250" | 62 occurrences
  IFCBEAMTYPE "PL20*284" | 4 occurrences
  IFCWALLTYPE "3020*250" | 2 occurrences
  IFCWALLTYPE "3270*200" | 1 occurrence
  IFCWALLTYPE "3270*250" | 1 occurrence
  IFCWALLTYPE "3300*200" | 1 occurrence
  IFCWALLTYPE "3020*220" | 5 occurrences
  IFCWALLTYPE "3020*200" | 1 occurrence
  IFCSLABTYPE "250*9081" | 1 occurrence
  IFCSLABTYPE "250*14291" | 1 occurrence
  IFCCOLUMNTYPE "CFRHS100X8" | 2 occurrences
  IFCCOLUMNTYPE "CFRHS80X6" | 22 occurrences
  IFCBEAMTYPE "CFRHS80X6" | 6 occurrences
  IFCBEAMTYPE "CFRHS100X8" | 1 occurrence
  IFCBEAMTYPE "CFRHS150X100X8" | 1 occurrence
  IFCWALLTYPE "650*200" | 3 occurrences
  IFCSLABTYPE "200*2752" | 1 occurrence
  IFCPLATETYPE "25*170" | 6 occurrences
  IFCBEAMTYPE "50*3" | 8 occurrences
  IFCBEAMTYPE "D12" | 16 occurrences
  IFCPLATETYPE "PL4*90" | 8 occurrences
  IFCBEAMTYPE "P50*80*4" | 8 occurrences
  IFCBEAMTYPE "P40*70*4" | 8 occurrences
  IFCPLATETYPE "PL12*150" | 2 occurrences
  IFCWALLTYPE "2650*250" | 6 occurrences
  IFCWALLTYPE "2900*200" | 7 occurrences
  IFCWALLTYPE "2900*250" | 7 occurrences
  IFCWALLTYPE "2650*220" | 16 occurrences
  IFCSLABTYPE "250*9138" | 3 occurrences
  IFCSLABTYPE "250*14016" | 1 occurrence
  IFCWALLTYPE "2650*200" | 3 occurrences
  IFCCOLUMNTYPE "CFRHS120X80X8" | 2 occurrences
  IFCBEAMTYPE "CFRHS100X10" | 1 occurrence
  IFCSLABTYPE "200*1840" | 2 occurrences
  IFCSLABTYPE "200*1455" | 2 occurrences
  IFCBEAMTYPE "50*15" | 4 occurrences
  IFCSLABTYPE "170*80" | 15 occurrences
  IFCSLABTYPE "250*13772" | 1 occurrence
  IFCBEAMTYPE "CFRHS120X80X8" | 1 occurrence
  IFCBEAMTYPE "PL20*150" | 4 occurrences
  IFCSLABTYPE "250*13528" | 1 occurrence
  IFCWALLTYPE "2900*220" | 2 occurrences
  IFCSLABTYPE "200*1620" | 1 occurrence
  IFCBEAMTYPE "PL5*40" | 4 occurrences
  IFCCOLUMNTYPE "D20" | 4 occurrences
  IFCCOLUMNTYPE "40*40" | 4 occurrences
  IFCWALLTYPE "5000*200" | 1 occurrence
  IFCWALLTYPE "2430*220" | 1 occurrence
  IFCWALLTYPE "1390*250" | 1 occurrence
  IFCWALLTYPE "2700*200" | 1 occurrence
  IFCWALLTYPE "2700*250" | 1 occurrence
  IFCWALLTYPE "1445*250" | 1 occurrence
  IFCWALLTYPE "1240*220" | 1 occurrence
  IFCSLABTYPE "250*9964" | 1 occurrence
  IFCSLABTYPE "200*1705" | 1 occurrence
  IFCWALLTYPE "3000*200" | 1 occurrence

Property sets
  Tekla Common | properties | on 1 object (1 IFCFOOTING)
    Assembly mark = "PF-0(?)" (IFCLABEL)
    Bottom elevation = "+2.500" (IFCLABEL)
    Center of gravity X = -5.38452718836846E-007 (IFCLENGTHMEASURE) [MILLI METRE]
    Center of gravity Y = 6.37097207064083E-007 (IFCLENGTHMEASURE) [MILLI METRE]
    Center of gravity Z = 3000.00000000001 (IFCLENGTHMEASURE) [MILLI METRE]
    Class = "260" (IFCLABEL)
    Control number (no value)
    Finish = "" (IFCLABEL)
    Grade = "B35" (IFCLABEL)
    Name = "PLASSTØPTFUNDAMENT" (IFCLABEL)
    Part mark = "Concrete-805" (IFCLABEL)
    Phase = 1 (IFCINTEGER)
    Preliminary mark = "" (IFCLABEL)
    Profile = "1000*1000" (IFCLABEL)
    Top elevation = "+3.500" (IFCLABEL)
  Tekla Common | properties | on 1 object (1 IFCSLAB)
    Assembly mark = "BD-0(?)" (IFCLABEL)
    Bottom elevation = "+20.540" (IFCLABEL)
    Center of gravity X = 112794.29547496 (IFCLENGTHMEASURE) [MILLI METRE]
    Center of gravity Y = -13914.756655764 (IFCLENGTHMEASURE) [MILLI METRE]
    Center of gravity Z = 20625. (IFCLENGTHMEASURE) [MILLI METRE]
    Class = "500" (IFCLABEL)
    Control number (no value)
    Finish = "" (IFCLABEL)
    Grade = "MINERALULL" (IFCLABEL)
    Name = "MINERALULL" (IFCLABEL)
    Part mark = "Concrete-0(?)" (IFCLABEL)
    Phase = 1 (IFCINTEGER)
    Preliminary mark = "" (IFCLABEL)
    Profile = "170*80" (IFCLABEL)
    Top elevation = "+20.710" (IFCLABEL)
  Tekla Common | properties | on 1 object (1 IFCSLAB)
    Assembly mark = "BD-0(?)" (IFCLABEL)
    Bottom elevation = "+20.540" (IFCLABEL)
    Center of gravity X = 111357.285377747 (IFCLENGTHMEASURE) [MILLI METRE]
    Center of gravity Y = -15708.0152899952 (IFCLENGTHMEASURE) [MILLI METRE]
    Center of gravity Z = 20625. (IFCLENGTHMEASURE) [MILLI METRE]
    Class = "500" (IFCLABEL)
    Control number (no value)
    Finish = "" (IFCLABEL)
    Grade = "MINERALULL" (IFCLABEL)
    Name = "MINERALULL" (IFCLABEL)
    Part mark = "Concrete-0(?)" (IFCLABEL)
    Phase = 1 (IFCINTEGER)
    Preliminary mark = "" (IFCLABEL)
    Profile = "170*80" (IFCLABEL)
    Top elevation = "+20.710" (IFCLABEL)
  Tekla Common | properties | on 1 object (1 IFCSLAB)
    Assembly mark = "BD-0(?)" (IFCLABEL)
    Bottom elevation = "+20.540" (IFCLABEL)
    Center of gravity X = 109920.520486333 (IFCLENGTHMEASURE) [MILLI METRE]
    Center of gravity Y = -17501.4473356072 (IFCLENGTHMEASURE) [MILLI METRE]
    Center of gravity Z = 20625. (IFCLENGTHMEASURE) [MILLI METRE]
    Class = "500" (IFCLABEL)
    Control number (no value)
    Finish = "" (IFCLABEL)
    Grade = "MINERALULL" (IFCLABEL)
    Name = "MINERALULL" (IFCLABEL)
    Part mark = "Concrete-0(?)" (IFCLABEL)
    Phase = 1 (IFCINTEGER)
    Preliminary mark = "" (IFCLABEL)
    Profile = "170*80" (IFCLABEL)
    Top elevation = "+20.710" (IFCLABEL)
  Tekla Common | properties | on 1 object (1 IFCSLAB)
    Assembly mark = "BD-0(?)" (IFCLABEL)
    Bottom elevation = "+17.640" (IFCLABEL)
    Center of gravity X = 112794.29547496 (IFCLENGTHMEASURE) [MILLI METRE]
    Center of gravity Y = -13914.756655764 (IFCLENGTHMEASURE) [MILLI METRE]
    Center of gravity Z = 17725. (IFCLENGTHMEASURE) [MILLI METRE]
    Class = "500" (IFCLABEL)
    Control number (no value)
    Finish = "" (IFCLABEL)
    Grade = "MINERALULL" (IFCLABEL)
    Name = "MINERALULL" (IFCLABEL)
    Part mark = "Concrete-0(?)" (IFCLABEL)
    Phase = 1 (IFCINTEGER)
    Preliminary mark = "" (IFCLABEL)
    Profile = "170*80" (IFCLABEL)
    Top elevation = "+17.810" (IFCLABEL)
  Tekla Common | properties | on 1 object (1 IFCSLAB)
    Assembly mark = "BD-0(?)" (IFCLABEL)
    Bottom elevation = "+17.640" (IFCLABEL)
    Center of gravity X = 111357.285377747 (IFCLENGTHMEASURE) [MILLI METRE]
    Center of gravity Y = -15708.0152899952 (IFCLENGTHMEASURE) [MILLI METRE]
    Center of gravity Z = 17725. (IFCLENGTHMEASURE) [MILLI METRE]
    Class = "500" (IFCLABEL)
    Control number (no value)
    Finish = "" (IFCLABEL)
    Grade = "MINERALULL" (IFCLABEL)
    Name = "MINERALULL" (IFCLABEL)
    Part mark = "Concrete-0(?)" (IFCLABEL)
    Phase = 1 (IFCINTEGER)
    Preliminary mark = "" (IFCLABEL)
    Profile = "170*80" (IFCLABEL)
    Top elevation = "+17.810" (IFCLABEL)
  Tekla Common | properties | on 1 object (1 IFCSLAB)
    Assembly mark = "BD-0(?)" (IFCLABEL)
    Bottom elevation = "+17.640" (IFCLABEL)
    Center of gravity X = 109920.520486333 (IFCLENGTHMEASURE) [MILLI METRE]
    Center of gravity Y = -17501.4473356072 (IFCLENGTHMEASURE) [MILLI METRE]
    Center of gravity Z = 17725. (IFCLENGTHMEASURE) [MILLI METRE]
    Class = "500" (IFCLABEL)
    Control number (no value)
    Finish = "" (IFCLABEL)
    Grade = "MINERALULL" (IFCLABEL)
    Name = "MINERALULL" (IFCLABEL)
    Part mark = "Concrete-0(?)" (IFCLABEL)
    Phase = 1 (IFCINTEGER)
    Preliminary mark = "" (IFCLABEL)
    Profile = "170*80" (IFCLABEL)
    Top elevation = "+17.810" (IFCLABEL)
  Tekla Common | properties | on 1 object (1 IFCSLAB)
    Assembly mark = "BD-0(?)" (IFCLABEL)
    Bottom elevation = "+14.740" (IFCLABEL)
    Center of gravity X = 112794.29547496 (IFCLENGTHMEASURE) [MILLI METRE]
    Center of gravity Y = -13914.756655764 (IFCLENGTHMEASURE) [MILLI METRE]
    Center of gravity Z = 14825. (IFCLENGTHMEASURE) [MILLI METRE]
    Class = "500" (IFCLABEL)
    Control number (no value)
    Finish = "" (IFCLABEL)
    Grade = "MINERALULL" (IFCLABEL)
    Name = "MINERALULL" (IFCLABEL)
    Part mark = "Concrete-0(?)" (IFCLABEL)
    Phase = 1 (IFCINTEGER)
    Preliminary mark = "" (IFCLABEL)
    Profile = "170*80" (IFCLABEL)
    Top elevation = "+14.910" (IFCLABEL)
  Tekla Common: 637 more contents on 637 objects not shown
  Tekla Quantity | properties | on 5 objects (5 IFCSLAB)
    Area per tons = 2035.13911830818 (IFCAREAMEASURE) [SQUARE_METRE]
    Gross area = 0.0401458889209116 (IFCAREAMEASURE) [SQUARE_METRE]
    Gross footprint area = 0.039930477891101 (IFCAREAMEASURE) [SQUARE_METRE]
    Gross volume = 0.00678818124151753 (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Gross weight = 0.136496022331099 (IFCMASSMEASURE) [KILO GRAM]
    Height = 80.2911859986489 (IFCLENGTHMEASURE) [MILLI METRE]
    Length = 500.003685604883 (IFCLENGTHMEASURE) [MILLI METRE]
    Net surface area = 0.276297863735561 (IFCAREAMEASURE) [SQUARE_METRE]
    Net volume = 0.00678818124151753 (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Net weight = 0.135763624830351 (IFCMASSMEASURE) [KILO GRAM]
    Weight = 0.135763624830351 (IFCMASSMEASURE) [KILO GRAM]
    Weight per unit length (no value)
    Width = 170. (IFCLENGTHMEASURE) [MILLI METRE]
  Tekla Quantity | properties | on 5 objects (5 IFCSLAB)
    Area per tons = 2035.13911830816 (IFCAREAMEASURE) [SQUARE_METRE]
    Gross area = 0.040145888920925 (IFCAREAMEASURE) [SQUARE_METRE]
    Gross footprint area = 0.039930477891101 (IFCAREAMEASURE) [SQUARE_METRE]
    Gross volume = 0.00678818124151776 (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Gross weight = 0.136496022331145 (IFCMASSMEASURE) [KILO GRAM]
    Height = 80.291185998678 (IFCLENGTHMEASURE) [MILLI METRE]
    Length = 500.003685604868 (IFCLENGTHMEASURE) [MILLI METRE]
    Net surface area = 0.276297863735569 (IFCAREAMEASURE) [SQUARE_METRE]
    Net volume = 0.00678818124151776 (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Net weight = 0.135763624830355 (IFCMASSMEASURE) [KILO GRAM]
    Weight = 0.135763624830355 (IFCMASSMEASURE) [KILO GRAM]
    Weight per unit length (no value)
    Width = 170. (IFCLENGTHMEASURE) [MILLI METRE]
  Tekla Quantity | properties | on 5 objects (5 IFCSLAB)
    Area per tons = 2035.13911830978 (IFCAREAMEASURE) [SQUARE_METRE]
    Gross area = 0.040145888920854 (IFCAREAMEASURE) [SQUARE_METRE]
    Gross footprint area = 0.039930477891101 (IFCAREAMEASURE) [SQUARE_METRE]
    Gross volume = 0.00678818124150025 (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Gross weight = 0.136496022330904 (IFCMASSMEASURE) [KILO GRAM]
    Height = 80.2911859986634 (IFCLENGTHMEASURE) [MILLI METRE]
    Length = 500.003685604075 (IFCLENGTHMEASURE) [MILLI METRE]
    Net surface area = 0.276297863735076 (IFCAREAMEASURE) [SQUARE_METRE]
    Net volume = 0.00678818124150025 (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Net weight = 0.135763624830005 (IFCMASSMEASURE) [KILO GRAM]
    Weight = 0.135763624830005 (IFCMASSMEASURE) [KILO GRAM]
    Weight per unit length (no value)
    Width = 170. (IFCLENGTHMEASURE) [MILLI METRE]
  Tekla Quantity | properties | on 3 objects (3 IFCWALL)
    Area per tons = 4.75706348195041 (IFCAREAMEASURE) [SQUARE_METRE]
    Gross area = 18.2094266553803 (IFCAREAMEASURE) [SQUARE_METRE]
    Gross footprint area = 0.549981505014489 (IFCAREAMEASURE) [SQUARE_METRE]
    Gross volume = 1.59494636453699 (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Gross weight = 3827.87127506319 (IFCMASSMEASURE) [KILO GRAM]
    Height = 2900. (IFCLENGTHMEASURE) [MILLI METRE]
    Length = 2749.90752506112 (IFCLENGTHMEASURE) [MILLI METRE]
    Net surface area = 18.2094266553803 (IFCAREAMEASURE) [SQUARE_METRE]
    Net volume = 1.59494636453699 (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Net weight = 3827.87127488878 (IFCMASSMEASURE) [KILO GRAM]
    Weight = 3827.87127488878 (IFCMASSMEASURE) [KILO GRAM]
    Weight per unit length (no value)
    Width = 200.000000009306 (IFCLENGTHMEASURE) [MILLI METRE]
  Tekla Quantity | properties | on 3 objects (3 IFCBUILDINGELEMENTPART)
    Area per tons = 75.0177063690501 (IFCAREAMEASURE) [SQUARE_METRE]
    Gross area = 0.00450000000001198 (IFCAREAMEASURE) [SQUARE_METRE]
    Gross footprint area = 0.0149120697021472 (IFCAREAMEASURE) [SQUARE_METRE]
    Gross volume = 0.000224340522765092 (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Gross weight = 0.540000000032555 (IFCMASSMEASURE) [KILO GRAM]
    Height = 15. (IFCLENGTHMEASURE) [MILLI METRE]
    Length = 300.000000000799 (IFCLENGTHMEASURE) [MILLI METRE]
    Net surface area = 0.0403908275123301 (IFCAREAMEASURE) [SQUARE_METRE]
    Net volume = 0.000224340522765092 (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Net weight = 0.538417254636221 (IFCMASSMEASURE) [KILO GRAM]
    Weight = 0.538417254636221 (IFCMASSMEASURE) [KILO GRAM]
    Weight per unit length (no value)
    Width = 50.0000000028813 (IFCLENGTHMEASURE) [MILLI METRE]
  Tekla Quantity | properties | on 3 objects (3 IFCBUILDINGELEMENTPART)
    Area per tons = 75.0177063690524 (IFCAREAMEASURE) [SQUARE_METRE]
    Gross area = 0.00450000000000363 (IFCAREAMEASURE) [SQUARE_METRE]
    Gross footprint area = 0.0149120697021487 (IFCAREAMEASURE) [SQUARE_METRE]
    Gross volume = 0.000224340522765514 (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Gross weight = 0.540000000005465 (IFCMASSMEASURE) [KILO GRAM]
    Height = 15. (IFCLENGTHMEASURE) [MILLI METRE]
    Length = 300.000000000242 (IFCLENGTHMEASURE) [MILLI METRE]
    Net surface area = 0.0403908275124073 (IFCAREAMEASURE) [SQUARE_METRE]
    Net volume = 0.000224340522765514 (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Net weight = 0.538417254637233 (IFCMASSMEASURE) [KILO GRAM]
    Weight = 0.538417254637233 (IFCMASSMEASURE) [KILO GRAM]
    Weight per unit length (no value)
    Width = 50.0000000004657 (IFCLENGTHMEASURE) [MILLI METRE]
  Tekla Quantity | properties | on 3 objects (3 IFCBUILDINGELEMENTPART)
    Area per tons = 75.0177063690523 (IFCAREAMEASURE) [SQUARE_METRE]
    Gross area = 0.00450000000000363 (IFCAREAMEASURE) [SQUARE_METRE]
    Gross footprint area = 0.0149120697021487 (IFCAREAMEASURE) [SQUARE_METRE]
    Gross volume = 0.000224340522765515 (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Gross weight = 0.540000000005465 (IFCMASSMEASURE) [KILO GRAM]
    Height = 15. (IFCLENGTHMEASURE) [MILLI METRE]
    Length = 300.000000000242 (IFCLENGTHMEASURE) [MILLI METRE]
    Net surface area = 0.0403908275124074 (IFCAREAMEASURE) [SQUARE_METRE]
    Net volume = 0.000224340522765515 (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Net weight = 0.538417254637236 (IFCMASSMEASURE) [KILO GRAM]
    Weight = 0.538417254637236 (IFCMASSMEASURE) [KILO GRAM]
    Weight per unit length (no value)
    Width = 50.0000000004657 (IFCLENGTHMEASURE) [MILLI METRE]
  Tekla Quantity | properties | on 3 objects (3 IFCBUILDINGELEMENTPART)
    Area per tons = 75.0177063690529 (IFCAREAMEASURE) [SQUARE_METRE]
    Gross area = 0.00450000000000363 (IFCAREAMEASURE) [SQUARE_METRE]
    Gross footprint area = 0.0149120697021487 (IFCAREAMEASURE) [SQUARE_METRE]
    Gross volume = 0.000224340522765526 (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Gross weight = 0.540000000005465 (IFCMASSMEASURE) [KILO GRAM]
    Height = 15. (IFCLENGTHMEASURE) [MILLI METRE]
    Length = 300.000000000242 (IFCLENGTHMEASURE) [MILLI METRE]
    Net surface area = 0.0403908275124097 (IFCAREAMEASURE) [SQUARE_METRE]
    Net volume = 0.000224340522765526 (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Net weight = 0.538417254637262 (IFCMASSMEASURE) [KILO GRAM]
    Weight = 0.538417254637262 (IFCMASSMEASURE) [KILO GRAM]
    Weight per unit length (no value)
    Width = 50.0000000004657 (IFCLENGTHMEASURE) [MILLI METRE]
  Tekla Quantity: 603 more contents on 615 objects not shown