IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView_V2.0]"
File name: "20672_RIE_Vannkanten_B6.ifc"
Time stamp: "2014-04-08T15:35:38"
Author: "STEEL"
Organization: "Data Design System ASA"
Preprocessor: "DDS-IFC v2.0"
Originating system: "DDS-CAD Version 8.0 Win32 build 23/4-2013"
Authorization: "DDS"
Application: "DDS-CAD MEP" version "Version 8.0 Win32 build 23/4-2013" identifier "DDS-CAD MEP Version 8.0 Win32 build 23/4-2013" by Organization "Norconsult"

People and organizations
  3 x Person "steel" of Organization "Norconsult"
  2 x Owner history of Person "steel" of Organization "Norconsult" | application "DDS-CAD MEP" version "Version 8.0 Win32 build 23/4-2013" identifier "DDS-CAD MEP Version 8.0 Win32 build 23/4-2013" by Organization "Norconsult" | change NOCHANGE | created 1396964133 (2014-04-08T13:35:33Z)
  Owner history of Person "steel" of Organization "Norconsult" | application "DDS-CAD MEP" version "Version 8.0 Win32 build 23/4-2013" identifier "DDS-CAD MEP Version 8.0 Win32 build 23/4-2013" by Organization "Norconsult" | change NOCHANGE | created 1396964134 (2014-04-08T13:35:34Z)

Units
  LENGTHUNIT: METRE
  AREAUNIT: SQUARE_METRE
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  ELECTRICRESISTANCEUNIT: OHM
  POWERUNIT: WATT
  MASSUNIT: GRAM
  SOLIDANGLEUNIT: STERADIAN
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  PRESSUREUNIT: PASCAL
  LUMINOUSFLUXUNIT: LUMEN
  ILLUMINANCEUNIT: LUX
  FREQUENCYUNIT: HERTZ
  VOLUMEUNIT: CUBIC_METRE
  TIMEUNIT: SECOND
  VOLUMETRICFLOWRATEUNIT: derived
  THERMALTRANSMITTANCEUNIT: derived
  PLANEANGLEUNIT: DEGREE (conversion based)

Spatial structure
IFCPROJECT "2006117" | long name "SIRISKJÆR" | phase "Detailprojekt" | description "VANNKANTEN - B6"
  IFCSITE "Default" | latitude 58° 58′ 9.491271″ | longitude 5° 45′ 41.603851″ | elevation above sea level 2.5
    IFCBUILDING
      IFCBUILDINGSTOREY "00U" | elevation -3.74 | description "00U"
        contains 1 element
          1 x IFCBUILDINGELEMENTPROXY
      IFCBUILDINGSTOREY "01" | elevation 0. | description "01"
        contains 156 elements
          2 x IFCFLOWTERMINAL | type IFCOUTLETTYPE "E2_6950710_1010_100_010101_3_00" | names: "143", "151" | property sets: Pset_DDS
          2 x IFCFLOWTERMINAL | type IFCOUTLETTYPE "E2_6950710-_1011_100_010101_3_00" | names: "159", "167" | property sets: Pset_DDS
          4 x IFCFLOWTERMINAL | type IFCOUTLETTYPE "SK_1502164_1009_003_010101_3_0" | names: "175", "188", "201" (+1 more) | property sets: Pset_DDS
          49 x IFCFLOWTERMINAL | type IFCOUTLETTYPE "SK_1502134_1006_002_010101_3_0" | names: "227", "235", "243" (+46 more) | property sets: Pset_DDS
          8 x IFCFLOWTERMINAL | type IFCOUTLETTYPE "SK_1502102_1044_001_200101_3_0" | names: "379", "394", "409" (+5 more) | property sets: Pset_DDS
          2 x IFCFLOWTERMINAL | type IFCOUTLETTYPE "SK_1416000-_1007_013_010101_3_0" | names: "439", "647" | property sets: Pset_DDS
          6 x IFCFLOWTERMINAL | type IFCLIGHTFIXTURETYPE "LI_1513013_1005_202_010101_3_0021206000.5" | names: "945", "955", "985" (+3 more) | property sets: Pset_DDS
          5 x IFCFLOWTERMINAL | type IFCLIGHTFIXTURETYPE "LI_LI-090312092105_1004_202_010101_3_1021206010.5" | names: "1007", "1017", "1027" (+2 more) | property sets: Pset_DDS
          3 x IFCFLOWTERMINAL | type IFCOUTLETTYPE "E3_E3-231012175149_1048_296_020201_3_00" | names: "1127", "1138", "3437" | property sets: Pset_DDS
          2 x IFCFLOWTERMINAL | type IFCOUTLETTYPE "E3_E3-200312113551_1024_296_020201_3_00" | names: "1149", "1162" | property sets: Pset_DDS
          2 x IFCFLOWTERMINAL | type IFCOUTLETTYPE "SK_1513013-_1008_301_010101_3_0" | names: "1175", "1183" | property sets: Pset_DDS
          7 x IFCFLOWCONTROLLER | type IFCSWITCHINGDEVICETYPE "S1_1409900_1001_001_010101_3_0" | names: "1191", "1217", "1243" (+4 more) | property sets: Pset_DDS
          3 x IFCFLOWCONTROLLER | type IFCSWITCHINGDEVICETYPE "S1_04401_1077_071_030101_3_0" | names: "1321", "2783", "3714" | property sets: Pset_DDS
          1 x IFCFLOWCONTROLLER | type IFCSWITCHINGDEVICETYPE "S1_044AB_1076_073_030101_3_0" | names: "1394" | property sets: Pset_DDS
          3 x IFCFLOWCONTROLLER | type IFCSWITCHINGDEVICETYPE "S1_1409903_1043_011_200101_3_0" | names: "1431", "1444", "2807" | property sets: Pset_DDS
          3 x IFCFLOWFITTING | type IFCJUNCTIONBOXTYPE "T1_042AC_1021_011_020101_3_0" | names: "1460", "1473", "1481" | property sets: Pset_DDS
          2 x IFCELECTRICDISTRIBUTIONPOINT | object type "SB_02104_1000_010_010101_3_030100.580.110.55" | DISTRIBUTIONBOARD | names: "EL/IKT-SKAP", "EL/IKT-SKAP-Kopi" | property sets: Pset_DDS
          8 x IFCFLOWSEGMENT
          1 x IFCELECTRICDISTRIBUTIONPOINT | object type "SB_02104_1000_010_010101_3_030100.300.050.30" | DISTRIBUTIONBOARD | names: "Brannmannspanel" | property sets: Pset_DDS
          1 x IFCELECTRICDISTRIBUTIONPOINT | object type "SB_02104_1000_010_010101_3_030100.100.050.30" | DISTRIBUTIONBOARD | names: "Brannmannspanel-Kopi" | property sets: Pset_DDS
          1 x IFCFLOWTERMINAL | type IFCOUTLETTYPE "E3_E3-M5008_1061_163_200101_3_00" | names: "2277" | property sets: Pset_DDS
          1 x IFCFLOWTERMINAL | type IFCLIGHTFIXTURETYPE "LF_07ACE_1064_265_120101_3_0011201110.5" | names: "2870" | property sets: Pset_DDS
          1 x IFCFLOWTERMINAL | type IFCOUTLETTYPE "E4_065AF_1070_210_020301_3_00" | names: "2871" | property sets: Pset_DDS
          2 x IFCFLOWCONTROLLER | type IFCSWITCHINGDEVICETYPE "S1_034ss_1071_060_090101_3_0" | names: "3110", "2868" | property sets: Pset_DDS
          1 x IFCFLOWTERMINAL | type IFCLIGHTFIXTURETYPE "LF_07AAC_1041_251_120101_3_001120810.5" | names: "3131" | property sets: Pset_DDS
          2 x IFCBUILDINGELEMENTPROXY
          2 x IFCFLOWTERMINAL | type IFCOUTLETTYPE "E4_09219_1022_176_020101_3_00" | names: "124", "3400" | property sets: Pset_DDS
          16 x IFCFLOWTERMINAL | type IFCLIGHTFIXTURETYPE "LI_LI-201013194004_1075_202_010101_3_102120900.5" | names: "3546", "3557", "997" (+13 more) | property sets: Pset_DDS
          3 x IFCFLOWTERMINAL | type IFCLIGHTFIXTURETYPE "LF_LF-110314070706_1078_400_200101_3_1011201830.5" | names: "3846", "3856", "3866" | property sets: Pset_DDS
          1 x IFCFLOWTERMINAL | type IFCLIGHTFIXTURETYPE "LI_LI-110314071042_1079_202_200101_3_1011206010.5" | names: "3799" | property sets: Pset_DDS
          3 x IFCFLOWCONTROLLER | type IFCSWITCHINGDEVICETYPE "S1_04204_1085_040_010101_3_0" | names: "672", "1386", "3241" | property sets: Pset_DDS
          5 x IFCDISTRIBUTIONCONTROLELEMENT | type IFCACTUATORTYPE "T2_T2-M0001_1090_110_200101_3_0" | names: "1404", "3902", "4017" (+2 more) | property sets: Pset_DDS
          3 x IFCFLOWCONTROLLER | type IFCSWITCHINGDEVICETYPE "S1_S1-M0001_1089_001_200101_3_0" | names: "2408", "3915", "4025" | property sets: Pset_DDS
          1 x IFCFLOWTERMINAL | type IFCLIGHTFIXTURETYPE "LF_LF-M5007_1093_400_200101_3_1011205810.5" | names: "3813" | property sets: Pset_DDS
      IFCBUILDINGSTOREY "02" | elevation 2.9 | description "02"
        contains 308 elements
          4 x IFCFLOWTERMINAL | type IFCOUTLETTYPE "E2_6950710_1010_100_010101_3_00" | names: "272", "282", "290" (+1 more) | property sets: Pset_DDS
          4 x IFCFLOWTERMINAL | type IFCOUTLETTYPE "E2_6950710-_1011_100_010101_3_00" | names: "153", "159", "269" (+1 more) | property sets: Pset_DDS
          8 x IFCFLOWTERMINAL | type IFCOUTLETTYPE "SK_1502164_1009_003_010101_3_0" | names: "140", "425", "147" (+5 more) | property sets: Pset_DDS
          121 x IFCFLOWTERMINAL | type IFCOUTLETTYPE "SK_1502134_1006_002_010101_3_0" | names: "514", "529", "515" (+118 more) | property sets: Pset_DDS
          18 x IFCFLOWTERMINAL | type IFCOUTLETTYPE "SK_1502102_1044_001_200101_3_0" | names: "1064", "1079", "1065" (+15 more) | property sets: Pset_DDS
          4 x IFCFLOWTERMINAL | type IFCOUTLETTYPE "SK_1416000-_1007_013_010101_3_0" | names: "1066", "1645", "1853" (+1 more) | property sets: Pset_DDS
          20 x IFCFLOWTERMINAL | type IFCLIGHTFIXTURETYPE "LI_1513013_1005_202_010101_3_0021206000.5" | names: "2169", "2486", "2177" (+17 more) | property sets: Pset_DDS
          20 x IFCFLOWTERMINAL | type IFCLIGHTFIXTURETYPE "LI_LI-090312092105_1004_202_010101_3_1021206010.5" | names: "2560", "2572", "2561" (+17 more) | property sets: Pset_DDS
          4 x IFCFLOWTERMINAL | type IFCOUTLETTYPE "E3_E3-200312113551_1024_296_020201_3_00" | names: "2870", "3163", "3164" (+1 more) | property sets: Pset_DDS
          6 x IFCFLOWTERMINAL | type IFCOUTLETTYPE "E3_E3-231012175149_1048_296_020201_3_00" | names: "3094", "3095", "3119" (+3 more) | property sets: Pset_DDS
          5 x IFCFLOWTERMINAL | type IFCOUTLETTYPE "SK_1513013-_1008_301_010101_3_0" | names: "2883", "2890", "3206" (+2 more) | property sets: Pset_DDS
          22 x IFCFLOWCONTROLLER | type IFCSWITCHINGDEVICETYPE "S1_1409900_1001_001_010101_3_0" | names: "3239", "3240", "3328" (+19 more) | property sets: Pset_DDS
          2 x IFCFLOWCONTROLLER | type IFCSWITCHINGDEVICETYPE "S1_S1-M5004_1086_011_200101_3_0" | names: "3225", "2021" | property sets: Pset_DDS
          8 x IFCFLOWCONTROLLER | type IFCSWITCHINGDEVICETYPE "S1_1409903_1043_011_200101_3_0" | names: "3716", "3705", "3991" (+5 more) | property sets: Pset_DDS
          9 x IFCFLOWFITTING | type IFCJUNCTIONBOXTYPE "T1_042AC_1021_011_020101_3_0" | names: "3746", "3755", "3869" (+6 more) | property sets: Pset_DDS
          4 x IFCELECTRICDISTRIBUTIONPOINT | object type "SB_02104_1000_010_010101_3_030100.580.110.55" | DISTRIBUTIONBOARD | names: "EL/IKT-SKAP-Kopi-Kop" | property sets: Pset_DDS
          8 x IFCFLOWSEGMENT
          1 x IFCFLOWTERMINAL | type IFCLIGHTFIXTURETYPE "LF_07ACA_1066_261_120101_3_0011201110.5" | names: "2703" | property sets: Pset_DDS
          2 x IFCBUILDINGELEMENTPROXY
          4 x IFCFLOWTERMINAL | type IFCOUTLETTYPE "E4_09219_1022_176_020101_3_00" | names: "5041", "5169", "5198" (+1 more) | property sets: Pset_DDS
          3 x IFCFLOWTERMINAL | type IFCLIGHTFIXTURETYPE "LF_LF-110314070706_1078_400_200101_3_1011201830.5" | names: "5389", "5401", "5411" | property sets: Pset_DDS
          1 x IFCFLOWTERMINAL | type IFCLIGHTFIXTURETYPE "LI_LI-110314071042_1079_202_200101_3_1011206010.5" | names: "122" | property sets: Pset_DDS
          4 x IFCFLOWCONTROLLER | type IFCSWITCHINGDEVICETYPE "S1_034ss_1071_060_090101_3_0" | names: "2860", "5713", "5734" (+1 more) | property sets: Pset_DDS
          7 x IFCFLOWCONTROLLER | type IFCSWITCHINGDEVICETYPE "S1_04204_1085_040_010101_3_0" | names: "1868", "3531", "3527" (+4 more) | property sets: Pset_DDS
          11 x IFCDISTRIBUTIONCONTROLELEMENT | type IFCACTUATORTYPE "T2_T2-M0001_1090_110_200101_3_0" | names: "1892", "5482", "5801" (+8 more) | property sets: Pset_DDS
          7 x IFCFLOWCONTROLLER | type IFCSWITCHINGDEVICETYPE "S1_S1-M0001_1089_001_200101_3_0" | names: "3602", "5787", "5809" (+4 more) | property sets: Pset_DDS
          1 x IFCFLOWTERMINAL | type IFCLIGHTFIXTURETYPE "LF_LF-M5007_1093_400_200101_3_1011205810.5" | names: "2850" | property sets: Pset_DDS
      IFCBUILDINGSTOREY "03" | elevation 5.8 | description "03"
        contains 312 elements
          5 x IFCFLOWTERMINAL | type IFCOUTLETTYPE "E2_6950710_1010_100_010101_3_00" | names: "141", "149", "157" (+2 more) | property sets: Pset_DDS
          4 x IFCFLOWTERMINAL | type IFCOUTLETTYPE "E2_6950710-_1011_100_010101_3_00" | names: "173", "181", "189" (+1 more) | property sets: Pset_DDS
          8 x IFCFLOWTERMINAL | type IFCOUTLETTYPE "SK_1502164_1009_003_010101_3_0" | names: "205", "218", "231" (+5 more) | property sets: Pset_DDS
          119 x IFCFLOWTERMINAL | type IFCOUTLETTYPE "SK_1502134_1006_002_010101_3_0" | names: "309", "322", "335" (+116 more) | property sets: Pset_DDS
          18 x IFCFLOWTERMINAL | type IFCOUTLETTYPE "SK_1502102_1044_001_200101_3_0" | names: "811", "826", "841" (+15 more) | property sets: Pset_DDS
          4 x IFCFLOWTERMINAL | type IFCOUTLETTYPE "SK_1416000-_1007_013_010101_3_0" | names: "871", "1287", "1495" (+1 more) | property sets: Pset_DDS
          20 x IFCFLOWTERMINAL | type IFCLIGHTFIXTURETYPE "LI_1513013_1005_202_010101_3_0021206000.5" | names: "2007", "2017", "2027" (+17 more) | property sets: Pset_DDS
          17 x IFCFLOWTERMINAL | type IFCLIGHTFIXTURETYPE "LI_LI-090312092105_1004_202_010101_3_1021206010.5" | names: "2099", "2109", "2119" (+14 more) | property sets: Pset_DDS
          2 x IFCFLOWTERMINAL | type IFCLIGHTFIXTURETYPE "LI_LI-110314090322_1081_202_200101_3_1011206010.5" | names: "2199", "5513" | property sets: Pset_DDS
          4 x IFCFLOWTERMINAL | type IFCOUTLETTYPE "E3_E3-200312113551_1024_296_020201_3_00" | names: "2399", "2478", "2491" (+1 more) | property sets: Pset_DDS
          6 x IFCFLOWTERMINAL | type IFCOUTLETTYPE "E3_E3-231012175149_1048_296_020201_3_00" | names: "2423", "2434", "2445" (+3 more) | property sets: Pset_DDS
          5 x IFCFLOWTERMINAL | type IFCOUTLETTYPE "SK_1513013-_1008_301_010101_3_0" | names: "2517", "2530", "2538" (+2 more) | property sets: Pset_DDS
          2 x IFCFLOWCONTROLLER | type IFCSWITCHINGDEVICETYPE "S1_S1-M5004_1086_011_200101_3_0" | names: "2554", "2580" | property sets: Pset_DDS
          18 x IFCFLOWCONTROLLER | type IFCSWITCHINGDEVICETYPE "S1_1409900_1001_001_010101_3_0" | names: "2567", "2632", "2658" (+15 more) | property sets: Pset_DDS
          5 x IFCFLOWCONTROLLER | type IFCSWITCHINGDEVICETYPE "S1_S1-M5008_1074_071_200101_3_0" | names: "2736", "3008", "5481" (+2 more) | property sets: Pset_DDS
          2 x IFCFLOWCONTROLLER | type IFCSWITCHINGDEVICETYPE "S1_1410222-_1056_002_200101_3_0" | names: "2939", "2955" | property sets: Pset_DDS
          9 x IFCFLOWFITTING | type IFCJUNCTIONBOXTYPE "T1_042AC_1021_011_020101_3_0" | names: "3037", "3050", "3058" (+6 more) | property sets: Pset_DDS
          6 x IFCFLOWCONTROLLER | type IFCSWITCHINGDEVICETYPE "S1_1409903_1043_011_200101_3_0" | names: "3178", "3186", "3194" (+3 more) | property sets: Pset_DDS
          4 x IFCFLOWCONTROLLER | type IFCSWITCHINGDEVICETYPE "S1_1409906_1069_021_200101_3_0" | names: "3210", "3218", "3258" (+1 more) | property sets: Pset_DDS
          4 x IFCELECTRICDISTRIBUTIONPOINT | object type "SB_02104_1000_010_010101_3_030100.580.110.55" | DISTRIBUTIONBOARD | names: "EL/IKT-SKAP-Kopi-Kop" | property sets: Pset_DDS
          8 x IFCFLOWSEGMENT
          4 x IFCFLOWTERMINAL | type IFCOUTLETTYPE "E4_09219_1022_176_020101_3_00" | names: "2994", "5201", "5230" (+1 more) | property sets: Pset_DDS
          1 x IFCBUILDINGELEMENTPROXY
          1 x IFCFLOWTERMINAL | type IFCLIGHTFIXTURETYPE "LF_07ACA_1066_261_120101_3_0011201110.5" | names: "704" | property sets: Pset_DDS
          3 x IFCFLOWTERMINAL | type IFCLIGHTFIXTURETYPE "LF_LF-110314070706_1078_400_200101_3_1011201830.5" | names: "2097", "2276", "109" | property sets: Pset_DDS
          1 x IFCFLOWTERMINAL | type IFCLIGHTFIXTURETYPE "LI_LI-110314071042_1079_202_200101_3_1011206010.5" | names: "5349" | property sets: Pset_DDS
          4 x IFCFLOWCONTROLLER | type IFCSWITCHINGDEVICETYPE "S1_034ss_1071_060_090101_3_0" | names: "5385", "5406", "5427" (+1 more) | property sets: Pset_DDS
          4 x IFCFLOWCONTROLLER | type IFCSWITCHINGDEVICETYPE "S1_044AB_1076_073_030101_3_0" | names: "5497", "5539", "2593" (+1 more) | property sets: Pset_DDS
          1 x IFCFLOWTERMINAL | type IFCLIGHTFIXTURETYPE "LF_LF-M5007_1093_400_200101_3_1011205810.5" | names: "118" | property sets: Pset_DDS
          11 x IFCDISTRIBUTIONCONTROLELEMENT | type IFCACTUATORTYPE "T2_T2-M0001_1090_110_200101_3_0" | names: "911", "2965", "5248" (+8 more) | property sets: Pset_DDS
          5 x IFCFLOWCONTROLLER | type IFCSWITCHINGDEVICETYPE "S1_04204_1085_040_010101_3_0" | names: "896", "1312", "886" (+2 more) | property sets: Pset_DDS
          7 x IFCFLOWCONTROLLER | type IFCSWITCHINGDEVICETYPE "S1_S1-M0001_1089_001_200101_3_0" | names: "5694", "5716", "5737" (+4 more) | property sets: Pset_DDS
      IFCBUILDINGSTOREY "04" | elevation 8.700000000000001 | description "04"
        contains 300 elements
          4 x IFCFLOWTERMINAL | type IFCOUTLETTYPE "E2_6950710_1010_100_010101_3_00" | names: "139", "147", "155" (+1 more) | property sets: Pset_DDS
          4 x IFCFLOWTERMINAL | type IFCOUTLETTYPE "E2_6950710-_1011_100_010101_3_00" | names: "171", "179", "187" (+1 more) | property sets: Pset_DDS
          8 x IFCFLOWTERMINAL | type IFCOUTLETTYPE "SK_1502164_1009_003_010101_3_0" | names: "203", "216", "229" (+5 more) | property sets: Pset_DDS
          115 x IFCFLOWTERMINAL | type IFCOUTLETTYPE "SK_1502134_1006_002_010101_3_0" | names: "307", "320", "333" (+112 more) | property sets: Pset_DDS
          17 x IFCFLOWTERMINAL | type IFCOUTLETTYPE "SK_1502102_1044_001_200101_3_0" | names: "801", "816", "831" (+14 more) | property sets: Pset_DDS
          4 x IFCFLOWTERMINAL | type IFCOUTLETTYPE "SK_1416000-_1007_013_010101_3_0" | names: "861", "1273", "1481" (+1 more) | property sets: Pset_DDS
          20 x IFCFLOWTERMINAL | type IFCLIGHTFIXTURETYPE "LI_1513013_1005_202_010101_3_0021206000.5" | names: "1991", "2001", "2011" (+17 more) | property sets: Pset_DDS
          15 x IFCFLOWTERMINAL | type IFCLIGHTFIXTURETYPE "LI_LI-090312092105_1004_202_010101_3_1021206010.5" | names: "2081", "2101", "2111" (+12 more) | property sets: Pset_DDS
          4 x IFCFLOWTERMINAL | type IFCOUTLETTYPE "E3_E3-200312113551_1024_296_020201_3_00" | names: "2371", "2439", "2452" (+1 more) | property sets: Pset_DDS
          6 x IFCFLOWTERMINAL | type IFCOUTLETTYPE "E3_E3-231012175149_1048_296_020201_3_00" | names: "2384", "2395", "2406" (+3 more) | property sets: Pset_DDS
          5 x IFCFLOWTERMINAL | type IFCOUTLETTYPE "SK_1513013-_1008_301_010101_3_0" | names: "2478", "2491", "2499" (+2 more) | property sets: Pset_DDS
          19 x IFCFLOWCONTROLLER | type IFCSWITCHINGDEVICETYPE "S1_1409900_1001_001_010101_3_0" | names: "2528", "2554", "2593" (+16 more) | property sets: Pset_DDS
          1 x IFCFLOWCONTROLLER | type IFCSWITCHINGDEVICETYPE "S1_S1-M5004_1086_011_200101_3_0" | names: "2541" | property sets: Pset_DDS
          3 x IFCFLOWCONTROLLER | type IFCSWITCHINGDEVICETYPE "S1_S1-M5005_1082_021_200101_3_0" | names: "2749", "5450", "5471" | property sets: Pset_DDS
          8 x IFCFLOWCONTROLLER | type IFCSWITCHINGDEVICETYPE "S1_1409903_1043_011_200101_3_0" | names: "2969", "3139", "3147" (+5 more) | property sets: Pset_DDS
          8 x IFCFLOWFITTING | type IFCJUNCTIONBOXTYPE "T1_042AC_1021_011_020101_3_0" | names: "2998", "3011", "3019" (+5 more) | property sets: Pset_DDS
          2 x IFCFLOWCONTROLLER | type IFCSWITCHINGDEVICETYPE "S1_1409906_1069_021_200101_3_0" | names: "3171", "3179" | property sets: Pset_DDS
          4 x IFCELECTRICDISTRIBUTIONPOINT | object type "SB_02104_1000_010_010101_3_030100.580.110.55" | DISTRIBUTIONBOARD | names: "EL/IKT-SKAP-Kopi-Kop" | property sets: Pset_DDS
          8 x IFCFLOWSEGMENT
          4 x IFCFLOWTERMINAL | type IFCOUTLETTYPE "E4_09219_1022_176_020101_3_00" | names: "2950", "5135", "5164" (+1 more) | property sets: Pset_DDS
          1 x IFCBUILDINGELEMENTPROXY
          1 x IFCFLOWTERMINAL | type IFCLIGHTFIXTURETYPE "LF_07ACA_1066_261_120101_3_0011201110.5" | names: "2078" | property sets: Pset_DDS
          3 x IFCFLOWTERMINAL | type IFCLIGHTFIXTURETYPE "LF_LF-110314070706_1078_400_200101_3_1011201830.5" | names: "2370", "3278", "5283" | property sets: Pset_DDS
          1 x IFCFLOWTERMINAL | type IFCLIGHTFIXTURETYPE "LI_LI-110314071042_1079_202_200101_3_1011206010.5" | names: "5293" | property sets: Pset_DDS
          3 x IFCFLOWCONTROLLER | type IFCSWITCHINGDEVICETYPE "S1_034ss_1071_060_090101_3_0" | names: "2091", "5322", "5343" | property sets: Pset_DDS
          6 x IFCFLOWTERMINAL | type IFCLIGHTFIXTURETYPE "LI_LI-201013194004_1075_202_010101_3_102120900.5" | names: "5394", "5407", "2192" (+3 more) | property sets: Pset_DDS
          1 x IFCFLOWTERMINAL | type IFCLIGHTFIXTURETYPE "LF_LF-M5007_1093_400_200101_3_1011205810.5" | names: "108" | property sets: Pset_DDS
          7 x IFCFLOWCONTROLLER | type IFCSWITCHINGDEVICETYPE "S1_04204_1085_040_010101_3_0" | names: "1520", "901", "886" (+4 more) | property sets: Pset_DDS
          11 x IFCDISTRIBUTIONCONTROLELEMENT | type IFCACTUATORTYPE "T2_T2-M0001_1090_110_200101_3_0" | names: "2181", "5511", "5541" (+8 more) | property sets: Pset_DDS
          7 x IFCFLOWCONTROLLER | type IFCSWITCHINGDEVICETYPE "S1_S1-M0001_1089_001_200101_3_0" | names: "2912", "5519", "5549" (+4 more) | property sets: Pset_DDS
      IFCBUILDINGSTOREY "05" | elevation 11.6 | description "05"
        contains 245 elements
          3 x IFCFLOWTERMINAL | type IFCOUTLETTYPE "E2_6950710_1010_100_010101_3_00" | names: "139", "147", "155" | property sets: Pset_DDS
          3 x IFCFLOWTERMINAL | type IFCOUTLETTYPE "E2_6950710-_1011_100_010101_3_00" | names: "171", "179", "187" | property sets: Pset_DDS
          6 x IFCFLOWTERMINAL | type IFCOUTLETTYPE "SK_1502164_1009_003_010101_3_0" | names: "203", "216", "229" (+3 more) | property sets: Pset_DDS
          96 x IFCFLOWTERMINAL | type IFCOUTLETTYPE "SK_1502134_1006_002_010101_3_0" | names: "307", "320", "333" (+93 more) | property sets: Pset_DDS
          13 x IFCFLOWTERMINAL | type IFCOUTLETTYPE "SK_1502102_1044_001_200101_3_0" | names: "793", "808", "823" (+10 more) | property sets: Pset_DDS
          3 x IFCFLOWTERMINAL | type IFCOUTLETTYPE "SK_1416000-_1007_013_010101_3_0" | names: "853", "1265", "1060" | property sets: Pset_DDS
          18 x IFCFLOWTERMINAL | type IFCLIGHTFIXTURETYPE "LI_1513013_1005_202_010101_3_0021206000.5" | names: "1965", "1975", "2005" (+15 more) | property sets: Pset_DDS
          11 x IFCFLOWTERMINAL | type IFCLIGHTFIXTURETYPE "LI_LI-090312092105_1004_202_010101_3_1021206010.5" | names: "2055", "2075", "2085" (+8 more) | property sets: Pset_DDS
          3 x IFCFLOWTERMINAL | type IFCOUTLETTYPE "E3_E3-200312113551_1024_296_020201_3_00" | names: "2345", "2426", "2439" | property sets: Pset_DDS
          7 x IFCFLOWTERMINAL | type IFCOUTLETTYPE "E3_E3-231012175149_1048_296_020201_3_00" | names: "2358", "2369", "2380" (+4 more) | property sets: Pset_DDS
          5 x IFCFLOWTERMINAL | type IFCOUTLETTYPE "SK_1513013-_1008_301_010101_3_0" | names: "2452", "2465", "2473" (+2 more) | property sets: Pset_DDS
          14 x IFCFLOWCONTROLLER | type IFCSWITCHINGDEVICETYPE "S1_1409900_1001_001_010101_3_0" | names: "2489", "2554", "2606" (+11 more) | property sets: Pset_DDS
          1 x IFCFLOWCONTROLLER | type IFCSWITCHINGDEVICETYPE "S1_S1-M5001_1031_001_200101_3_0" | names: "2885" | property sets: Pset_DDS
          5 x IFCFLOWFITTING | type IFCJUNCTIONBOXTYPE "T1_042AC_1021_011_020101_3_0" | names: "2943", "2972", "2980" (+2 more) | property sets: Pset_DDS
          7 x IFCFLOWCONTROLLER | type IFCSWITCHINGDEVICETYPE "S1_1409903_1043_011_200101_3_0" | names: "3068", "3076", "3084" (+4 more) | property sets: Pset_DDS
          2 x IFCFLOWCONTROLLER | type IFCSWITCHINGDEVICETYPE "S1_1409906_1069_021_200101_3_0" | names: "3100", "3108" | property sets: Pset_DDS
          3 x IFCELECTRICDISTRIBUTIONPOINT | object type "SB_02104_1000_010_010101_3_030100.580.110.55" | DISTRIBUTIONBOARD | names: "EL/IKT-SKAP-Kopi-Kop" | property sets: Pset_DDS
          6 x IFCFLOWSEGMENT
          3 x IFCFLOWTERMINAL | type IFCOUTLETTYPE "E4_09219_1022_176_020101_3_00" | names: "4080", "4208", "4237" | property sets: Pset_DDS
          1 x IFCBUILDINGELEMENTPROXY
          1 x IFCFLOWTERMINAL | type IFCLIGHTFIXTURETYPE "LF_07ACA_1066_261_120101_3_0011201110.5" | names: "2068" | property sets: Pset_DDS
          3 x IFCFLOWTERMINAL | type IFCLIGHTFIXTURETYPE "LF_LF-110314070706_1078_400_200101_3_1011201830.5" | names: "2344", "4308", "4318" | property sets: Pset_DDS
          1 x IFCFLOWTERMINAL | type IFCLIGHTFIXTURETYPE "LI_LI-110314071042_1079_202_200101_3_1011206010.5" | names: "4328" | property sets: Pset_DDS
          2 x IFCFLOWCONTROLLER | type IFCSWITCHINGDEVICETYPE "S1_034ss_1071_060_090101_3_0" | names: "3172", "4365" | property sets: Pset_DDS
          1 x IFCFLOWCONTROLLER | type IFCSWITCHINGDEVICETYPE "S1_S1-M5005_1082_021_200101_3_0" | names: "4423" | property sets: Pset_DDS
          7 x IFCFLOWTERMINAL | type IFCLIGHTFIXTURETYPE "LI_LI-201013194004_1075_202_010101_3_102120900.5" | names: "2145", "4476", "4487" (+4 more) | property sets: Pset_DDS
          1 x IFCFLOWCONTROLLER | type IFCSWITCHINGDEVICETYPE "S1_044AB_1076_073_030101_3_0" | names: "4509" | property sets: Pset_DDS
          1 x IFCFLOWTERMINAL | type IFCLIGHTFIXTURETYPE "LF_LF-M5007_1093_400_200101_3_1011205810.5" | names: "108" | property sets: Pset_DDS
          8 x IFCDISTRIBUTIONCONTROLELEMENT | type IFCACTUATORTYPE "T2_T2-M0001_1090_110_200101_3_0" | names: "2042", "2067", "4639" (+5 more) | property sets: Pset_DDS
          5 x IFCFLOWCONTROLLER | type IFCSWITCHINGDEVICETYPE "S1_04204_1085_040_010101_3_0" | names: "1236", "892", "874" (+2 more) | property sets: Pset_DDS
          5 x IFCFLOWCONTROLLER | type IFCSWITCHINGDEVICETYPE "S1_S1-M0001_1089_001_200101_3_0" | names: "4523", "4668", "4690" (+2 more) | property sets: Pset_DDS

Types
  IFCOUTLETTYPE "E2_6950710_1010_100_010101_3_00" | element type "E2_6950710_1010_100_010101_3_00" | COMMUNICATIONSOUTLET | 18 occurrences | property sets: Pset_ManufacturerTypeInformation, Pset_OutletTypeCommon, Pset_ElectricalDeviceCommon | description "2-IKT (2x Cat5UTP 6991160) + (1x1410113) Lexcom"
  IFCOUTLETTYPE "E2_6950710-_1011_100_010101_3_00" | element type "E2_6950710-_1011_100_010101_3_00" | COMMUNICATIONSOUTLET | 17 occurrences | property sets: Pset_ManufacturerTypeInformation, Pset_OutletTypeCommon, Pset_ElectricalDeviceCommon | description "1-IKT (1x Cat5UTP 6991160) + (1x1410113) Lexcom"
  IFCOUTLETTYPE "SK_1502164_1009_003_010101_3_0" | element type "SK_1502164_1009_003_010101_3_0" | POWEROUTLET | 34 occurrences | property sets: Pset_ManufacturerTypeInformation, Pset_OutletTypeCommon, Pset_ElectricalDeviceCommon | description "Trippel stikk innfelt Exxact"
  IFCOUTLETTYPE "SK_1502134_1006_002_010101_3_0" | element type "SK_1502134_1006_002_010101_3_0" | POWEROUTLET | 500 occurrences | property sets: Pset_ManufacturerTypeInformation, Pset_OutletTypeCommon, Pset_ElectricalDeviceCommon | description "Stikkontakt dobbel m/jord innfelt Exxact"
  IFCOUTLETTYPE "SK_1502102_1044_001_200101_3_0" | element type "SK_1502102_1044_001_200101_3_0" | POWEROUTLET | 74 occurrences | property sets: Pset_ManufacturerTypeInformation, Pset_OutletTypeCommon, Pset_ElectricalDeviceCommon | description "Stikkontakt enkel Exxact"
  IFCOUTLETTYPE "SK_1416000-_1007_013_010101_3_0" | element type "SK_1416000-_1007_013_010101_3_0" | POWEROUTLET | 17 occurrences | property sets: Pset_ManufacturerTypeInformation, Pset_OutletTypeCommon, Pset_ElectricalDeviceCommon | description "Stikk flatstift 25A (Inngår i komfyrvakt)"
  IFCLIGHTFIXTURETYPE "LI_1513013_1005_202_010101_3_0021206000.5" | element type "LI_1513013_1005_202_010101_3_0021206000.5" | POINTSOURCE | 84 occurrences | property sets: Pset_ManufacturerTypeInformation, Pset_LightFixtureTypeCommon, Pset_ElectricalDeviceCommon | description "Lyspunkt DCL i tak Exxact"
  IFCLIGHTFIXTURETYPE "LI_LI-090312092105_1004_202_010101_3_1021206010.5" | element type "LI_LI-090312092105_1004_202_010101_3_1021206010.5" | POINTSOURCE | 68 occurrences | property sets: Pset_ManufacturerTypeInformation, Pset_LightFixtureTypeCommon, Pset_ElectricalDeviceCommon | description "Lyspunkt m/armatur"
  IFCOUTLETTYPE "E3_E3-231012175149_1048_296_020201_3_00" | element type "E3_E3-231012175149_1048_296_020201_3_00" | 28 occurrences | property sets: Pset_ManufacturerTypeInformation, Pset_OutletTypeCommon, Pset_ElectricalDeviceCommon | description "RØKDETEKTOR M/ALARMORGAN"
  IFCOUTLETTYPE "E3_E3-200312113551_1024_296_020201_3_00" | element type "E3_E3-200312113551_1024_296_020201_3_00" | 17 occurrences | property sets: Pset_ManufacturerTypeInformation, Pset_OutletTypeCommon, Pset_ElectricalDeviceCommon | description "RØKDETEKTOR OPTISK M/ALARMORGAN"
  IFCOUTLETTYPE "SK_1513013-_1008_301_010101_3_0" | element type "SK_1513013-_1008_301_010101_3_0" | POWEROUTLET | 22 occurrences | property sets: Pset_ManufacturerTypeInformation, Pset_OutletTypeCommon, Pset_ElectricalDeviceCommon | description "DCL Takuttak Exxact"
  IFCSWITCHINGDEVICETYPE "S1_1409900_1001_001_010101_3_0" | element type "S1_1409900_1001_001_010101_3_0" | TOGGLESWITCH | 80 occurrences | property sets: Pset_ManufacturerTypeInformation, Pset_SwitchingDeviceTypeCommon, Pset_SwitchingDeviceTypeToggleSwitch, Pset_ElectricalDeviceCommon | description "Bryter 1p innfelt Exxact"
  IFCSWITCHINGDEVICETYPE "S1_04401_1077_071_030101_3_0" | element type "S1_04401_1077_071_030101_3_0" | TOGGLESWITCH | 3 occurrences | property sets: Pset_ManufacturerTypeInformation, Pset_SwitchingDeviceTypeCommon, Pset_SwitchingDeviceTypeToggleSwitch, Pset_ElectricalDeviceCommon | description "Lysreg. for gl.lamp m/boks 300W"
  IFCSWITCHINGDEVICETYPE "S1_044AB_1076_073_030101_3_0" | element type "S1_044AB_1076_073_030101_3_0" | TOGGLESWITCH | 6 occurrences | property sets: Pset_ManufacturerTypeInformation, Pset_SwitchingDeviceTypeCommon, Pset_SwitchingDeviceTypeToggleSwitch, Pset_ElectricalDeviceCommon | description "Lysreg. for gl.lamp m/boks 300W 2 polt"
  IFCSWITCHINGDEVICETYPE "S1_1409903_1043_011_200101_3_0" | element type "S1_1409903_1043_011_200101_3_0" | TOGGLESWITCH | 32 occurrences | property sets: Pset_ManufacturerTypeInformation, Pset_SwitchingDeviceTypeCommon, Pset_SwitchingDeviceTypeToggleSwitch, Pset_ElectricalDeviceCommon | description "Kronevender innfelt Exxact"
  IFCJUNCTIONBOXTYPE "T1_042AC_1021_011_020101_3_0" | element type "T1_042AC_1021_011_020101_3_0" | 34 occurrences | property sets: Pset_ManufacturerTypeInformation, Pset_ElectricalDeviceCommon | description "Veggboks for lampepunkt"
  IFCOUTLETTYPE "E3_E3-M5008_1061_163_200101_3_00" | element type "E3_E3-M5008_1061_163_200101_3_00" | 1 occurrence | property sets: Pset_ManufacturerTypeInformation, Pset_OutletTypeCommon, Pset_ElectricalDeviceCommon | description "Manuell brannmelder"
  IFCLIGHTFIXTURETYPE "LF_07ACE_1064_265_120101_3_0011201110.5" | element type "LF_07ACE_1064_265_120101_3_0011201110.5" | DIRECTIONSOURCE | 1 occurrence | property sets: Pset_ManufacturerTypeInformation, Pset_LightFixtureTypeCommon, Pset_ElectricalDeviceCommon | description "Nødlys, pil opp"
  IFCOUTLETTYPE "E4_065AF_1070_210_020301_3_00" | element type "E4_065AF_1070_210_020301_3_00" | AUDIOVISUALOUTLET | 1 occurrence | property sets: Pset_ManufacturerTypeInformation, Pset_OutletTypeCommon, Pset_ElectricalDeviceCommon | description "Trykknappsats 1 rekke 10 knapper innf"
  IFCSWITCHINGDEVICETYPE "S1_034ss_1071_060_090101_3_0" | element type "S1_034ss_1071_060_090101_3_0" | TOGGLESWITCH | 15 occurrences | property sets: Pset_ManufacturerTypeInformation, Pset_SwitchingDeviceTypeCommon, Pset_SwitchingDeviceTypeToggleSwitch, Pset_ElectricalDeviceCommon | description "Ringeknapp v/dør"
  IFCLIGHTFIXTURETYPE "LF_07AAC_1041_251_120101_3_001120810.5" | element type "LF_07AAC_1041_251_120101_3_001120810.5" | DIRECTIONSOURCE | 1 occurrence | property sets: Pset_ManufacturerTypeInformation, Pset_LightFixtureTypeCommon, Pset_ElectricalDeviceCommon | description "Markeringslys 8W dobbeltsidig"
  IFCOUTLETTYPE "E4_09219_1022_176_020101_3_00" | element type "E4_09219_1022_176_020101_3_00" | AUDIOVISUALOUTLET | 17 occurrences | property sets: Pset_ManufacturerTypeInformation, Pset_OutletTypeCommon, Pset_ElectricalDeviceCommon | description "SVARAPPARAT VEGGMONT FOR VEGGBOKS"
  IFCLIGHTFIXTURETYPE "LI_LI-201013194004_1075_202_010101_3_102120900.5" | element type "LI_LI-201013194004_1075_202_010101_3_102120900.5" | POINTSOURCE | 29 occurrences | property sets: Pset_ManufacturerTypeInformation, Pset_LightFixtureTypeCommon, Pset_ElectricalDeviceCommon | description "Nordesign LED 9W"
  IFCLIGHTFIXTURETYPE "LF_LF-110314070706_1078_400_200101_3_1011201830.5" | element type "LF_LF-110314070706_1078_400_200101_3_1011201830.5" | DIRECTIONSOURCE | 15 occurrences | property sets: Pset_ManufacturerTypeInformation, Pset_LightFixtureTypeCommon, Pset_ElectricalDeviceCommon | description "Lysrørarmatur 2x14W T5"
  IFCLIGHTFIXTURETYPE "LI_LI-110314071042_1079_202_200101_3_1011206010.5" | element type "LI_LI-110314071042_1079_202_200101_3_1011206010.5" | POINTSOURCE | 5 occurrences | property sets: Pset_ManufacturerTypeInformation, Pset_LightFixtureTypeCommon, Pset_ElectricalDeviceCommon | description "OptiLED"
  IFCSWITCHINGDEVICETYPE "S1_04204_1085_040_010101_3_0" | element type "S1_04204_1085_040_010101_3_0" | TOGGLESWITCH | 27 occurrences | property sets: Pset_ManufacturerTypeInformation, Pset_SwitchingDeviceTypeCommon, Pset_SwitchingDeviceTypeToggleSwitch, Pset_ElectricalDeviceCommon | description "Bryter 2/16A+1/16A m/boks"
  IFCACTUATORTYPE "T2_T2-M0001_1090_110_200101_3_0" | element type "T2_T2-M0001_1090_110_200101_3_0" | THERMOSTATICACTUATOR | 46 occurrences | property sets: Pset_ManufacturerTypeInformation, Pset_ActuatorTypeCommon, Pset_ElectricalDeviceCommon | description "Termostat"
  IFCSWITCHINGDEVICETYPE "S1_S1-M0001_1089_001_200101_3_0" | element type "S1_S1-M0001_1089_001_200101_3_0" | TOGGLESWITCH | 29 occurrences | property sets: Pset_ManufacturerTypeInformation, Pset_SwitchingDeviceTypeCommon, Pset_SwitchingDeviceTypeToggleSwitch, Pset_ElectricalDeviceCommon | description "Bryter 1-pol m/boks"
  IFCLIGHTFIXTURETYPE "LF_LF-M5007_1093_400_200101_3_1011205810.5" | element type "LF_LF-M5007_1093_400_200101_3_1011205810.5" | DIRECTIONSOURCE | 5 occurrences | property sets: Pset_ManufacturerTypeInformation, Pset_LightFixtureTypeCommon, Pset_ElectricalDeviceCommon | description "Lysrørarmatur 1x58W"
  IFCSWITCHINGDEVICETYPE "S1_S1-M5004_1086_011_200101_3_0" | element type "S1_S1-M5004_1086_011_200101_3_0" | TOGGLESWITCH | 5 occurrences | property sets: Pset_ManufacturerTypeInformation, Pset_SwitchingDeviceTypeCommon, Pset_SwitchingDeviceTypeToggleSwitch, Pset_ElectricalDeviceCommon | description "Serievender"
  IFCLIGHTFIXTURETYPE "LF_07ACA_1066_261_120101_3_0011201110.5" | element type "LF_07ACA_1066_261_120101_3_0011201110.5" | DIRECTIONSOURCE | 4 occurrences | property sets: Pset_ManufacturerTypeInformation, Pset_LightFixtureTypeCommon, Pset_ElectricalDeviceCommon | description "Nødlys, pil venstre"
  IFCLIGHTFIXTURETYPE "LI_LI-110314090322_1081_202_200101_3_1011206010.5" | element type "LI_LI-110314090322_1081_202_200101_3_1011206010.5" | POINTSOURCE | 2 occurrences | property sets: Pset_ManufacturerTypeInformation, Pset_LightFixtureTypeCommon, Pset_ElectricalDeviceCommon | description "Kopi av Rund armatur"
  IFCSWITCHINGDEVICETYPE "S1_S1-M5008_1074_071_200101_3_0" | element type "S1_S1-M5008_1074_071_200101_3_0" | TOGGLESWITCH | 5 occurrences | property sets: Pset_ManufacturerTypeInformation, Pset_SwitchingDeviceTypeCommon, Pset_SwitchingDeviceTypeToggleSwitch, Pset_ElectricalDeviceCommon | description "Lysregulator"
  IFCSWITCHINGDEVICETYPE "S1_1410222-_1056_002_200101_3_0" | element type "S1_1410222-_1056_002_200101_3_0" | TOGGLESWITCH | 2 occurrences | property sets: Pset_ManufacturerTypeInformation, Pset_SwitchingDeviceTypeCommon, Pset_SwitchingDeviceTypeToggleSwitch, Pset_ElectricalDeviceCommon | description "2p-Bryter innfelt Exxact"
  IFCSWITCHINGDEVICETYPE "S1_1409906_1069_021_200101_3_0" | element type "S1_1409906_1069_021_200101_3_0" | TOGGLESWITCH | 8 occurrences | property sets: Pset_ManufacturerTypeInformation, Pset_SwitchingDeviceTypeCommon, Pset_SwitchingDeviceTypeToggleSwitch, Pset_ElectricalDeviceCommon | description "Endevender exxact"
  IFCSWITCHINGDEVICETYPE "S1_S1-M5005_1082_021_200101_3_0" | element type "S1_S1-M5005_1082_021_200101_3_0" | TOGGLESWITCH | 4 occurrences | property sets: Pset_ManufacturerTypeInformation, Pset_SwitchingDeviceTypeCommon, Pset_SwitchingDeviceTypeToggleSwitch, Pset_ElectricalDeviceCommon | description "Vekselvender"
  IFCSWITCHINGDEVICETYPE "S1_S1-M5001_1031_001_200101_3_0" | element type "S1_S1-M5001_1031_001_200101_3_0" | TOGGLESWITCH | 1 occurrence | property sets: Pset_ManufacturerTypeInformation, Pset_SwitchingDeviceTypeCommon, Pset_SwitchingDeviceTypeToggleSwitch, Pset_ElectricalDeviceCommon | description "Bryter 1-pol"

Property sets
  Pset_DDS | properties | on 2 objects (2 IFCFLOWCONTROLLER)
    Antall poler = "0" (IFCTEXT)
    Beskrivelse = "Lysregulator" (IFCTEXT)
    Bygningsdel = "Bygning: 0" (IFCTEXT)
    Etasjenummer = "Etasje: 4" (IFCTEXT)
    Group = "" (IFCTEXT)
    HOH, ref UK = "NNUK=13.14 m" (IFCTEXT)
    HOH, ref senter = "NN=13.14 m" (IFCTEXT)
    Høyde over ferdig gulv = "Senter= 1.10m OFG" (IFCTEXT)
    Høyde over rådekke = "Senter= 1.10m OKD" (IFCTEXT)
    Høyde underkant tak = "Senter= 1.63m UKT" (IFCTEXT)
    Lagnummer = 440 (IFCINTEGER)
    Modellnummer = "Modelllnr: 12" (IFCTEXT)
    Montasjehøyde = "1.10 m" (IFCTEXT)
    OK underkant tak = "OK= 0.00m UKT" (IFCTEXT)
    Produkt nr. = "S1-M5008" (IFCTEXT)
    Prosjektnavn = "1540_B6" (IFCTEXT)
    UK over rådekke = "UK= 1.10m OKD" (IFCTEXT)
    X-koordinat = "X=92.37" (IFCTEXT)
    Y-koordinat = "Y=-54.05" (IFCTEXT)
    Ytelse = "0.00" (IFCTEXT)
  Pset_DDS | properties | on 2 objects (2 IFCFLOWCONTROLLER)
    Antall poler = "0" (IFCTEXT)
    Beskrivelse = "Lysregulator" (IFCTEXT)
    Bygningsdel = "Bygning: 0" (IFCTEXT)
    Etasjenummer = "Etasje: 4" (IFCTEXT)
    Group = "" (IFCTEXT)
    HOH, ref UK = "NNUK=13.14 m" (IFCTEXT)
    HOH, ref senter = "NN=13.14 m" (IFCTEXT)
    Høyde over ferdig gulv = "Senter= 1.10m OFG" (IFCTEXT)
    Høyde over rådekke = "Senter= 1.10m OKD" (IFCTEXT)
    Høyde underkant tak = "Senter= 1.63m UKT" (IFCTEXT)
    Lagnummer = 440 (IFCINTEGER)
    Modellnummer = "Modelllnr: 12" (IFCTEXT)
    Montasjehøyde = "1.10 m" (IFCTEXT)
    OK underkant tak = "OK= 0.00m UKT" (IFCTEXT)
    Produkt nr. = "S1-M5008" (IFCTEXT)
    Prosjektnavn = "1540_B6" (IFCTEXT)
    UK over rådekke = "UK= 1.10m OKD" (IFCTEXT)
    X-koordinat = "X=90.82" (IFCTEXT)
    Y-koordinat = "Y=-51.67" (IFCTEXT)
    Ytelse = "0.00" (IFCTEXT)
  Pset_DDS | properties | on 2 objects (2 IFCFLOWCONTROLLER)
    Antall poler = "0" (IFCTEXT)
    Beskrivelse = "Kronevender innfelt Exxact" (IFCTEXT)
    Bygningsdel = "Bygning: 0" (IFCTEXT)
    Etasjenummer = "Etasje: 5" (IFCTEXT)
    Group = "" (IFCTEXT)
    HOH, ref UK = "NNUK=16.04 m" (IFCTEXT)
    HOH, ref senter = "NN=16.04 m" (IFCTEXT)
    Høyde over ferdig gulv = "Senter= 1.10m OFG" (IFCTEXT)
    Høyde over rådekke = "Senter= 1.10m OKD" (IFCTEXT)
    Høyde underkant tak = "Senter= 1.77m UKT" (IFCTEXT)
    Lagnummer = 440 (IFCINTEGER)
    Modellnummer = "Modelllnr: 13" (IFCTEXT)
    Montasjehøyde = "1.10 m" (IFCTEXT)
    OK underkant tak = "OK= 0.00m UKT" (IFCTEXT)
    Produkt nr. = "1409903" (IFCTEXT)
    Prosjektnavn = "1540_B6" (IFCTEXT)
    UK over rådekke = "UK= 1.10m OKD" (IFCTEXT)
    X-koordinat = "X=104.69" (IFCTEXT)
    Y-koordinat = "Y=-40.39" (IFCTEXT)
    Ytelse = "0.00" (IFCTEXT)
  Pset_DDS | properties | on 2 objects (2 IFCFLOWCONTROLLER)
    Antall poler = "0" (IFCTEXT)
    Beskrivelse = "Kronevender innfelt Exxact" (IFCTEXT)
    Bygningsdel = "Bygning: 0" (IFCTEXT)
    Etasjenummer = "Etasje: 6" (IFCTEXT)
    Group = "" (IFCTEXT)
    HOH, ref UK = "NNUK=18.94 m" (IFCTEXT)
    HOH, ref senter = "NN=18.94 m" (IFCTEXT)
    Høyde over ferdig gulv = "Senter= 1.10m OFG" (IFCTEXT)
    Høyde over rådekke = "Senter= 1.10m OKD" (IFCTEXT)
    Høyde underkant tak = "Senter= 1.77m UKT" (IFCTEXT)
    Lagnummer = 440 (IFCINTEGER)
    Modellnummer = "Modelllnr: 14" (IFCTEXT)
    Montasjehøyde = "1.10 m" (IFCTEXT)
    OK underkant tak = "OK= 0.00m UKT" (IFCTEXT)
    Produkt nr. = "1409903" (IFCTEXT)
    Prosjektnavn = "1540_B6" (IFCTEXT)
    UK over rådekke = "UK= 1.10m OKD" (IFCTEXT)
    X-koordinat = "X=97.32" (IFCTEXT)
    Y-koordinat = "Y=-47.19" (IFCTEXT)
    Ytelse = "0.00" (IFCTEXT)
  Pset_DDS | properties | on 1 object (1 IFCFLOWTERMINAL)
    Beskrivelse = "2-IKT (2x Cat5UTP 6991160) + (1x1410113) Lexcom" (IFCTEXT)
    Bygningsdel = "Bygning: 0" (IFCTEXT)
    Etasjenummer = "Etasje: 2" (IFCTEXT)
    Group = "" (IFCTEXT)
    HOH, ref UK = "NNUK=6.39 m" (IFCTEXT)
    HOH, ref senter = "NN=6.39 m" (IFCTEXT)
    Høyde over ferdig gulv = "Senter= 0.15m OFG" (IFCTEXT)
    Høyde over rådekke = "Senter= 0.15m OKD" (IFCTEXT)
    Høyde underkant tak = "Senter= 2.50m UKT" (IFCTEXT)
    Lagnummer = 532 (IFCINTEGER)
    Modellnummer = "Modelllnr: 10" (IFCTEXT)
    Montasjehøyde = "0.15 m" (IFCTEXT)
    OK underkant tak = "OK= 0.00m UKT" (IFCTEXT)
    Produkt nr. = "6950710" (IFCTEXT)
    Prosjektnavn = "1540_B6" (IFCTEXT)
    UK over rådekke = "UK= 0.15m OKD" (IFCTEXT)
    X-koordinat = "X=97.60" (IFCTEXT)
    Y-koordinat = "Y=-48.89" (IFCTEXT)
  Pset_DDS | properties | on 1 object (1 IFCFLOWTERMINAL)
    Beskrivelse = "2-IKT (2x Cat5UTP 6991160) + (1x1410113) Lexcom" (IFCTEXT)
    Bygningsdel = "Bygning: 0" (IFCTEXT)
    Etasjenummer = "Etasje: 2" (IFCTEXT)
    Group = "" (IFCTEXT)
    HOH, ref UK = "NNUK=6.39 m" (IFCTEXT)
    HOH, ref senter = "NN=6.39 m" (IFCTEXT)
    Høyde over ferdig gulv = "Senter= 0.15m OFG" (IFCTEXT)
    Høyde over rådekke = "Senter= 0.15m OKD" (IFCTEXT)
    Høyde underkant tak = "Senter= 2.50m UKT" (IFCTEXT)
    Lagnummer = 532 (IFCINTEGER)
    Modellnummer = "Modelllnr: 10" (IFCTEXT)
    Montasjehøyde = "0.15 m" (IFCTEXT)
    OK underkant tak = "OK= 0.00m UKT" (IFCTEXT)
    Produkt nr. = "6950710" (IFCTEXT)
    Prosjektnavn = "1540_B6" (IFCTEXT)
    UK over rådekke = "UK= 0.15m OKD" (IFCTEXT)
    X-koordinat = "X=91.47" (IFCTEXT)
    Y-koordinat = "Y=-52.69" (IFCTEXT)
  Pset_DDS | properties | on 1 object (1 IFCFLOWTERMINAL)
    Beskrivelse = "1-IKT (1x Cat5UTP 6991160) + (1x1410113) Lexcom" (IFCTEXT)
    Bygningsdel = "Bygning: 0" (IFCTEXT)
    Etasjenummer = "Etasje: 2" (IFCTEXT)
    Group = "" (IFCTEXT)
    HOH, ref UK = "NNUK=6.39 m" (IFCTEXT)
    HOH, ref senter = "NN=6.39 m" (IFCTEXT)
    Høyde over ferdig gulv = "Senter= 0.15m OFG" (IFCTEXT)
    Høyde over rådekke = "Senter= 0.15m OKD" (IFCTEXT)
    Høyde underkant tak = "Senter= 2.50m UKT" (IFCTEXT)
    Lagnummer = 532 (IFCINTEGER)
    Modellnummer = "Modelllnr: 10" (IFCTEXT)
    Montasjehøyde = "0.15 m" (IFCTEXT)
    OK underkant tak = "OK= 0.00m UKT" (IFCTEXT)
    Produkt nr. = "6950710-" (IFCTEXT)
    Prosjektnavn = "1540_B6" (IFCTEXT)
    UK over rådekke = "UK= 0.15m OKD" (IFCTEXT)
    X-koordinat = "X=96.56" (IFCTEXT)
    Y-koordinat = "Y=-49.52" (IFCTEXT)
  Pset_DDS | properties | on 1 object (1 IFCFLOWTERMINAL)
    Beskrivelse = "1-IKT (1x Cat5UTP 6991160) + (1x1410113) Lexcom" (IFCTEXT)
    Bygningsdel = "Bygning: 0" (IFCTEXT)
    Etasjenummer = "Etasje: 2" (IFCTEXT)
    Group = "" (IFCTEXT)
    HOH, ref UK = "NNUK=6.39 m" (IFCTEXT)
    HOH, ref senter = "NN=6.39 m" (IFCTEXT)
    Høyde over ferdig gulv = "Senter= 0.15m OFG" (IFCTEXT)
    Høyde over rådekke = "Senter= 0.15m OKD" (IFCTEXT)
    Høyde underkant tak = "Senter= 2.50m UKT" (IFCTEXT)
    Lagnummer = 532 (IFCINTEGER)
    Modellnummer = "Modelllnr: 10" (IFCTEXT)
    Montasjehøyde = "0.15 m" (IFCTEXT)
    OK underkant tak = "OK= 0.00m UKT" (IFCTEXT)
    Produkt nr. = "6950710-" (IFCTEXT)
    Prosjektnavn = "1540_B6" (IFCTEXT)
    UK over rådekke = "UK= 0.15m OKD" (IFCTEXT)
    X-koordinat = "X=94.73" (IFCTEXT)
    Y-koordinat = "Y=-55.78" (IFCTEXT)
  Pset_DDS: 1264 more contents on 1264 objects not shown
  Pset_ManufacturerTypeInformation | properties | on 1 type object
    ArticleNumber = "6950710" (IFCIDENTIFIER)
    ModelLabel = "2-IKT (2x Cat5UTP 6991160) + (1x1410113) Lexcom" (IFCLABEL)
    ModelReference = "2-IKT (2x Cat5UTP 6991160) + (1x1410113) Lexcom" (IFCLABEL)
  Pset_ManufacturerTypeInformation | properties | on 1 type object
    ArticleNumber = "6950710-" (IFCIDENTIFIER)
    ModelLabel = "1-IKT (1x Cat5UTP 6991160) + (1x1410113) Lexcom" (IFCLABEL)
    ModelReference = "1-IKT (1x Cat5UTP 6991160) + (1x1410113) Lexcom" (IFCLABEL)
  Pset_ManufacturerTypeInformation | properties | on 1 type object
    ArticleNumber = "1502164" (IFCIDENTIFIER)
    ModelLabel = "Trippel stikk innfelt Exxact" (IFCLABEL)
    ModelReference = "Trippel stikk innfelt Exxact" (IFCLABEL)
  Pset_ManufacturerTypeInformation | properties | on 1 type object
    ArticleNumber = "1502134" (IFCIDENTIFIER)
    ModelLabel = "Stikkontakt dobbel m/jord innfelt Exxact" (IFCLABEL)
    ModelReference = "Stikkontakt dobbel m/jord innfelt Exxact" (IFCLABEL)
  Pset_ManufacturerTypeInformation | properties | on 1 type object
    ArticleNumber = "1502102" (IFCIDENTIFIER)
    ModelLabel = "Stikkontakt enkel Exxact" (IFCLABEL)
    ModelReference = "Stikkontakt enkel Exxact" (IFCLABEL)
  Pset_ManufacturerTypeInformation | properties | on 1 type object
    ArticleNumber = "1416000-" (IFCIDENTIFIER)
    ModelLabel = "Stikk flatstift 25A (Inngår i komfyrvakt)" (IFCLABEL)
    ModelReference = "Stikk flatstift 25A (Inngår i komfyrvakt)" (IFCLABEL)
  Pset_ManufacturerTypeInformation | properties | on 1 type object
    ArticleNumber = "1513013" (IFCIDENTIFIER)
    ModelLabel = "Lyspunkt DCL i tak Exxact" (IFCLABEL)
    ModelReference = "Lyspunkt DCL i tak Exxact" (IFCLABEL)
  Pset_ManufacturerTypeInformation | properties | on 1 type object
    ArticleNumber = "LI-090312092105" (IFCIDENTIFIER)
    ModelLabel = "Lyspunkt m/armatur" (IFCLABEL)
    ModelReference = "Lyspunkt m/armatur" (IFCLABEL)
  Pset_ManufacturerTypeInformation: 29 more contents on 0 objects not shown
  Pset_OutletTypeCommon | properties | on 12 type objects
    IsPluggableOutlet = TRUE (IFCLOGICAL)
  Pset_ElectricalDeviceCommon | properties | on 17 type objects
    HasProtectiveEarth = FALSE (IFCBOOLEAN)
    InsulationStandardClass in {"UNSET"} (IFCLABEL)
    NominalVoltage = 220. .. 240. (IFCELECTRICVOLTAGEMEASURE) [VOLT]
  Pset_ElectricalDeviceCommon | properties | on 8 type objects
    HasProtectiveEarth = FALSE (IFCBOOLEAN)
    InsulationStandardClass in {"UNSET"} (IFCLABEL)
    NominalCurrent = 0. (IFCELECTRICCURRENTMEASURE) [AMPERE]
    NominalVoltage = 220. .. 240. (IFCELECTRICVOLTAGEMEASURE) [VOLT]
    NumberOfPoles = 0 (IFCINTEGER)
  Pset_ElectricalDeviceCommon | properties | on 3 type objects
    HasProtectiveEarth = TRUE (IFCBOOLEAN)
    InsulationStandardClass in {"UNSET"} (IFCLABEL)
    NominalCurrent = 16. (IFCELECTRICCURRENTMEASURE) [AMPERE]
    NominalVoltage = 220. .. 240. (IFCELECTRICVOLTAGEMEASURE) [VOLT]
    NumberOfPoles = 2 (IFCINTEGER)
  Pset_ElectricalDeviceCommon | properties | on 3 type objects
    HasProtectiveEarth = FALSE (IFCBOOLEAN)
    InsulationStandardClass in {"UNSET"} (IFCLABEL)
    NominalCurrent = 16. (IFCELECTRICCURRENTMEASURE) [AMPERE]
    NominalVoltage = 220. .. 240. (IFCELECTRICVOLTAGEMEASURE) [VOLT]
    NumberOfPoles = 1 (IFCINTEGER)
  Pset_ElectricalDeviceCommon | properties | on 2 type objects
    HasProtectiveEarth = FALSE (IFCBOOLEAN)
    InsulationStandardClass in {"UNSET"} (IFCLABEL)
    NominalCurrent = 0. (IFCELECTRICCURRENTMEASURE) [AMPERE]
    NominalVoltage = 220. .. 240. (IFCELECTRICVOLTAGEMEASURE) [VOLT]
    NumberOfPoles = 1 (IFCINTEGER)
  Pset_ElectricalDeviceCommon | properties | on 1 type object
    HasProtectiveEarth = TRUE (IFCBOOLEAN)
    InsulationStandardClass in {"UNSET"} (IFCLABEL)
    NominalCurrent = 0. (IFCELECTRICCURRENTMEASURE) [AMPERE]
    NominalVoltage = 220. .. 240. (IFCELECTRICVOLTAGEMEASURE) [VOLT]
    NumberOfPoles = 2 (IFCINTEGER)
  Pset_ElectricalDeviceCommon | properties | on 1 type object
    HasProtectiveEarth = TRUE (IFCBOOLEAN)
    InsulationStandardClass in {"UNSET"} (IFCLABEL)
    NominalCurrent = 25. (IFCELECTRICCURRENTMEASURE) [AMPERE]
    NominalVoltage = 220. .. 240. (IFCELECTRICVOLTAGEMEASURE) [VOLT]
    NumberOfPoles = 2 (IFCINTEGER)
  Pset_ElectricalDeviceCommon | properties | on 1 type object
    HasProtectiveEarth = FALSE (IFCBOOLEAN)
    InsulationStandardClass in {"UNSET"} (IFCLABEL)
    NominalCurrent = 16. (IFCELECTRICCURRENTMEASURE) [AMPERE]
    NominalVoltage = 220. .. 240. (IFCELECTRICVOLTAGEMEASURE) [VOLT]
  Pset_ElectricalDeviceCommon: 1 more content on 0 objects not shown
  Pset_LightFixtureTypeCommon | properties | on 2 type objects
    LightFixtureMountingType in {"SURFACE", "SUSPENDED", "POLE_SIDE"} (IFCLABEL)
    LightFixturePlacingType in {"WALL"} (IFCLABEL)
    MaintenanceFactor = 1.25 (IFCREAL)
    NumberOfSources = 0 (IFCINTEGER)
    TotalWattage = 0. (IFCPOWERMEASURE) [WATT]
  Pset_LightFixtureTypeCommon | properties | on 2 type objects
    LightFixtureMountingType in {"SURFACE", "SUSPENDED", "POLE_SIDE"} (IFCLABEL)
    LightFixturePlacingType in {"WALL"} (IFCLABEL)
    MaintenanceFactor = 1.25 (IFCREAL)
    NumberOfSources = 1 (IFCINTEGER)
    TotalWattage = 60. (IFCPOWERMEASURE) [WATT]
  Pset_LightFixtureTypeCommon | properties | on 2 type objects
    LightFixtureMountingType in {"SURFACE", "SUSPENDED", "POLE_SIDE"} (IFCLABEL)
    LightFixturePlacingType in {"WALL"} (IFCLABEL)
    MaintenanceFactor = 1.25 (IFCREAL)
    NumberOfSources = 1 (IFCINTEGER)
    TotalWattage = 11. (IFCPOWERMEASURE) [WATT]
  Pset_LightFixtureTypeCommon | properties | on 1 type object
    LightFixtureMountingType in {"SURFACE", "SUSPENDED", "POLE_SIDE"} (IFCLABEL)
    LightFixturePlacingType in {"WALL"} (IFCLABEL)
    MaintenanceFactor = 1.25 (IFCREAL)
    NumberOfSources = 1 (IFCINTEGER)
    TotalWattage = 8. (IFCPOWERMEASURE) [WATT]
  Pset_LightFixtureTypeCommon | properties | on 1 type object
    LightFixtureMountingType in {"SURFACE", "SUSPENDED", "POLE_SIDE"} (IFCLABEL)
    LightFixturePlacingType in {"WALL"} (IFCLABEL)
    MaintenanceFactor = 1.25 (IFCREAL)
    NumberOfSources = 3 (IFCINTEGER)
    TotalWattage = 54. (IFCPOWERMEASURE) [WATT]
  Pset_LightFixtureTypeCommon | properties | on 1 type object
    LightFixtureMountingType in {"UNSET"} (IFCLABEL)
    LightFixturePlacingType in {"UNSET"} (IFCLABEL)
    MaintenanceFactor = 1.25 (IFCREAL)
    NumberOfSources = 1 (IFCINTEGER)
    TotalWattage = 60. (IFCPOWERMEASURE) [WATT]
  Pset_LightFixtureTypeCommon | properties | on 1 type object
    LightFixtureMountingType in {"SURFACE", "SUSPENDED", "POLE_SIDE"} (IFCLABEL)
    LightFixturePlacingType in {"WALL"} (IFCLABEL)
    MaintenanceFactor = 1.25 (IFCREAL)
    NumberOfSources = 1 (IFCINTEGER)
    TotalWattage = 58. (IFCPOWERMEASURE) [WATT]
  Pset_SwitchingDeviceTypeCommon | properties | on 13 type objects
    HasLock = FALSE (IFCBOOLEAN)
    NumberOfGangs = 1 (IFCINTEGER)
    SwitchFunction in {"ONOFFSWITCH"} (IFCLABEL)
  Pset_SwitchingDeviceTypeToggleSwitch | properties | on 13 type objects
    IsIlluminated = FALSE (IFCBOOLEAN)
    Legend = "ALLROUND" (IFCLABEL)
    SwitchActivation in {"HAND"} (IFCLABEL)
    SwitchUsage in {"START", "STOP"} (IFCLABEL)
    ToggleSwitchType in {"CHANGEOVER"} (IFCLABEL)
  Pset_ActuatorTypeCommon | properties | on 1 type object
    ManualOverride = FALSE (IFCBOOLEAN)